ARM GAS  /tmp/ccPRqU3T.s 			page 1


   1              		.cpu cortex-m4
   2              		.arch armv7e-m
   3              		.fpu fpv4-sp-d16
   4              		.eabi_attribute 27, 1
   5              		.eabi_attribute 28, 1
   6              		.eabi_attribute 20, 1
   7              		.eabi_attribute 21, 1
   8              		.eabi_attribute 23, 3
   9              		.eabi_attribute 24, 1
  10              		.eabi_attribute 25, 1
  11              		.eabi_attribute 26, 1
  12              		.eabi_attribute 30, 1
  13              		.eabi_attribute 34, 1
  14              		.eabi_attribute 18, 4
  15              		.file	"stm32f4xx_hal_cortex.c"
  16              		.text
  17              	.Ltext0:
  18              		.cfi_sections	.debug_frame
  19              		.section	.text.HAL_NVIC_SetPriorityGrouping,"ax",%progbits
  20              		.align	1
  21              		.global	HAL_NVIC_SetPriorityGrouping
  22              		.syntax unified
  23              		.thumb
  24              		.thumb_func
  26              	HAL_NVIC_SetPriorityGrouping:
  27              	.LVL0:
  28              	.LFB130:
  29              		.file 1 "Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c"
   1:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
   2:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ******************************************************************************
   3:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @file    stm32f4xx_hal_cortex.c
   4:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @author  MCD Application Team
   5:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief   CORTEX HAL module driver.
   6:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *          This file provides firmware functions to manage the following 
   7:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *          functionalities of the CORTEX:
   8:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           + Initialization and de-initialization functions
   9:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           + Peripheral Control functions 
  10:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *
  11:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   @verbatim  
  12:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ==============================================================================
  13:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                         ##### How to use this driver #####
  14:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ==============================================================================
  15:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  16:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     [..]  
  17:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     *** How to configure Interrupts using CORTEX HAL driver ***
  18:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     ===========================================================
  19:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     [..]     
  20:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     This section provides functions allowing to configure the NVIC interrupts (IRQ).
  21:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     The Cortex-M4 exceptions are managed by CMSIS functions.
  22:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    
  23:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     (#) Configure the NVIC Priority Grouping using HAL_NVIC_SetPriorityGrouping()
  24:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         function according to the following table.
  25:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     (#) Configure the priority of the selected IRQ Channels using HAL_NVIC_SetPriority(). 
  26:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     (#) Enable the selected IRQ Channels using HAL_NVIC_EnableIRQ().
  27:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     (#) please refer to programming manual for details in how to configure priority. 
  28:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****       
  29:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****      -@- When the NVIC_PRIORITYGROUP_0 is selected, IRQ preemption is no more possible. 
ARM GAS  /tmp/ccPRqU3T.s 			page 2


  30:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****          The pending IRQ priority will be managed only by the sub priority.
  31:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    
  32:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****      -@- IRQ priority order (sorted by highest to lowest priority):
  33:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (+@) Lowest preemption priority
  34:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (+@) Lowest sub priority
  35:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (+@) Lowest hardware priority (IRQ number)
  36:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  
  37:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     [..]  
  38:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     *** How to configure Systick using CORTEX HAL driver ***
  39:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     ========================================================
  40:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     [..]
  41:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     Setup SysTick Timer for time base.
  42:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****            
  43:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    (+) The HAL_SYSTICK_Config() function calls the SysTick_Config() function which
  44:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        is a CMSIS function that:
  45:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (++) Configures the SysTick Reload register with value passed as function parameter.
  46:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (++) Configures the SysTick IRQ priority to the lowest value 0x0F.
  47:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (++) Resets the SysTick Counter register.
  48:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (++) Configures the SysTick Counter clock source to be Core Clock Source (HCLK).
  49:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (++) Enables the SysTick Interrupt.
  50:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****         (++) Starts the SysTick Counter.
  51:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     
  52:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    (+) You can change the SysTick Clock source to be HCLK_Div8 by calling the macro
  53:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        __HAL_CORTEX_SYSTICKCLK_CONFIG(SYSTICK_CLKSOURCE_HCLK_DIV8) just after the
  54:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        HAL_SYSTICK_Config() function call. The __HAL_CORTEX_SYSTICKCLK_CONFIG() macro is defined
  55:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        inside the stm32f4xx_hal_cortex.h file.
  56:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  57:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    (+) You can change the SysTick IRQ priority by calling the
  58:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        HAL_NVIC_SetPriority(SysTick_IRQn,...) function just after the HAL_SYSTICK_Config() function
  59:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        call. The HAL_NVIC_SetPriority() call the NVIC_SetPriority() function which is a CMSIS funct
  60:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  61:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    (+) To adjust the SysTick time base, use the following formula:
  62:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                             
  63:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        Reload Value = SysTick Counter Clock (Hz) x  Desired Time base (s)
  64:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        (++) Reload Value is the parameter to be passed for HAL_SYSTICK_Config() function
  65:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****        (++) Reload Value should not exceed 0xFFFFFF
  66:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    
  67:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   @endverbatim
  68:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ******************************************************************************
  69:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @attention
  70:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *
  71:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * <h2><center>&copy; Copyright (c) 2017 STMicroelectronics.
  72:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * All rights reserved.</center></h2>
  73:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *
  74:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * This software component is licensed by ST under BSD 3-Clause license,
  75:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * the "License"; You may not use this file except in compliance with the
  76:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * License. You may obtain a copy of the License at:
  77:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                        opensource.org/licenses/BSD-3-Clause
  78:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *
  79:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ******************************************************************************
  80:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
  81:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  82:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Includes ------------------------------------------------------------------*/
  83:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** #include "stm32f4xx_hal.h"
  84:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  85:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /** @addtogroup STM32F4xx_HAL_Driver
  86:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @{
ARM GAS  /tmp/ccPRqU3T.s 			page 3


  87:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
  88:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  89:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /** @defgroup CORTEX CORTEX
  90:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief CORTEX HAL module driver
  91:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @{
  92:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
  93:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  94:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** #ifdef HAL_CORTEX_MODULE_ENABLED
  95:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
  96:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Private types -------------------------------------------------------------*/
  97:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Private variables ---------------------------------------------------------*/
  98:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Private constants ---------------------------------------------------------*/
  99:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Private macros ------------------------------------------------------------*/
 100:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Private functions ---------------------------------------------------------*/
 101:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /* Exported functions --------------------------------------------------------*/
 102:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 103:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /** @defgroup CORTEX_Exported_Functions CORTEX Exported Functions
 104:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @{
 105:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 106:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 107:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 108:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /** @defgroup CORTEX_Exported_Functions_Group1 Initialization and de-initialization functions
 109:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  *  @brief    Initialization and Configuration functions 
 110:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  *
 111:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** @verbatim    
 112:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ==============================================================================
 113:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****               ##### Initialization and de-initialization functions #####
 114:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ==============================================================================
 115:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     [..]
 116:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****       This section provides the CORTEX HAL driver functions allowing to configure Interrupts
 117:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****       Systick functionalities 
 118:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 119:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** @endverbatim
 120:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @{
 121:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 122:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 123:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 124:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 125:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Sets the priority grouping field (preemption priority and subpriority)
 126:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         using the required unlock sequence.
 127:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  PriorityGroup The priority grouping bits length. 
 128:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be one of the following values:
 129:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         @arg NVIC_PRIORITYGROUP_0: 0 bits for preemption priority
 130:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                    4 bits for subpriority
 131:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         @arg NVIC_PRIORITYGROUP_1: 1 bits for preemption priority
 132:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                    3 bits for subpriority
 133:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         @arg NVIC_PRIORITYGROUP_2: 2 bits for preemption priority
 134:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                    2 bits for subpriority
 135:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         @arg NVIC_PRIORITYGROUP_3: 3 bits for preemption priority
 136:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                    1 bits for subpriority
 137:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         @arg NVIC_PRIORITYGROUP_4: 4 bits for preemption priority
 138:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                    0 bits for subpriority
 139:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @note   When the NVIC_PriorityGroup_0 is selected, IRQ preemption is no more possible. 
 140:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         The pending IRQ priority will be managed only by the subpriority. 
 141:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 142:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 143:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_SetPriorityGrouping(uint32_t PriorityGroup)
ARM GAS  /tmp/ccPRqU3T.s 			page 4


 144:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
  30              		.loc 1 144 1 view -0
  31              		.cfi_startproc
  32              		@ args = 0, pretend = 0, frame = 0
  33              		@ frame_needed = 0, uses_anonymous_args = 0
  34              		@ link register save eliminated.
 145:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 146:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_PRIORITY_GROUP(PriorityGroup));
  35              		.loc 1 146 3 view .LVU1
 147:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 148:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Set the PRIGROUP[10:8] bits according to the PriorityGroup parameter value */
 149:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_SetPriorityGrouping(PriorityGroup);
  36              		.loc 1 149 3 view .LVU2
  37              	.LBB38:
  38              	.LBI38:
  39              		.file 2 "Drivers/CMSIS/Include/core_cm4.h"
   1:Drivers/CMSIS/Include/core_cm4.h **** /**************************************************************************//**
   2:Drivers/CMSIS/Include/core_cm4.h ****  * @file     core_cm4.h
   3:Drivers/CMSIS/Include/core_cm4.h ****  * @brief    CMSIS Cortex-M4 Core Peripheral Access Layer Header File
   4:Drivers/CMSIS/Include/core_cm4.h ****  * @version  V5.0.8
   5:Drivers/CMSIS/Include/core_cm4.h ****  * @date     04. June 2018
   6:Drivers/CMSIS/Include/core_cm4.h ****  ******************************************************************************/
   7:Drivers/CMSIS/Include/core_cm4.h **** /*
   8:Drivers/CMSIS/Include/core_cm4.h ****  * Copyright (c) 2009-2018 Arm Limited. All rights reserved.
   9:Drivers/CMSIS/Include/core_cm4.h ****  *
  10:Drivers/CMSIS/Include/core_cm4.h ****  * SPDX-License-Identifier: Apache-2.0
  11:Drivers/CMSIS/Include/core_cm4.h ****  *
  12:Drivers/CMSIS/Include/core_cm4.h ****  * Licensed under the Apache License, Version 2.0 (the License); you may
  13:Drivers/CMSIS/Include/core_cm4.h ****  * not use this file except in compliance with the License.
  14:Drivers/CMSIS/Include/core_cm4.h ****  * You may obtain a copy of the License at
  15:Drivers/CMSIS/Include/core_cm4.h ****  *
  16:Drivers/CMSIS/Include/core_cm4.h ****  * www.apache.org/licenses/LICENSE-2.0
  17:Drivers/CMSIS/Include/core_cm4.h ****  *
  18:Drivers/CMSIS/Include/core_cm4.h ****  * Unless required by applicable law or agreed to in writing, software
  19:Drivers/CMSIS/Include/core_cm4.h ****  * distributed under the License is distributed on an AS IS BASIS, WITHOUT
  20:Drivers/CMSIS/Include/core_cm4.h ****  * WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  21:Drivers/CMSIS/Include/core_cm4.h ****  * See the License for the specific language governing permissions and
  22:Drivers/CMSIS/Include/core_cm4.h ****  * limitations under the License.
  23:Drivers/CMSIS/Include/core_cm4.h ****  */
  24:Drivers/CMSIS/Include/core_cm4.h **** 
  25:Drivers/CMSIS/Include/core_cm4.h **** #if   defined ( __ICCARM__ )
  26:Drivers/CMSIS/Include/core_cm4.h ****   #pragma system_include         /* treat file as system include file for MISRA check */
  27:Drivers/CMSIS/Include/core_cm4.h **** #elif defined (__clang__)
  28:Drivers/CMSIS/Include/core_cm4.h ****   #pragma clang system_header   /* treat file as system include file */
  29:Drivers/CMSIS/Include/core_cm4.h **** #endif
  30:Drivers/CMSIS/Include/core_cm4.h **** 
  31:Drivers/CMSIS/Include/core_cm4.h **** #ifndef __CORE_CM4_H_GENERIC
  32:Drivers/CMSIS/Include/core_cm4.h **** #define __CORE_CM4_H_GENERIC
  33:Drivers/CMSIS/Include/core_cm4.h **** 
  34:Drivers/CMSIS/Include/core_cm4.h **** #include <stdint.h>
  35:Drivers/CMSIS/Include/core_cm4.h **** 
  36:Drivers/CMSIS/Include/core_cm4.h **** #ifdef __cplusplus
  37:Drivers/CMSIS/Include/core_cm4.h ****  extern "C" {
  38:Drivers/CMSIS/Include/core_cm4.h **** #endif
  39:Drivers/CMSIS/Include/core_cm4.h **** 
  40:Drivers/CMSIS/Include/core_cm4.h **** /**
  41:Drivers/CMSIS/Include/core_cm4.h ****   \page CMSIS_MISRA_Exceptions  MISRA-C:2004 Compliance Exceptions
ARM GAS  /tmp/ccPRqU3T.s 			page 5


  42:Drivers/CMSIS/Include/core_cm4.h ****   CMSIS violates the following MISRA-C:2004 rules:
  43:Drivers/CMSIS/Include/core_cm4.h **** 
  44:Drivers/CMSIS/Include/core_cm4.h ****    \li Required Rule 8.5, object/function definition in header file.<br>
  45:Drivers/CMSIS/Include/core_cm4.h ****      Function definitions in header files are used to allow 'inlining'.
  46:Drivers/CMSIS/Include/core_cm4.h **** 
  47:Drivers/CMSIS/Include/core_cm4.h ****    \li Required Rule 18.4, declaration of union type or object of union type: '{...}'.<br>
  48:Drivers/CMSIS/Include/core_cm4.h ****      Unions are used for effective representation of core registers.
  49:Drivers/CMSIS/Include/core_cm4.h **** 
  50:Drivers/CMSIS/Include/core_cm4.h ****    \li Advisory Rule 19.7, Function-like macro defined.<br>
  51:Drivers/CMSIS/Include/core_cm4.h ****      Function-like macros are used to allow more efficient code.
  52:Drivers/CMSIS/Include/core_cm4.h ****  */
  53:Drivers/CMSIS/Include/core_cm4.h **** 
  54:Drivers/CMSIS/Include/core_cm4.h **** 
  55:Drivers/CMSIS/Include/core_cm4.h **** /*******************************************************************************
  56:Drivers/CMSIS/Include/core_cm4.h ****  *                 CMSIS definitions
  57:Drivers/CMSIS/Include/core_cm4.h ****  ******************************************************************************/
  58:Drivers/CMSIS/Include/core_cm4.h **** /**
  59:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup Cortex_M4
  60:Drivers/CMSIS/Include/core_cm4.h ****   @{
  61:Drivers/CMSIS/Include/core_cm4.h ****  */
  62:Drivers/CMSIS/Include/core_cm4.h **** 
  63:Drivers/CMSIS/Include/core_cm4.h **** #include "cmsis_version.h"
  64:Drivers/CMSIS/Include/core_cm4.h **** 
  65:Drivers/CMSIS/Include/core_cm4.h **** /* CMSIS CM4 definitions */
  66:Drivers/CMSIS/Include/core_cm4.h **** #define __CM4_CMSIS_VERSION_MAIN  (__CM_CMSIS_VERSION_MAIN)              /*!< \deprecated [31:16] C
  67:Drivers/CMSIS/Include/core_cm4.h **** #define __CM4_CMSIS_VERSION_SUB   (__CM_CMSIS_VERSION_SUB)               /*!< \deprecated [15:0]  C
  68:Drivers/CMSIS/Include/core_cm4.h **** #define __CM4_CMSIS_VERSION       ((__CM4_CMSIS_VERSION_MAIN << 16U) | \
  69:Drivers/CMSIS/Include/core_cm4.h ****                                     __CM4_CMSIS_VERSION_SUB           )  /*!< \deprecated CMSIS HAL
  70:Drivers/CMSIS/Include/core_cm4.h **** 
  71:Drivers/CMSIS/Include/core_cm4.h **** #define __CORTEX_M                (4U)                                   /*!< Cortex-M Core */
  72:Drivers/CMSIS/Include/core_cm4.h **** 
  73:Drivers/CMSIS/Include/core_cm4.h **** /** __FPU_USED indicates whether an FPU is used or not.
  74:Drivers/CMSIS/Include/core_cm4.h ****     For this, __FPU_PRESENT has to be checked prior to making use of FPU specific registers and fun
  75:Drivers/CMSIS/Include/core_cm4.h **** */
  76:Drivers/CMSIS/Include/core_cm4.h **** #if defined ( __CC_ARM )
  77:Drivers/CMSIS/Include/core_cm4.h ****   #if defined __TARGET_FPU_VFP
  78:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
  79:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
  80:Drivers/CMSIS/Include/core_cm4.h ****     #else
  81:Drivers/CMSIS/Include/core_cm4.h ****       #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)
  82:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
  83:Drivers/CMSIS/Include/core_cm4.h ****     #endif
  84:Drivers/CMSIS/Include/core_cm4.h ****   #else
  85:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
  86:Drivers/CMSIS/Include/core_cm4.h ****   #endif
  87:Drivers/CMSIS/Include/core_cm4.h **** 
  88:Drivers/CMSIS/Include/core_cm4.h **** #elif defined (__ARMCC_VERSION) && (__ARMCC_VERSION >= 6010050)
  89:Drivers/CMSIS/Include/core_cm4.h ****   #if defined __ARM_PCS_VFP
  90:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
  91:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
  92:Drivers/CMSIS/Include/core_cm4.h ****     #else
  93:Drivers/CMSIS/Include/core_cm4.h ****       #warning "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESEN
  94:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
  95:Drivers/CMSIS/Include/core_cm4.h ****     #endif
  96:Drivers/CMSIS/Include/core_cm4.h ****   #else
  97:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
  98:Drivers/CMSIS/Include/core_cm4.h ****   #endif
ARM GAS  /tmp/ccPRqU3T.s 			page 6


  99:Drivers/CMSIS/Include/core_cm4.h **** 
 100:Drivers/CMSIS/Include/core_cm4.h **** #elif defined ( __GNUC__ )
 101:Drivers/CMSIS/Include/core_cm4.h ****   #if defined (__VFP_FP__) && !defined(__SOFTFP__)
 102:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
 103:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
 104:Drivers/CMSIS/Include/core_cm4.h ****     #else
 105:Drivers/CMSIS/Include/core_cm4.h ****       #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)
 106:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
 107:Drivers/CMSIS/Include/core_cm4.h ****     #endif
 108:Drivers/CMSIS/Include/core_cm4.h ****   #else
 109:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
 110:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 111:Drivers/CMSIS/Include/core_cm4.h **** 
 112:Drivers/CMSIS/Include/core_cm4.h **** #elif defined ( __ICCARM__ )
 113:Drivers/CMSIS/Include/core_cm4.h ****   #if defined __ARMVFP__
 114:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
 115:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
 116:Drivers/CMSIS/Include/core_cm4.h ****     #else
 117:Drivers/CMSIS/Include/core_cm4.h ****       #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)
 118:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
 119:Drivers/CMSIS/Include/core_cm4.h ****     #endif
 120:Drivers/CMSIS/Include/core_cm4.h ****   #else
 121:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
 122:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 123:Drivers/CMSIS/Include/core_cm4.h **** 
 124:Drivers/CMSIS/Include/core_cm4.h **** #elif defined ( __TI_ARM__ )
 125:Drivers/CMSIS/Include/core_cm4.h ****   #if defined __TI_VFP_SUPPORT__
 126:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
 127:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
 128:Drivers/CMSIS/Include/core_cm4.h ****     #else
 129:Drivers/CMSIS/Include/core_cm4.h ****       #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)
 130:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
 131:Drivers/CMSIS/Include/core_cm4.h ****     #endif
 132:Drivers/CMSIS/Include/core_cm4.h ****   #else
 133:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
 134:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 135:Drivers/CMSIS/Include/core_cm4.h **** 
 136:Drivers/CMSIS/Include/core_cm4.h **** #elif defined ( __TASKING__ )
 137:Drivers/CMSIS/Include/core_cm4.h ****   #if defined __FPU_VFP__
 138:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
 139:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
 140:Drivers/CMSIS/Include/core_cm4.h ****     #else
 141:Drivers/CMSIS/Include/core_cm4.h ****       #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)
 142:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
 143:Drivers/CMSIS/Include/core_cm4.h ****     #endif
 144:Drivers/CMSIS/Include/core_cm4.h ****   #else
 145:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
 146:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 147:Drivers/CMSIS/Include/core_cm4.h **** 
 148:Drivers/CMSIS/Include/core_cm4.h **** #elif defined ( __CSMC__ )
 149:Drivers/CMSIS/Include/core_cm4.h ****   #if ( __CSMC__ & 0x400U)
 150:Drivers/CMSIS/Include/core_cm4.h ****     #if defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)
 151:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       1U
 152:Drivers/CMSIS/Include/core_cm4.h ****     #else
 153:Drivers/CMSIS/Include/core_cm4.h ****       #error "Compiler generates FPU instructions for a device without an FPU (check __FPU_PRESENT)
 154:Drivers/CMSIS/Include/core_cm4.h ****       #define __FPU_USED       0U
 155:Drivers/CMSIS/Include/core_cm4.h ****     #endif
ARM GAS  /tmp/ccPRqU3T.s 			page 7


 156:Drivers/CMSIS/Include/core_cm4.h ****   #else
 157:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_USED         0U
 158:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 159:Drivers/CMSIS/Include/core_cm4.h **** 
 160:Drivers/CMSIS/Include/core_cm4.h **** #endif
 161:Drivers/CMSIS/Include/core_cm4.h **** 
 162:Drivers/CMSIS/Include/core_cm4.h **** #include "cmsis_compiler.h"               /* CMSIS compiler specific defines */
 163:Drivers/CMSIS/Include/core_cm4.h **** 
 164:Drivers/CMSIS/Include/core_cm4.h **** 
 165:Drivers/CMSIS/Include/core_cm4.h **** #ifdef __cplusplus
 166:Drivers/CMSIS/Include/core_cm4.h **** }
 167:Drivers/CMSIS/Include/core_cm4.h **** #endif
 168:Drivers/CMSIS/Include/core_cm4.h **** 
 169:Drivers/CMSIS/Include/core_cm4.h **** #endif /* __CORE_CM4_H_GENERIC */
 170:Drivers/CMSIS/Include/core_cm4.h **** 
 171:Drivers/CMSIS/Include/core_cm4.h **** #ifndef __CMSIS_GENERIC
 172:Drivers/CMSIS/Include/core_cm4.h **** 
 173:Drivers/CMSIS/Include/core_cm4.h **** #ifndef __CORE_CM4_H_DEPENDANT
 174:Drivers/CMSIS/Include/core_cm4.h **** #define __CORE_CM4_H_DEPENDANT
 175:Drivers/CMSIS/Include/core_cm4.h **** 
 176:Drivers/CMSIS/Include/core_cm4.h **** #ifdef __cplusplus
 177:Drivers/CMSIS/Include/core_cm4.h ****  extern "C" {
 178:Drivers/CMSIS/Include/core_cm4.h **** #endif
 179:Drivers/CMSIS/Include/core_cm4.h **** 
 180:Drivers/CMSIS/Include/core_cm4.h **** /* check device defines and use defaults */
 181:Drivers/CMSIS/Include/core_cm4.h **** #if defined __CHECK_DEVICE_DEFINES
 182:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef __CM4_REV
 183:Drivers/CMSIS/Include/core_cm4.h ****     #define __CM4_REV               0x0000U
 184:Drivers/CMSIS/Include/core_cm4.h ****     #warning "__CM4_REV not defined in device header file; using default!"
 185:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 186:Drivers/CMSIS/Include/core_cm4.h **** 
 187:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef __FPU_PRESENT
 188:Drivers/CMSIS/Include/core_cm4.h ****     #define __FPU_PRESENT             0U
 189:Drivers/CMSIS/Include/core_cm4.h ****     #warning "__FPU_PRESENT not defined in device header file; using default!"
 190:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 191:Drivers/CMSIS/Include/core_cm4.h **** 
 192:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef __MPU_PRESENT
 193:Drivers/CMSIS/Include/core_cm4.h ****     #define __MPU_PRESENT             0U
 194:Drivers/CMSIS/Include/core_cm4.h ****     #warning "__MPU_PRESENT not defined in device header file; using default!"
 195:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 196:Drivers/CMSIS/Include/core_cm4.h **** 
 197:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef __NVIC_PRIO_BITS
 198:Drivers/CMSIS/Include/core_cm4.h ****     #define __NVIC_PRIO_BITS          3U
 199:Drivers/CMSIS/Include/core_cm4.h ****     #warning "__NVIC_PRIO_BITS not defined in device header file; using default!"
 200:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 201:Drivers/CMSIS/Include/core_cm4.h **** 
 202:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef __Vendor_SysTickConfig
 203:Drivers/CMSIS/Include/core_cm4.h ****     #define __Vendor_SysTickConfig    0U
 204:Drivers/CMSIS/Include/core_cm4.h ****     #warning "__Vendor_SysTickConfig not defined in device header file; using default!"
 205:Drivers/CMSIS/Include/core_cm4.h ****   #endif
 206:Drivers/CMSIS/Include/core_cm4.h **** #endif
 207:Drivers/CMSIS/Include/core_cm4.h **** 
 208:Drivers/CMSIS/Include/core_cm4.h **** /* IO definitions (access restrictions to peripheral registers) */
 209:Drivers/CMSIS/Include/core_cm4.h **** /**
 210:Drivers/CMSIS/Include/core_cm4.h ****     \defgroup CMSIS_glob_defs CMSIS Global Defines
 211:Drivers/CMSIS/Include/core_cm4.h **** 
 212:Drivers/CMSIS/Include/core_cm4.h ****     <strong>IO Type Qualifiers</strong> are used
ARM GAS  /tmp/ccPRqU3T.s 			page 8


 213:Drivers/CMSIS/Include/core_cm4.h ****     \li to specify the access to peripheral variables.
 214:Drivers/CMSIS/Include/core_cm4.h ****     \li for automatic generation of peripheral register debug information.
 215:Drivers/CMSIS/Include/core_cm4.h **** */
 216:Drivers/CMSIS/Include/core_cm4.h **** #ifdef __cplusplus
 217:Drivers/CMSIS/Include/core_cm4.h ****   #define   __I     volatile             /*!< Defines 'read only' permissions */
 218:Drivers/CMSIS/Include/core_cm4.h **** #else
 219:Drivers/CMSIS/Include/core_cm4.h ****   #define   __I     volatile const       /*!< Defines 'read only' permissions */
 220:Drivers/CMSIS/Include/core_cm4.h **** #endif
 221:Drivers/CMSIS/Include/core_cm4.h **** #define     __O     volatile             /*!< Defines 'write only' permissions */
 222:Drivers/CMSIS/Include/core_cm4.h **** #define     __IO    volatile             /*!< Defines 'read / write' permissions */
 223:Drivers/CMSIS/Include/core_cm4.h **** 
 224:Drivers/CMSIS/Include/core_cm4.h **** /* following defines should be used for structure members */
 225:Drivers/CMSIS/Include/core_cm4.h **** #define     __IM     volatile const      /*! Defines 'read only' structure member permissions */
 226:Drivers/CMSIS/Include/core_cm4.h **** #define     __OM     volatile            /*! Defines 'write only' structure member permissions */
 227:Drivers/CMSIS/Include/core_cm4.h **** #define     __IOM    volatile            /*! Defines 'read / write' structure member permissions */
 228:Drivers/CMSIS/Include/core_cm4.h **** 
 229:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group Cortex_M4 */
 230:Drivers/CMSIS/Include/core_cm4.h **** 
 231:Drivers/CMSIS/Include/core_cm4.h **** 
 232:Drivers/CMSIS/Include/core_cm4.h **** 
 233:Drivers/CMSIS/Include/core_cm4.h **** /*******************************************************************************
 234:Drivers/CMSIS/Include/core_cm4.h ****  *                 Register Abstraction
 235:Drivers/CMSIS/Include/core_cm4.h ****   Core Register contain:
 236:Drivers/CMSIS/Include/core_cm4.h ****   - Core Register
 237:Drivers/CMSIS/Include/core_cm4.h ****   - Core NVIC Register
 238:Drivers/CMSIS/Include/core_cm4.h ****   - Core SCB Register
 239:Drivers/CMSIS/Include/core_cm4.h ****   - Core SysTick Register
 240:Drivers/CMSIS/Include/core_cm4.h ****   - Core Debug Register
 241:Drivers/CMSIS/Include/core_cm4.h ****   - Core MPU Register
 242:Drivers/CMSIS/Include/core_cm4.h ****   - Core FPU Register
 243:Drivers/CMSIS/Include/core_cm4.h ****  ******************************************************************************/
 244:Drivers/CMSIS/Include/core_cm4.h **** /**
 245:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_core_register Defines and Type Definitions
 246:Drivers/CMSIS/Include/core_cm4.h ****   \brief Type definitions and defines for Cortex-M processor based devices.
 247:Drivers/CMSIS/Include/core_cm4.h **** */
 248:Drivers/CMSIS/Include/core_cm4.h **** 
 249:Drivers/CMSIS/Include/core_cm4.h **** /**
 250:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup    CMSIS_core_register
 251:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup   CMSIS_CORE  Status and Control Registers
 252:Drivers/CMSIS/Include/core_cm4.h ****   \brief      Core Register type definitions.
 253:Drivers/CMSIS/Include/core_cm4.h ****   @{
 254:Drivers/CMSIS/Include/core_cm4.h ****  */
 255:Drivers/CMSIS/Include/core_cm4.h **** 
 256:Drivers/CMSIS/Include/core_cm4.h **** /**
 257:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Union type to access the Application Program Status Register (APSR).
 258:Drivers/CMSIS/Include/core_cm4.h ****  */
 259:Drivers/CMSIS/Include/core_cm4.h **** typedef union
 260:Drivers/CMSIS/Include/core_cm4.h **** {
 261:Drivers/CMSIS/Include/core_cm4.h ****   struct
 262:Drivers/CMSIS/Include/core_cm4.h ****   {
 263:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t _reserved0:16;              /*!< bit:  0..15  Reserved */
 264:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t GE:4;                       /*!< bit: 16..19  Greater than or Equal flags */
 265:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t _reserved1:7;               /*!< bit: 20..26  Reserved */
 266:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t Q:1;                        /*!< bit:     27  Saturation condition flag */
 267:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t V:1;                        /*!< bit:     28  Overflow condition code flag */
 268:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t C:1;                        /*!< bit:     29  Carry condition code flag */
 269:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t Z:1;                        /*!< bit:     30  Zero condition code flag */
ARM GAS  /tmp/ccPRqU3T.s 			page 9


 270:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t N:1;                        /*!< bit:     31  Negative condition code flag */
 271:Drivers/CMSIS/Include/core_cm4.h ****   } b;                                   /*!< Structure used for bit  access */
 272:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t w;                            /*!< Type      used for word access */
 273:Drivers/CMSIS/Include/core_cm4.h **** } APSR_Type;
 274:Drivers/CMSIS/Include/core_cm4.h **** 
 275:Drivers/CMSIS/Include/core_cm4.h **** /* APSR Register Definitions */
 276:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_N_Pos                         31U                                            /*!< APSR
 277:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_N_Msk                         (1UL << APSR_N_Pos)                            /*!< APSR
 278:Drivers/CMSIS/Include/core_cm4.h **** 
 279:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_Z_Pos                         30U                                            /*!< APSR
 280:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_Z_Msk                         (1UL << APSR_Z_Pos)                            /*!< APSR
 281:Drivers/CMSIS/Include/core_cm4.h **** 
 282:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_C_Pos                         29U                                            /*!< APSR
 283:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_C_Msk                         (1UL << APSR_C_Pos)                            /*!< APSR
 284:Drivers/CMSIS/Include/core_cm4.h **** 
 285:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_V_Pos                         28U                                            /*!< APSR
 286:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_V_Msk                         (1UL << APSR_V_Pos)                            /*!< APSR
 287:Drivers/CMSIS/Include/core_cm4.h **** 
 288:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_Q_Pos                         27U                                            /*!< APSR
 289:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_Q_Msk                         (1UL << APSR_Q_Pos)                            /*!< APSR
 290:Drivers/CMSIS/Include/core_cm4.h **** 
 291:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_GE_Pos                        16U                                            /*!< APSR
 292:Drivers/CMSIS/Include/core_cm4.h **** #define APSR_GE_Msk                        (0xFUL << APSR_GE_Pos)                         /*!< APSR
 293:Drivers/CMSIS/Include/core_cm4.h **** 
 294:Drivers/CMSIS/Include/core_cm4.h **** 
 295:Drivers/CMSIS/Include/core_cm4.h **** /**
 296:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Union type to access the Interrupt Program Status Register (IPSR).
 297:Drivers/CMSIS/Include/core_cm4.h ****  */
 298:Drivers/CMSIS/Include/core_cm4.h **** typedef union
 299:Drivers/CMSIS/Include/core_cm4.h **** {
 300:Drivers/CMSIS/Include/core_cm4.h ****   struct
 301:Drivers/CMSIS/Include/core_cm4.h ****   {
 302:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t ISR:9;                      /*!< bit:  0.. 8  Exception number */
 303:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t _reserved0:23;              /*!< bit:  9..31  Reserved */
 304:Drivers/CMSIS/Include/core_cm4.h ****   } b;                                   /*!< Structure used for bit  access */
 305:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t w;                            /*!< Type      used for word access */
 306:Drivers/CMSIS/Include/core_cm4.h **** } IPSR_Type;
 307:Drivers/CMSIS/Include/core_cm4.h **** 
 308:Drivers/CMSIS/Include/core_cm4.h **** /* IPSR Register Definitions */
 309:Drivers/CMSIS/Include/core_cm4.h **** #define IPSR_ISR_Pos                        0U                                            /*!< IPSR
 310:Drivers/CMSIS/Include/core_cm4.h **** #define IPSR_ISR_Msk                       (0x1FFUL /*<< IPSR_ISR_Pos*/)                  /*!< IPSR
 311:Drivers/CMSIS/Include/core_cm4.h **** 
 312:Drivers/CMSIS/Include/core_cm4.h **** 
 313:Drivers/CMSIS/Include/core_cm4.h **** /**
 314:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Union type to access the Special-Purpose Program Status Registers (xPSR).
 315:Drivers/CMSIS/Include/core_cm4.h ****  */
 316:Drivers/CMSIS/Include/core_cm4.h **** typedef union
 317:Drivers/CMSIS/Include/core_cm4.h **** {
 318:Drivers/CMSIS/Include/core_cm4.h ****   struct
 319:Drivers/CMSIS/Include/core_cm4.h ****   {
 320:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t ISR:9;                      /*!< bit:  0.. 8  Exception number */
 321:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t _reserved0:1;               /*!< bit:      9  Reserved */
 322:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t ICI_IT_1:6;                 /*!< bit: 10..15  ICI/IT part 1 */
 323:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t GE:4;                       /*!< bit: 16..19  Greater than or Equal flags */
 324:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t _reserved1:4;               /*!< bit: 20..23  Reserved */
 325:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t T:1;                        /*!< bit:     24  Thumb bit */
 326:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t ICI_IT_2:2;                 /*!< bit: 25..26  ICI/IT part 2 */
ARM GAS  /tmp/ccPRqU3T.s 			page 10


 327:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t Q:1;                        /*!< bit:     27  Saturation condition flag */
 328:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t V:1;                        /*!< bit:     28  Overflow condition code flag */
 329:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t C:1;                        /*!< bit:     29  Carry condition code flag */
 330:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t Z:1;                        /*!< bit:     30  Zero condition code flag */
 331:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t N:1;                        /*!< bit:     31  Negative condition code flag */
 332:Drivers/CMSIS/Include/core_cm4.h ****   } b;                                   /*!< Structure used for bit  access */
 333:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t w;                            /*!< Type      used for word access */
 334:Drivers/CMSIS/Include/core_cm4.h **** } xPSR_Type;
 335:Drivers/CMSIS/Include/core_cm4.h **** 
 336:Drivers/CMSIS/Include/core_cm4.h **** /* xPSR Register Definitions */
 337:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_N_Pos                         31U                                            /*!< xPSR
 338:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_N_Msk                         (1UL << xPSR_N_Pos)                            /*!< xPSR
 339:Drivers/CMSIS/Include/core_cm4.h **** 
 340:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_Z_Pos                         30U                                            /*!< xPSR
 341:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_Z_Msk                         (1UL << xPSR_Z_Pos)                            /*!< xPSR
 342:Drivers/CMSIS/Include/core_cm4.h **** 
 343:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_C_Pos                         29U                                            /*!< xPSR
 344:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_C_Msk                         (1UL << xPSR_C_Pos)                            /*!< xPSR
 345:Drivers/CMSIS/Include/core_cm4.h **** 
 346:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_V_Pos                         28U                                            /*!< xPSR
 347:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_V_Msk                         (1UL << xPSR_V_Pos)                            /*!< xPSR
 348:Drivers/CMSIS/Include/core_cm4.h **** 
 349:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_Q_Pos                         27U                                            /*!< xPSR
 350:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_Q_Msk                         (1UL << xPSR_Q_Pos)                            /*!< xPSR
 351:Drivers/CMSIS/Include/core_cm4.h **** 
 352:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_ICI_IT_2_Pos                  25U                                            /*!< xPSR
 353:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_ICI_IT_2_Msk                  (3UL << xPSR_ICI_IT_2_Pos)                     /*!< xPSR
 354:Drivers/CMSIS/Include/core_cm4.h **** 
 355:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_T_Pos                         24U                                            /*!< xPSR
 356:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_T_Msk                         (1UL << xPSR_T_Pos)                            /*!< xPSR
 357:Drivers/CMSIS/Include/core_cm4.h **** 
 358:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_GE_Pos                        16U                                            /*!< xPSR
 359:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_GE_Msk                        (0xFUL << xPSR_GE_Pos)                         /*!< xPSR
 360:Drivers/CMSIS/Include/core_cm4.h **** 
 361:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_ICI_IT_1_Pos                  10U                                            /*!< xPSR
 362:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_ICI_IT_1_Msk                  (0x3FUL << xPSR_ICI_IT_1_Pos)                  /*!< xPSR
 363:Drivers/CMSIS/Include/core_cm4.h **** 
 364:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_ISR_Pos                        0U                                            /*!< xPSR
 365:Drivers/CMSIS/Include/core_cm4.h **** #define xPSR_ISR_Msk                       (0x1FFUL /*<< xPSR_ISR_Pos*/)                  /*!< xPSR
 366:Drivers/CMSIS/Include/core_cm4.h **** 
 367:Drivers/CMSIS/Include/core_cm4.h **** 
 368:Drivers/CMSIS/Include/core_cm4.h **** /**
 369:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Union type to access the Control Registers (CONTROL).
 370:Drivers/CMSIS/Include/core_cm4.h ****  */
 371:Drivers/CMSIS/Include/core_cm4.h **** typedef union
 372:Drivers/CMSIS/Include/core_cm4.h **** {
 373:Drivers/CMSIS/Include/core_cm4.h ****   struct
 374:Drivers/CMSIS/Include/core_cm4.h ****   {
 375:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t nPRIV:1;                    /*!< bit:      0  Execution privilege in Thread mode */
 376:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t SPSEL:1;                    /*!< bit:      1  Stack to be used */
 377:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t FPCA:1;                     /*!< bit:      2  FP extension active flag */
 378:Drivers/CMSIS/Include/core_cm4.h ****     uint32_t _reserved0:29;              /*!< bit:  3..31  Reserved */
 379:Drivers/CMSIS/Include/core_cm4.h ****   } b;                                   /*!< Structure used for bit  access */
 380:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t w;                            /*!< Type      used for word access */
 381:Drivers/CMSIS/Include/core_cm4.h **** } CONTROL_Type;
 382:Drivers/CMSIS/Include/core_cm4.h **** 
 383:Drivers/CMSIS/Include/core_cm4.h **** /* CONTROL Register Definitions */
ARM GAS  /tmp/ccPRqU3T.s 			page 11


 384:Drivers/CMSIS/Include/core_cm4.h **** #define CONTROL_FPCA_Pos                    2U                                            /*!< CONT
 385:Drivers/CMSIS/Include/core_cm4.h **** #define CONTROL_FPCA_Msk                   (1UL << CONTROL_FPCA_Pos)                      /*!< CONT
 386:Drivers/CMSIS/Include/core_cm4.h **** 
 387:Drivers/CMSIS/Include/core_cm4.h **** #define CONTROL_SPSEL_Pos                   1U                                            /*!< CONT
 388:Drivers/CMSIS/Include/core_cm4.h **** #define CONTROL_SPSEL_Msk                  (1UL << CONTROL_SPSEL_Pos)                     /*!< CONT
 389:Drivers/CMSIS/Include/core_cm4.h **** 
 390:Drivers/CMSIS/Include/core_cm4.h **** #define CONTROL_nPRIV_Pos                   0U                                            /*!< CONT
 391:Drivers/CMSIS/Include/core_cm4.h **** #define CONTROL_nPRIV_Msk                  (1UL /*<< CONTROL_nPRIV_Pos*/)                 /*!< CONT
 392:Drivers/CMSIS/Include/core_cm4.h **** 
 393:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_CORE */
 394:Drivers/CMSIS/Include/core_cm4.h **** 
 395:Drivers/CMSIS/Include/core_cm4.h **** 
 396:Drivers/CMSIS/Include/core_cm4.h **** /**
 397:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup    CMSIS_core_register
 398:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup   CMSIS_NVIC  Nested Vectored Interrupt Controller (NVIC)
 399:Drivers/CMSIS/Include/core_cm4.h ****   \brief      Type definitions for the NVIC Registers
 400:Drivers/CMSIS/Include/core_cm4.h ****   @{
 401:Drivers/CMSIS/Include/core_cm4.h ****  */
 402:Drivers/CMSIS/Include/core_cm4.h **** 
 403:Drivers/CMSIS/Include/core_cm4.h **** /**
 404:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Nested Vectored Interrupt Controller (NVIC).
 405:Drivers/CMSIS/Include/core_cm4.h ****  */
 406:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
 407:Drivers/CMSIS/Include/core_cm4.h **** {
 408:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ISER[8U];               /*!< Offset: 0x000 (R/W)  Interrupt Set Enable Register */
 409:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[24U];
 410:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ICER[8U];               /*!< Offset: 0x080 (R/W)  Interrupt Clear Enable Register 
 411:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RSERVED1[24U];
 412:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ISPR[8U];               /*!< Offset: 0x100 (R/W)  Interrupt Set Pending Register *
 413:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED2[24U];
 414:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ICPR[8U];               /*!< Offset: 0x180 (R/W)  Interrupt Clear Pending Register
 415:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED3[24U];
 416:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t IABR[8U];               /*!< Offset: 0x200 (R/W)  Interrupt Active bit Register */
 417:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED4[56U];
 418:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint8_t  IP[240U];               /*!< Offset: 0x300 (R/W)  Interrupt Priority Register (8Bi
 419:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED5[644U];
 420:Drivers/CMSIS/Include/core_cm4.h ****   __OM  uint32_t STIR;                   /*!< Offset: 0xE00 ( /W)  Software Trigger Interrupt Regis
 421:Drivers/CMSIS/Include/core_cm4.h **** }  NVIC_Type;
 422:Drivers/CMSIS/Include/core_cm4.h **** 
 423:Drivers/CMSIS/Include/core_cm4.h **** /* Software Triggered Interrupt Register Definitions */
 424:Drivers/CMSIS/Include/core_cm4.h **** #define NVIC_STIR_INTID_Pos                 0U                                         /*!< STIR: I
 425:Drivers/CMSIS/Include/core_cm4.h **** #define NVIC_STIR_INTID_Msk                (0x1FFUL /*<< NVIC_STIR_INTID_Pos*/)        /*!< STIR: I
 426:Drivers/CMSIS/Include/core_cm4.h **** 
 427:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_NVIC */
 428:Drivers/CMSIS/Include/core_cm4.h **** 
 429:Drivers/CMSIS/Include/core_cm4.h **** 
 430:Drivers/CMSIS/Include/core_cm4.h **** /**
 431:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
 432:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_SCB     System Control Block (SCB)
 433:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the System Control Block Registers
 434:Drivers/CMSIS/Include/core_cm4.h ****   @{
 435:Drivers/CMSIS/Include/core_cm4.h ****  */
 436:Drivers/CMSIS/Include/core_cm4.h **** 
 437:Drivers/CMSIS/Include/core_cm4.h **** /**
 438:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the System Control Block (SCB).
 439:Drivers/CMSIS/Include/core_cm4.h ****  */
 440:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
ARM GAS  /tmp/ccPRqU3T.s 			page 12


 441:Drivers/CMSIS/Include/core_cm4.h **** {
 442:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t CPUID;                  /*!< Offset: 0x000 (R/ )  CPUID Base Register */
 443:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ICSR;                   /*!< Offset: 0x004 (R/W)  Interrupt Control and State Regi
 444:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t VTOR;                   /*!< Offset: 0x008 (R/W)  Vector Table Offset Register */
 445:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t AIRCR;                  /*!< Offset: 0x00C (R/W)  Application Interrupt and Reset 
 446:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t SCR;                    /*!< Offset: 0x010 (R/W)  System Control Register */
 447:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CCR;                    /*!< Offset: 0x014 (R/W)  Configuration Control Register *
 448:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint8_t  SHP[12U];               /*!< Offset: 0x018 (R/W)  System Handlers Priority Registe
 449:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t SHCSR;                  /*!< Offset: 0x024 (R/W)  System Handler Control and State
 450:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CFSR;                   /*!< Offset: 0x028 (R/W)  Configurable Fault Status Regist
 451:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t HFSR;                   /*!< Offset: 0x02C (R/W)  HardFault Status Register */
 452:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t DFSR;                   /*!< Offset: 0x030 (R/W)  Debug Fault Status Register */
 453:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t MMFAR;                  /*!< Offset: 0x034 (R/W)  MemManage Fault Address Register
 454:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t BFAR;                   /*!< Offset: 0x038 (R/W)  BusFault Address Register */
 455:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t AFSR;                   /*!< Offset: 0x03C (R/W)  Auxiliary Fault Status Register 
 456:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PFR[2U];                /*!< Offset: 0x040 (R/ )  Processor Feature Register */
 457:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t DFR;                    /*!< Offset: 0x048 (R/ )  Debug Feature Register */
 458:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t ADR;                    /*!< Offset: 0x04C (R/ )  Auxiliary Feature Register */
 459:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t MMFR[4U];               /*!< Offset: 0x050 (R/ )  Memory Model Feature Register */
 460:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t ISAR[5U];               /*!< Offset: 0x060 (R/ )  Instruction Set Attributes Regis
 461:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[5U];
 462:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CPACR;                  /*!< Offset: 0x088 (R/W)  Coprocessor Access Control Regis
 463:Drivers/CMSIS/Include/core_cm4.h **** } SCB_Type;
 464:Drivers/CMSIS/Include/core_cm4.h **** 
 465:Drivers/CMSIS/Include/core_cm4.h **** /* SCB CPUID Register Definitions */
 466:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_IMPLEMENTER_Pos          24U                                            /*!< SCB 
 467:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_IMPLEMENTER_Msk          (0xFFUL << SCB_CPUID_IMPLEMENTER_Pos)          /*!< SCB 
 468:Drivers/CMSIS/Include/core_cm4.h **** 
 469:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_VARIANT_Pos              20U                                            /*!< SCB 
 470:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_VARIANT_Msk              (0xFUL << SCB_CPUID_VARIANT_Pos)               /*!< SCB 
 471:Drivers/CMSIS/Include/core_cm4.h **** 
 472:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_ARCHITECTURE_Pos         16U                                            /*!< SCB 
 473:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_ARCHITECTURE_Msk         (0xFUL << SCB_CPUID_ARCHITECTURE_Pos)          /*!< SCB 
 474:Drivers/CMSIS/Include/core_cm4.h **** 
 475:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_PARTNO_Pos                4U                                            /*!< SCB 
 476:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_PARTNO_Msk               (0xFFFUL << SCB_CPUID_PARTNO_Pos)              /*!< SCB 
 477:Drivers/CMSIS/Include/core_cm4.h **** 
 478:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_REVISION_Pos              0U                                            /*!< SCB 
 479:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CPUID_REVISION_Msk             (0xFUL /*<< SCB_CPUID_REVISION_Pos*/)          /*!< SCB 
 480:Drivers/CMSIS/Include/core_cm4.h **** 
 481:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Interrupt Control State Register Definitions */
 482:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_NMIPENDSET_Pos            31U                                            /*!< SCB 
 483:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_NMIPENDSET_Msk            (1UL << SCB_ICSR_NMIPENDSET_Pos)               /*!< SCB 
 484:Drivers/CMSIS/Include/core_cm4.h **** 
 485:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSVSET_Pos             28U                                            /*!< SCB 
 486:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSVSET_Msk             (1UL << SCB_ICSR_PENDSVSET_Pos)                /*!< SCB 
 487:Drivers/CMSIS/Include/core_cm4.h **** 
 488:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSVCLR_Pos             27U                                            /*!< SCB 
 489:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSVCLR_Msk             (1UL << SCB_ICSR_PENDSVCLR_Pos)                /*!< SCB 
 490:Drivers/CMSIS/Include/core_cm4.h **** 
 491:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSTSET_Pos             26U                                            /*!< SCB 
 492:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSTSET_Msk             (1UL << SCB_ICSR_PENDSTSET_Pos)                /*!< SCB 
 493:Drivers/CMSIS/Include/core_cm4.h **** 
 494:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSTCLR_Pos             25U                                            /*!< SCB 
 495:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_PENDSTCLR_Msk             (1UL << SCB_ICSR_PENDSTCLR_Pos)                /*!< SCB 
 496:Drivers/CMSIS/Include/core_cm4.h **** 
 497:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_ISRPREEMPT_Pos            23U                                            /*!< SCB 
ARM GAS  /tmp/ccPRqU3T.s 			page 13


 498:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_ISRPREEMPT_Msk            (1UL << SCB_ICSR_ISRPREEMPT_Pos)               /*!< SCB 
 499:Drivers/CMSIS/Include/core_cm4.h **** 
 500:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_ISRPENDING_Pos            22U                                            /*!< SCB 
 501:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_ISRPENDING_Msk            (1UL << SCB_ICSR_ISRPENDING_Pos)               /*!< SCB 
 502:Drivers/CMSIS/Include/core_cm4.h **** 
 503:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_VECTPENDING_Pos           12U                                            /*!< SCB 
 504:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_VECTPENDING_Msk           (0x1FFUL << SCB_ICSR_VECTPENDING_Pos)          /*!< SCB 
 505:Drivers/CMSIS/Include/core_cm4.h **** 
 506:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_RETTOBASE_Pos             11U                                            /*!< SCB 
 507:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_RETTOBASE_Msk             (1UL << SCB_ICSR_RETTOBASE_Pos)                /*!< SCB 
 508:Drivers/CMSIS/Include/core_cm4.h **** 
 509:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_VECTACTIVE_Pos             0U                                            /*!< SCB 
 510:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_ICSR_VECTACTIVE_Msk            (0x1FFUL /*<< SCB_ICSR_VECTACTIVE_Pos*/)       /*!< SCB 
 511:Drivers/CMSIS/Include/core_cm4.h **** 
 512:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Vector Table Offset Register Definitions */
 513:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_VTOR_TBLOFF_Pos                 7U                                            /*!< SCB 
 514:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_VTOR_TBLOFF_Msk                (0x1FFFFFFUL << SCB_VTOR_TBLOFF_Pos)           /*!< SCB 
 515:Drivers/CMSIS/Include/core_cm4.h **** 
 516:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Application Interrupt and Reset Control Register Definitions */
 517:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTKEY_Pos              16U                                            /*!< SCB 
 518:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTKEY_Msk              (0xFFFFUL << SCB_AIRCR_VECTKEY_Pos)            /*!< SCB 
 519:Drivers/CMSIS/Include/core_cm4.h **** 
 520:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTKEYSTAT_Pos          16U                                            /*!< SCB 
 521:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTKEYSTAT_Msk          (0xFFFFUL << SCB_AIRCR_VECTKEYSTAT_Pos)        /*!< SCB 
 522:Drivers/CMSIS/Include/core_cm4.h **** 
 523:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_ENDIANESS_Pos            15U                                            /*!< SCB 
 524:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_ENDIANESS_Msk            (1UL << SCB_AIRCR_ENDIANESS_Pos)               /*!< SCB 
 525:Drivers/CMSIS/Include/core_cm4.h **** 
 526:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_PRIGROUP_Pos              8U                                            /*!< SCB 
 527:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_PRIGROUP_Msk             (7UL << SCB_AIRCR_PRIGROUP_Pos)                /*!< SCB 
 528:Drivers/CMSIS/Include/core_cm4.h **** 
 529:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_SYSRESETREQ_Pos           2U                                            /*!< SCB 
 530:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_SYSRESETREQ_Msk          (1UL << SCB_AIRCR_SYSRESETREQ_Pos)             /*!< SCB 
 531:Drivers/CMSIS/Include/core_cm4.h **** 
 532:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTCLRACTIVE_Pos         1U                                            /*!< SCB 
 533:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTCLRACTIVE_Msk        (1UL << SCB_AIRCR_VECTCLRACTIVE_Pos)           /*!< SCB 
 534:Drivers/CMSIS/Include/core_cm4.h **** 
 535:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTRESET_Pos             0U                                            /*!< SCB 
 536:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_AIRCR_VECTRESET_Msk            (1UL /*<< SCB_AIRCR_VECTRESET_Pos*/)           /*!< SCB 
 537:Drivers/CMSIS/Include/core_cm4.h **** 
 538:Drivers/CMSIS/Include/core_cm4.h **** /* SCB System Control Register Definitions */
 539:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SCR_SEVONPEND_Pos               4U                                            /*!< SCB 
 540:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SCR_SEVONPEND_Msk              (1UL << SCB_SCR_SEVONPEND_Pos)                 /*!< SCB 
 541:Drivers/CMSIS/Include/core_cm4.h **** 
 542:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SCR_SLEEPDEEP_Pos               2U                                            /*!< SCB 
 543:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SCR_SLEEPDEEP_Msk              (1UL << SCB_SCR_SLEEPDEEP_Pos)                 /*!< SCB 
 544:Drivers/CMSIS/Include/core_cm4.h **** 
 545:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SCR_SLEEPONEXIT_Pos             1U                                            /*!< SCB 
 546:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SCR_SLEEPONEXIT_Msk            (1UL << SCB_SCR_SLEEPONEXIT_Pos)               /*!< SCB 
 547:Drivers/CMSIS/Include/core_cm4.h **** 
 548:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Configuration Control Register Definitions */
 549:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_STKALIGN_Pos                9U                                            /*!< SCB 
 550:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_STKALIGN_Msk               (1UL << SCB_CCR_STKALIGN_Pos)                  /*!< SCB 
 551:Drivers/CMSIS/Include/core_cm4.h **** 
 552:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_BFHFNMIGN_Pos               8U                                            /*!< SCB 
 553:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_BFHFNMIGN_Msk              (1UL << SCB_CCR_BFHFNMIGN_Pos)                 /*!< SCB 
 554:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 14


 555:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_DIV_0_TRP_Pos               4U                                            /*!< SCB 
 556:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_DIV_0_TRP_Msk              (1UL << SCB_CCR_DIV_0_TRP_Pos)                 /*!< SCB 
 557:Drivers/CMSIS/Include/core_cm4.h **** 
 558:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_UNALIGN_TRP_Pos             3U                                            /*!< SCB 
 559:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_UNALIGN_TRP_Msk            (1UL << SCB_CCR_UNALIGN_TRP_Pos)               /*!< SCB 
 560:Drivers/CMSIS/Include/core_cm4.h **** 
 561:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_USERSETMPEND_Pos            1U                                            /*!< SCB 
 562:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_USERSETMPEND_Msk           (1UL << SCB_CCR_USERSETMPEND_Pos)              /*!< SCB 
 563:Drivers/CMSIS/Include/core_cm4.h **** 
 564:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_NONBASETHRDENA_Pos          0U                                            /*!< SCB 
 565:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CCR_NONBASETHRDENA_Msk         (1UL /*<< SCB_CCR_NONBASETHRDENA_Pos*/)        /*!< SCB 
 566:Drivers/CMSIS/Include/core_cm4.h **** 
 567:Drivers/CMSIS/Include/core_cm4.h **** /* SCB System Handler Control and State Register Definitions */
 568:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_USGFAULTENA_Pos          18U                                            /*!< SCB 
 569:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_USGFAULTENA_Msk          (1UL << SCB_SHCSR_USGFAULTENA_Pos)             /*!< SCB 
 570:Drivers/CMSIS/Include/core_cm4.h **** 
 571:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_BUSFAULTENA_Pos          17U                                            /*!< SCB 
 572:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_BUSFAULTENA_Msk          (1UL << SCB_SHCSR_BUSFAULTENA_Pos)             /*!< SCB 
 573:Drivers/CMSIS/Include/core_cm4.h **** 
 574:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MEMFAULTENA_Pos          16U                                            /*!< SCB 
 575:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MEMFAULTENA_Msk          (1UL << SCB_SHCSR_MEMFAULTENA_Pos)             /*!< SCB 
 576:Drivers/CMSIS/Include/core_cm4.h **** 
 577:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_SVCALLPENDED_Pos         15U                                            /*!< SCB 
 578:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_SVCALLPENDED_Msk         (1UL << SCB_SHCSR_SVCALLPENDED_Pos)            /*!< SCB 
 579:Drivers/CMSIS/Include/core_cm4.h **** 
 580:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_BUSFAULTPENDED_Pos       14U                                            /*!< SCB 
 581:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_BUSFAULTPENDED_Msk       (1UL << SCB_SHCSR_BUSFAULTPENDED_Pos)          /*!< SCB 
 582:Drivers/CMSIS/Include/core_cm4.h **** 
 583:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MEMFAULTPENDED_Pos       13U                                            /*!< SCB 
 584:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MEMFAULTPENDED_Msk       (1UL << SCB_SHCSR_MEMFAULTPENDED_Pos)          /*!< SCB 
 585:Drivers/CMSIS/Include/core_cm4.h **** 
 586:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_USGFAULTPENDED_Pos       12U                                            /*!< SCB 
 587:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_USGFAULTPENDED_Msk       (1UL << SCB_SHCSR_USGFAULTPENDED_Pos)          /*!< SCB 
 588:Drivers/CMSIS/Include/core_cm4.h **** 
 589:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_SYSTICKACT_Pos           11U                                            /*!< SCB 
 590:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_SYSTICKACT_Msk           (1UL << SCB_SHCSR_SYSTICKACT_Pos)              /*!< SCB 
 591:Drivers/CMSIS/Include/core_cm4.h **** 
 592:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_PENDSVACT_Pos            10U                                            /*!< SCB 
 593:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_PENDSVACT_Msk            (1UL << SCB_SHCSR_PENDSVACT_Pos)               /*!< SCB 
 594:Drivers/CMSIS/Include/core_cm4.h **** 
 595:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MONITORACT_Pos            8U                                            /*!< SCB 
 596:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MONITORACT_Msk           (1UL << SCB_SHCSR_MONITORACT_Pos)              /*!< SCB 
 597:Drivers/CMSIS/Include/core_cm4.h **** 
 598:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_SVCALLACT_Pos             7U                                            /*!< SCB 
 599:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_SVCALLACT_Msk            (1UL << SCB_SHCSR_SVCALLACT_Pos)               /*!< SCB 
 600:Drivers/CMSIS/Include/core_cm4.h **** 
 601:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_USGFAULTACT_Pos           3U                                            /*!< SCB 
 602:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_USGFAULTACT_Msk          (1UL << SCB_SHCSR_USGFAULTACT_Pos)             /*!< SCB 
 603:Drivers/CMSIS/Include/core_cm4.h **** 
 604:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_BUSFAULTACT_Pos           1U                                            /*!< SCB 
 605:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_BUSFAULTACT_Msk          (1UL << SCB_SHCSR_BUSFAULTACT_Pos)             /*!< SCB 
 606:Drivers/CMSIS/Include/core_cm4.h **** 
 607:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MEMFAULTACT_Pos           0U                                            /*!< SCB 
 608:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_SHCSR_MEMFAULTACT_Msk          (1UL /*<< SCB_SHCSR_MEMFAULTACT_Pos*/)         /*!< SCB 
 609:Drivers/CMSIS/Include/core_cm4.h **** 
 610:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Configurable Fault Status Register Definitions */
 611:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_USGFAULTSR_Pos            16U                                            /*!< SCB 
ARM GAS  /tmp/ccPRqU3T.s 			page 15


 612:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_USGFAULTSR_Msk            (0xFFFFUL << SCB_CFSR_USGFAULTSR_Pos)          /*!< SCB 
 613:Drivers/CMSIS/Include/core_cm4.h **** 
 614:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_BUSFAULTSR_Pos             8U                                            /*!< SCB 
 615:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_BUSFAULTSR_Msk            (0xFFUL << SCB_CFSR_BUSFAULTSR_Pos)            /*!< SCB 
 616:Drivers/CMSIS/Include/core_cm4.h **** 
 617:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MEMFAULTSR_Pos             0U                                            /*!< SCB 
 618:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MEMFAULTSR_Msk            (0xFFUL /*<< SCB_CFSR_MEMFAULTSR_Pos*/)        /*!< SCB 
 619:Drivers/CMSIS/Include/core_cm4.h **** 
 620:Drivers/CMSIS/Include/core_cm4.h **** /* MemManage Fault Status Register (part of SCB Configurable Fault Status Register) */
 621:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MMARVALID_Pos             (SCB_SHCSR_MEMFAULTACT_Pos + 7U)               /*!< SCB 
 622:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MMARVALID_Msk             (1UL << SCB_CFSR_MMARVALID_Pos)                /*!< SCB 
 623:Drivers/CMSIS/Include/core_cm4.h **** 
 624:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MLSPERR_Pos               (SCB_SHCSR_MEMFAULTACT_Pos + 5U)               /*!< SCB 
 625:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MLSPERR_Msk               (1UL << SCB_CFSR_MLSPERR_Pos)                  /*!< SCB 
 626:Drivers/CMSIS/Include/core_cm4.h **** 
 627:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MSTKERR_Pos               (SCB_SHCSR_MEMFAULTACT_Pos + 4U)               /*!< SCB 
 628:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MSTKERR_Msk               (1UL << SCB_CFSR_MSTKERR_Pos)                  /*!< SCB 
 629:Drivers/CMSIS/Include/core_cm4.h **** 
 630:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MUNSTKERR_Pos             (SCB_SHCSR_MEMFAULTACT_Pos + 3U)               /*!< SCB 
 631:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_MUNSTKERR_Msk             (1UL << SCB_CFSR_MUNSTKERR_Pos)                /*!< SCB 
 632:Drivers/CMSIS/Include/core_cm4.h **** 
 633:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_DACCVIOL_Pos              (SCB_SHCSR_MEMFAULTACT_Pos + 1U)               /*!< SCB 
 634:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_DACCVIOL_Msk              (1UL << SCB_CFSR_DACCVIOL_Pos)                 /*!< SCB 
 635:Drivers/CMSIS/Include/core_cm4.h **** 
 636:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_IACCVIOL_Pos              (SCB_SHCSR_MEMFAULTACT_Pos + 0U)               /*!< SCB 
 637:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_IACCVIOL_Msk              (1UL /*<< SCB_CFSR_IACCVIOL_Pos*/)             /*!< SCB 
 638:Drivers/CMSIS/Include/core_cm4.h **** 
 639:Drivers/CMSIS/Include/core_cm4.h **** /* BusFault Status Register (part of SCB Configurable Fault Status Register) */
 640:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_BFARVALID_Pos            (SCB_CFSR_BUSFAULTSR_Pos + 7U)                  /*!< SCB 
 641:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_BFARVALID_Msk            (1UL << SCB_CFSR_BFARVALID_Pos)                 /*!< SCB 
 642:Drivers/CMSIS/Include/core_cm4.h **** 
 643:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_LSPERR_Pos               (SCB_CFSR_BUSFAULTSR_Pos + 5U)                  /*!< SCB 
 644:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_LSPERR_Msk               (1UL << SCB_CFSR_LSPERR_Pos)                    /*!< SCB 
 645:Drivers/CMSIS/Include/core_cm4.h **** 
 646:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_STKERR_Pos               (SCB_CFSR_BUSFAULTSR_Pos + 4U)                  /*!< SCB 
 647:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_STKERR_Msk               (1UL << SCB_CFSR_STKERR_Pos)                    /*!< SCB 
 648:Drivers/CMSIS/Include/core_cm4.h **** 
 649:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_UNSTKERR_Pos             (SCB_CFSR_BUSFAULTSR_Pos + 3U)                  /*!< SCB 
 650:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_UNSTKERR_Msk             (1UL << SCB_CFSR_UNSTKERR_Pos)                  /*!< SCB 
 651:Drivers/CMSIS/Include/core_cm4.h **** 
 652:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_IMPRECISERR_Pos          (SCB_CFSR_BUSFAULTSR_Pos + 2U)                  /*!< SCB 
 653:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_IMPRECISERR_Msk          (1UL << SCB_CFSR_IMPRECISERR_Pos)               /*!< SCB 
 654:Drivers/CMSIS/Include/core_cm4.h **** 
 655:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_PRECISERR_Pos            (SCB_CFSR_BUSFAULTSR_Pos + 1U)                  /*!< SCB 
 656:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_PRECISERR_Msk            (1UL << SCB_CFSR_PRECISERR_Pos)                 /*!< SCB 
 657:Drivers/CMSIS/Include/core_cm4.h **** 
 658:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_IBUSERR_Pos              (SCB_CFSR_BUSFAULTSR_Pos + 0U)                  /*!< SCB 
 659:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_IBUSERR_Msk              (1UL << SCB_CFSR_IBUSERR_Pos)                   /*!< SCB 
 660:Drivers/CMSIS/Include/core_cm4.h **** 
 661:Drivers/CMSIS/Include/core_cm4.h **** /* UsageFault Status Register (part of SCB Configurable Fault Status Register) */
 662:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_DIVBYZERO_Pos            (SCB_CFSR_USGFAULTSR_Pos + 9U)                  /*!< SCB 
 663:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_DIVBYZERO_Msk            (1UL << SCB_CFSR_DIVBYZERO_Pos)                 /*!< SCB 
 664:Drivers/CMSIS/Include/core_cm4.h **** 
 665:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_UNALIGNED_Pos            (SCB_CFSR_USGFAULTSR_Pos + 8U)                  /*!< SCB 
 666:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_UNALIGNED_Msk            (1UL << SCB_CFSR_UNALIGNED_Pos)                 /*!< SCB 
 667:Drivers/CMSIS/Include/core_cm4.h **** 
 668:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_NOCP_Pos                 (SCB_CFSR_USGFAULTSR_Pos + 3U)                  /*!< SCB 
ARM GAS  /tmp/ccPRqU3T.s 			page 16


 669:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_NOCP_Msk                 (1UL << SCB_CFSR_NOCP_Pos)                      /*!< SCB 
 670:Drivers/CMSIS/Include/core_cm4.h **** 
 671:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_INVPC_Pos                (SCB_CFSR_USGFAULTSR_Pos + 2U)                  /*!< SCB 
 672:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_INVPC_Msk                (1UL << SCB_CFSR_INVPC_Pos)                     /*!< SCB 
 673:Drivers/CMSIS/Include/core_cm4.h **** 
 674:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_INVSTATE_Pos             (SCB_CFSR_USGFAULTSR_Pos + 1U)                  /*!< SCB 
 675:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_INVSTATE_Msk             (1UL << SCB_CFSR_INVSTATE_Pos)                  /*!< SCB 
 676:Drivers/CMSIS/Include/core_cm4.h **** 
 677:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_UNDEFINSTR_Pos           (SCB_CFSR_USGFAULTSR_Pos + 0U)                  /*!< SCB 
 678:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_CFSR_UNDEFINSTR_Msk           (1UL << SCB_CFSR_UNDEFINSTR_Pos)                /*!< SCB 
 679:Drivers/CMSIS/Include/core_cm4.h **** 
 680:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Hard Fault Status Register Definitions */
 681:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_HFSR_DEBUGEVT_Pos              31U                                            /*!< SCB 
 682:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_HFSR_DEBUGEVT_Msk              (1UL << SCB_HFSR_DEBUGEVT_Pos)                 /*!< SCB 
 683:Drivers/CMSIS/Include/core_cm4.h **** 
 684:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_HFSR_FORCED_Pos                30U                                            /*!< SCB 
 685:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_HFSR_FORCED_Msk                (1UL << SCB_HFSR_FORCED_Pos)                   /*!< SCB 
 686:Drivers/CMSIS/Include/core_cm4.h **** 
 687:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_HFSR_VECTTBL_Pos                1U                                            /*!< SCB 
 688:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_HFSR_VECTTBL_Msk               (1UL << SCB_HFSR_VECTTBL_Pos)                  /*!< SCB 
 689:Drivers/CMSIS/Include/core_cm4.h **** 
 690:Drivers/CMSIS/Include/core_cm4.h **** /* SCB Debug Fault Status Register Definitions */
 691:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_EXTERNAL_Pos               4U                                            /*!< SCB 
 692:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_EXTERNAL_Msk              (1UL << SCB_DFSR_EXTERNAL_Pos)                 /*!< SCB 
 693:Drivers/CMSIS/Include/core_cm4.h **** 
 694:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_VCATCH_Pos                 3U                                            /*!< SCB 
 695:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_VCATCH_Msk                (1UL << SCB_DFSR_VCATCH_Pos)                   /*!< SCB 
 696:Drivers/CMSIS/Include/core_cm4.h **** 
 697:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_DWTTRAP_Pos                2U                                            /*!< SCB 
 698:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_DWTTRAP_Msk               (1UL << SCB_DFSR_DWTTRAP_Pos)                  /*!< SCB 
 699:Drivers/CMSIS/Include/core_cm4.h **** 
 700:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_BKPT_Pos                   1U                                            /*!< SCB 
 701:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_BKPT_Msk                  (1UL << SCB_DFSR_BKPT_Pos)                     /*!< SCB 
 702:Drivers/CMSIS/Include/core_cm4.h **** 
 703:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_HALTED_Pos                 0U                                            /*!< SCB 
 704:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_DFSR_HALTED_Msk                (1UL /*<< SCB_DFSR_HALTED_Pos*/)               /*!< SCB 
 705:Drivers/CMSIS/Include/core_cm4.h **** 
 706:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_SCB */
 707:Drivers/CMSIS/Include/core_cm4.h **** 
 708:Drivers/CMSIS/Include/core_cm4.h **** 
 709:Drivers/CMSIS/Include/core_cm4.h **** /**
 710:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
 711:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_SCnSCB System Controls not in SCB (SCnSCB)
 712:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the System Control and ID Register not in the SCB
 713:Drivers/CMSIS/Include/core_cm4.h ****   @{
 714:Drivers/CMSIS/Include/core_cm4.h ****  */
 715:Drivers/CMSIS/Include/core_cm4.h **** 
 716:Drivers/CMSIS/Include/core_cm4.h **** /**
 717:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the System Control and ID Register not in the SCB.
 718:Drivers/CMSIS/Include/core_cm4.h ****  */
 719:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
 720:Drivers/CMSIS/Include/core_cm4.h **** {
 721:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[1U];
 722:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t ICTR;                   /*!< Offset: 0x004 (R/ )  Interrupt Controller Type Regist
 723:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ACTLR;                  /*!< Offset: 0x008 (R/W)  Auxiliary Control Register */
 724:Drivers/CMSIS/Include/core_cm4.h **** } SCnSCB_Type;
 725:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 17


 726:Drivers/CMSIS/Include/core_cm4.h **** /* Interrupt Controller Type Register Definitions */
 727:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ICTR_INTLINESNUM_Pos         0U                                         /*!< ICTR: I
 728:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ICTR_INTLINESNUM_Msk        (0xFUL /*<< SCnSCB_ICTR_INTLINESNUM_Pos*/)  /*!< ICTR: I
 729:Drivers/CMSIS/Include/core_cm4.h **** 
 730:Drivers/CMSIS/Include/core_cm4.h **** /* Auxiliary Control Register Definitions */
 731:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISOOFP_Pos            9U                                         /*!< ACTLR: 
 732:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISOOFP_Msk           (1UL << SCnSCB_ACTLR_DISOOFP_Pos)           /*!< ACTLR: 
 733:Drivers/CMSIS/Include/core_cm4.h **** 
 734:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISFPCA_Pos            8U                                         /*!< ACTLR: 
 735:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISFPCA_Msk           (1UL << SCnSCB_ACTLR_DISFPCA_Pos)           /*!< ACTLR: 
 736:Drivers/CMSIS/Include/core_cm4.h **** 
 737:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISFOLD_Pos            2U                                         /*!< ACTLR: 
 738:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISFOLD_Msk           (1UL << SCnSCB_ACTLR_DISFOLD_Pos)           /*!< ACTLR: 
 739:Drivers/CMSIS/Include/core_cm4.h **** 
 740:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISDEFWBUF_Pos         1U                                         /*!< ACTLR: 
 741:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISDEFWBUF_Msk        (1UL << SCnSCB_ACTLR_DISDEFWBUF_Pos)        /*!< ACTLR: 
 742:Drivers/CMSIS/Include/core_cm4.h **** 
 743:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISMCYCINT_Pos         0U                                         /*!< ACTLR: 
 744:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB_ACTLR_DISMCYCINT_Msk        (1UL /*<< SCnSCB_ACTLR_DISMCYCINT_Pos*/)    /*!< ACTLR: 
 745:Drivers/CMSIS/Include/core_cm4.h **** 
 746:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_SCnotSCB */
 747:Drivers/CMSIS/Include/core_cm4.h **** 
 748:Drivers/CMSIS/Include/core_cm4.h **** 
 749:Drivers/CMSIS/Include/core_cm4.h **** /**
 750:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
 751:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_SysTick     System Tick Timer (SysTick)
 752:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the System Timer Registers.
 753:Drivers/CMSIS/Include/core_cm4.h ****   @{
 754:Drivers/CMSIS/Include/core_cm4.h ****  */
 755:Drivers/CMSIS/Include/core_cm4.h **** 
 756:Drivers/CMSIS/Include/core_cm4.h **** /**
 757:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the System Timer (SysTick).
 758:Drivers/CMSIS/Include/core_cm4.h ****  */
 759:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
 760:Drivers/CMSIS/Include/core_cm4.h **** {
 761:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CTRL;                   /*!< Offset: 0x000 (R/W)  SysTick Control and Status Regis
 762:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t LOAD;                   /*!< Offset: 0x004 (R/W)  SysTick Reload Value Register */
 763:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t VAL;                    /*!< Offset: 0x008 (R/W)  SysTick Current Value Register *
 764:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t CALIB;                  /*!< Offset: 0x00C (R/ )  SysTick Calibration Register */
 765:Drivers/CMSIS/Include/core_cm4.h **** } SysTick_Type;
 766:Drivers/CMSIS/Include/core_cm4.h **** 
 767:Drivers/CMSIS/Include/core_cm4.h **** /* SysTick Control / Status Register Definitions */
 768:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_COUNTFLAG_Pos         16U                                            /*!< SysT
 769:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_COUNTFLAG_Msk         (1UL << SysTick_CTRL_COUNTFLAG_Pos)            /*!< SysT
 770:Drivers/CMSIS/Include/core_cm4.h **** 
 771:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_CLKSOURCE_Pos          2U                                            /*!< SysT
 772:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_CLKSOURCE_Msk         (1UL << SysTick_CTRL_CLKSOURCE_Pos)            /*!< SysT
 773:Drivers/CMSIS/Include/core_cm4.h **** 
 774:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_TICKINT_Pos            1U                                            /*!< SysT
 775:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_TICKINT_Msk           (1UL << SysTick_CTRL_TICKINT_Pos)              /*!< SysT
 776:Drivers/CMSIS/Include/core_cm4.h **** 
 777:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_ENABLE_Pos             0U                                            /*!< SysT
 778:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CTRL_ENABLE_Msk            (1UL /*<< SysTick_CTRL_ENABLE_Pos*/)           /*!< SysT
 779:Drivers/CMSIS/Include/core_cm4.h **** 
 780:Drivers/CMSIS/Include/core_cm4.h **** /* SysTick Reload Register Definitions */
 781:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_LOAD_RELOAD_Pos             0U                                            /*!< SysT
 782:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_LOAD_RELOAD_Msk            (0xFFFFFFUL /*<< SysTick_LOAD_RELOAD_Pos*/)    /*!< SysT
ARM GAS  /tmp/ccPRqU3T.s 			page 18


 783:Drivers/CMSIS/Include/core_cm4.h **** 
 784:Drivers/CMSIS/Include/core_cm4.h **** /* SysTick Current Register Definitions */
 785:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_VAL_CURRENT_Pos             0U                                            /*!< SysT
 786:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_VAL_CURRENT_Msk            (0xFFFFFFUL /*<< SysTick_VAL_CURRENT_Pos*/)    /*!< SysT
 787:Drivers/CMSIS/Include/core_cm4.h **** 
 788:Drivers/CMSIS/Include/core_cm4.h **** /* SysTick Calibration Register Definitions */
 789:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CALIB_NOREF_Pos            31U                                            /*!< SysT
 790:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CALIB_NOREF_Msk            (1UL << SysTick_CALIB_NOREF_Pos)               /*!< SysT
 791:Drivers/CMSIS/Include/core_cm4.h **** 
 792:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CALIB_SKEW_Pos             30U                                            /*!< SysT
 793:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CALIB_SKEW_Msk             (1UL << SysTick_CALIB_SKEW_Pos)                /*!< SysT
 794:Drivers/CMSIS/Include/core_cm4.h **** 
 795:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CALIB_TENMS_Pos             0U                                            /*!< SysT
 796:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_CALIB_TENMS_Msk            (0xFFFFFFUL /*<< SysTick_CALIB_TENMS_Pos*/)    /*!< SysT
 797:Drivers/CMSIS/Include/core_cm4.h **** 
 798:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_SysTick */
 799:Drivers/CMSIS/Include/core_cm4.h **** 
 800:Drivers/CMSIS/Include/core_cm4.h **** 
 801:Drivers/CMSIS/Include/core_cm4.h **** /**
 802:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
 803:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_ITM     Instrumentation Trace Macrocell (ITM)
 804:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the Instrumentation Trace Macrocell (ITM)
 805:Drivers/CMSIS/Include/core_cm4.h ****   @{
 806:Drivers/CMSIS/Include/core_cm4.h ****  */
 807:Drivers/CMSIS/Include/core_cm4.h **** 
 808:Drivers/CMSIS/Include/core_cm4.h **** /**
 809:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Instrumentation Trace Macrocell Register (ITM).
 810:Drivers/CMSIS/Include/core_cm4.h ****  */
 811:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
 812:Drivers/CMSIS/Include/core_cm4.h **** {
 813:Drivers/CMSIS/Include/core_cm4.h ****   __OM  union
 814:Drivers/CMSIS/Include/core_cm4.h ****   {
 815:Drivers/CMSIS/Include/core_cm4.h ****     __OM  uint8_t    u8;                 /*!< Offset: 0x000 ( /W)  ITM Stimulus Port 8-bit */
 816:Drivers/CMSIS/Include/core_cm4.h ****     __OM  uint16_t   u16;                /*!< Offset: 0x000 ( /W)  ITM Stimulus Port 16-bit */
 817:Drivers/CMSIS/Include/core_cm4.h ****     __OM  uint32_t   u32;                /*!< Offset: 0x000 ( /W)  ITM Stimulus Port 32-bit */
 818:Drivers/CMSIS/Include/core_cm4.h ****   }  PORT [32U];                         /*!< Offset: 0x000 ( /W)  ITM Stimulus Port Registers */
 819:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[864U];
 820:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t TER;                    /*!< Offset: 0xE00 (R/W)  ITM Trace Enable Register */
 821:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED1[15U];
 822:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t TPR;                    /*!< Offset: 0xE40 (R/W)  ITM Trace Privilege Register */
 823:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED2[15U];
 824:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t TCR;                    /*!< Offset: 0xE80 (R/W)  ITM Trace Control Register */
 825:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED3[29U];
 826:Drivers/CMSIS/Include/core_cm4.h ****   __OM  uint32_t IWR;                    /*!< Offset: 0xEF8 ( /W)  ITM Integration Write Register *
 827:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t IRR;                    /*!< Offset: 0xEFC (R/ )  ITM Integration Read Register */
 828:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t IMCR;                   /*!< Offset: 0xF00 (R/W)  ITM Integration Mode Control Reg
 829:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED4[43U];
 830:Drivers/CMSIS/Include/core_cm4.h ****   __OM  uint32_t LAR;                    /*!< Offset: 0xFB0 ( /W)  ITM Lock Access Register */
 831:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t LSR;                    /*!< Offset: 0xFB4 (R/ )  ITM Lock Status Register */
 832:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED5[6U];
 833:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID4;                   /*!< Offset: 0xFD0 (R/ )  ITM Peripheral Identification Re
 834:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID5;                   /*!< Offset: 0xFD4 (R/ )  ITM Peripheral Identification Re
 835:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID6;                   /*!< Offset: 0xFD8 (R/ )  ITM Peripheral Identification Re
 836:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID7;                   /*!< Offset: 0xFDC (R/ )  ITM Peripheral Identification Re
 837:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID0;                   /*!< Offset: 0xFE0 (R/ )  ITM Peripheral Identification Re
 838:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID1;                   /*!< Offset: 0xFE4 (R/ )  ITM Peripheral Identification Re
 839:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID2;                   /*!< Offset: 0xFE8 (R/ )  ITM Peripheral Identification Re
ARM GAS  /tmp/ccPRqU3T.s 			page 19


 840:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PID3;                   /*!< Offset: 0xFEC (R/ )  ITM Peripheral Identification Re
 841:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t CID0;                   /*!< Offset: 0xFF0 (R/ )  ITM Component  Identification Re
 842:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t CID1;                   /*!< Offset: 0xFF4 (R/ )  ITM Component  Identification Re
 843:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t CID2;                   /*!< Offset: 0xFF8 (R/ )  ITM Component  Identification Re
 844:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t CID3;                   /*!< Offset: 0xFFC (R/ )  ITM Component  Identification Re
 845:Drivers/CMSIS/Include/core_cm4.h **** } ITM_Type;
 846:Drivers/CMSIS/Include/core_cm4.h **** 
 847:Drivers/CMSIS/Include/core_cm4.h **** /* ITM Trace Privilege Register Definitions */
 848:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TPR_PRIVMASK_Pos                0U                                            /*!< ITM 
 849:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TPR_PRIVMASK_Msk               (0xFFFFFFFFUL /*<< ITM_TPR_PRIVMASK_Pos*/)     /*!< ITM 
 850:Drivers/CMSIS/Include/core_cm4.h **** 
 851:Drivers/CMSIS/Include/core_cm4.h **** /* ITM Trace Control Register Definitions */
 852:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_BUSY_Pos                   23U                                            /*!< ITM 
 853:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_BUSY_Msk                   (1UL << ITM_TCR_BUSY_Pos)                      /*!< ITM 
 854:Drivers/CMSIS/Include/core_cm4.h **** 
 855:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_TraceBusID_Pos             16U                                            /*!< ITM 
 856:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_TraceBusID_Msk             (0x7FUL << ITM_TCR_TraceBusID_Pos)             /*!< ITM 
 857:Drivers/CMSIS/Include/core_cm4.h **** 
 858:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_GTSFREQ_Pos                10U                                            /*!< ITM 
 859:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_GTSFREQ_Msk                (3UL << ITM_TCR_GTSFREQ_Pos)                   /*!< ITM 
 860:Drivers/CMSIS/Include/core_cm4.h **** 
 861:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_TSPrescale_Pos              8U                                            /*!< ITM 
 862:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_TSPrescale_Msk             (3UL << ITM_TCR_TSPrescale_Pos)                /*!< ITM 
 863:Drivers/CMSIS/Include/core_cm4.h **** 
 864:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_SWOENA_Pos                  4U                                            /*!< ITM 
 865:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_SWOENA_Msk                 (1UL << ITM_TCR_SWOENA_Pos)                    /*!< ITM 
 866:Drivers/CMSIS/Include/core_cm4.h **** 
 867:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_DWTENA_Pos                  3U                                            /*!< ITM 
 868:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_DWTENA_Msk                 (1UL << ITM_TCR_DWTENA_Pos)                    /*!< ITM 
 869:Drivers/CMSIS/Include/core_cm4.h **** 
 870:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_SYNCENA_Pos                 2U                                            /*!< ITM 
 871:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_SYNCENA_Msk                (1UL << ITM_TCR_SYNCENA_Pos)                   /*!< ITM 
 872:Drivers/CMSIS/Include/core_cm4.h **** 
 873:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_TSENA_Pos                   1U                                            /*!< ITM 
 874:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_TSENA_Msk                  (1UL << ITM_TCR_TSENA_Pos)                     /*!< ITM 
 875:Drivers/CMSIS/Include/core_cm4.h **** 
 876:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_ITMENA_Pos                  0U                                            /*!< ITM 
 877:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_TCR_ITMENA_Msk                 (1UL /*<< ITM_TCR_ITMENA_Pos*/)                /*!< ITM 
 878:Drivers/CMSIS/Include/core_cm4.h **** 
 879:Drivers/CMSIS/Include/core_cm4.h **** /* ITM Integration Write Register Definitions */
 880:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_IWR_ATVALIDM_Pos                0U                                            /*!< ITM 
 881:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_IWR_ATVALIDM_Msk               (1UL /*<< ITM_IWR_ATVALIDM_Pos*/)              /*!< ITM 
 882:Drivers/CMSIS/Include/core_cm4.h **** 
 883:Drivers/CMSIS/Include/core_cm4.h **** /* ITM Integration Read Register Definitions */
 884:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_IRR_ATREADYM_Pos                0U                                            /*!< ITM 
 885:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_IRR_ATREADYM_Msk               (1UL /*<< ITM_IRR_ATREADYM_Pos*/)              /*!< ITM 
 886:Drivers/CMSIS/Include/core_cm4.h **** 
 887:Drivers/CMSIS/Include/core_cm4.h **** /* ITM Integration Mode Control Register Definitions */
 888:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_IMCR_INTEGRATION_Pos            0U                                            /*!< ITM 
 889:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_IMCR_INTEGRATION_Msk           (1UL /*<< ITM_IMCR_INTEGRATION_Pos*/)          /*!< ITM 
 890:Drivers/CMSIS/Include/core_cm4.h **** 
 891:Drivers/CMSIS/Include/core_cm4.h **** /* ITM Lock Status Register Definitions */
 892:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_LSR_ByteAcc_Pos                 2U                                            /*!< ITM 
 893:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_LSR_ByteAcc_Msk                (1UL << ITM_LSR_ByteAcc_Pos)                   /*!< ITM 
 894:Drivers/CMSIS/Include/core_cm4.h **** 
 895:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_LSR_Access_Pos                  1U                                            /*!< ITM 
 896:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_LSR_Access_Msk                 (1UL << ITM_LSR_Access_Pos)                    /*!< ITM 
ARM GAS  /tmp/ccPRqU3T.s 			page 20


 897:Drivers/CMSIS/Include/core_cm4.h **** 
 898:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_LSR_Present_Pos                 0U                                            /*!< ITM 
 899:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_LSR_Present_Msk                (1UL /*<< ITM_LSR_Present_Pos*/)               /*!< ITM 
 900:Drivers/CMSIS/Include/core_cm4.h **** 
 901:Drivers/CMSIS/Include/core_cm4.h **** /*@}*/ /* end of group CMSIS_ITM */
 902:Drivers/CMSIS/Include/core_cm4.h **** 
 903:Drivers/CMSIS/Include/core_cm4.h **** 
 904:Drivers/CMSIS/Include/core_cm4.h **** /**
 905:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
 906:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_DWT     Data Watchpoint and Trace (DWT)
 907:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the Data Watchpoint and Trace (DWT)
 908:Drivers/CMSIS/Include/core_cm4.h ****   @{
 909:Drivers/CMSIS/Include/core_cm4.h ****  */
 910:Drivers/CMSIS/Include/core_cm4.h **** 
 911:Drivers/CMSIS/Include/core_cm4.h **** /**
 912:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Data Watchpoint and Trace Register (DWT).
 913:Drivers/CMSIS/Include/core_cm4.h ****  */
 914:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
 915:Drivers/CMSIS/Include/core_cm4.h **** {
 916:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CTRL;                   /*!< Offset: 0x000 (R/W)  Control Register */
 917:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CYCCNT;                 /*!< Offset: 0x004 (R/W)  Cycle Count Register */
 918:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CPICNT;                 /*!< Offset: 0x008 (R/W)  CPI Count Register */
 919:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t EXCCNT;                 /*!< Offset: 0x00C (R/W)  Exception Overhead Count Registe
 920:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t SLEEPCNT;               /*!< Offset: 0x010 (R/W)  Sleep Count Register */
 921:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t LSUCNT;                 /*!< Offset: 0x014 (R/W)  LSU Count Register */
 922:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FOLDCNT;                /*!< Offset: 0x018 (R/W)  Folded-instruction Count Registe
 923:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t PCSR;                   /*!< Offset: 0x01C (R/ )  Program Counter Sample Register 
 924:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t COMP0;                  /*!< Offset: 0x020 (R/W)  Comparator Register 0 */
 925:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t MASK0;                  /*!< Offset: 0x024 (R/W)  Mask Register 0 */
 926:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FUNCTION0;              /*!< Offset: 0x028 (R/W)  Function Register 0 */
 927:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[1U];
 928:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t COMP1;                  /*!< Offset: 0x030 (R/W)  Comparator Register 1 */
 929:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t MASK1;                  /*!< Offset: 0x034 (R/W)  Mask Register 1 */
 930:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FUNCTION1;              /*!< Offset: 0x038 (R/W)  Function Register 1 */
 931:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED1[1U];
 932:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t COMP2;                  /*!< Offset: 0x040 (R/W)  Comparator Register 2 */
 933:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t MASK2;                  /*!< Offset: 0x044 (R/W)  Mask Register 2 */
 934:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FUNCTION2;              /*!< Offset: 0x048 (R/W)  Function Register 2 */
 935:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED2[1U];
 936:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t COMP3;                  /*!< Offset: 0x050 (R/W)  Comparator Register 3 */
 937:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t MASK3;                  /*!< Offset: 0x054 (R/W)  Mask Register 3 */
 938:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FUNCTION3;              /*!< Offset: 0x058 (R/W)  Function Register 3 */
 939:Drivers/CMSIS/Include/core_cm4.h **** } DWT_Type;
 940:Drivers/CMSIS/Include/core_cm4.h **** 
 941:Drivers/CMSIS/Include/core_cm4.h **** /* DWT Control Register Definitions */
 942:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NUMCOMP_Pos               28U                                         /*!< DWT CTR
 943:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NUMCOMP_Msk               (0xFUL << DWT_CTRL_NUMCOMP_Pos)             /*!< DWT CTR
 944:Drivers/CMSIS/Include/core_cm4.h **** 
 945:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOTRCPKT_Pos              27U                                         /*!< DWT CTR
 946:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOTRCPKT_Msk              (0x1UL << DWT_CTRL_NOTRCPKT_Pos)            /*!< DWT CTR
 947:Drivers/CMSIS/Include/core_cm4.h **** 
 948:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOEXTTRIG_Pos             26U                                         /*!< DWT CTR
 949:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOEXTTRIG_Msk             (0x1UL << DWT_CTRL_NOEXTTRIG_Pos)           /*!< DWT CTR
 950:Drivers/CMSIS/Include/core_cm4.h **** 
 951:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOCYCCNT_Pos              25U                                         /*!< DWT CTR
 952:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOCYCCNT_Msk              (0x1UL << DWT_CTRL_NOCYCCNT_Pos)            /*!< DWT CTR
 953:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 21


 954:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOPRFCNT_Pos              24U                                         /*!< DWT CTR
 955:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_NOPRFCNT_Msk              (0x1UL << DWT_CTRL_NOPRFCNT_Pos)            /*!< DWT CTR
 956:Drivers/CMSIS/Include/core_cm4.h **** 
 957:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CYCEVTENA_Pos             22U                                         /*!< DWT CTR
 958:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CYCEVTENA_Msk             (0x1UL << DWT_CTRL_CYCEVTENA_Pos)           /*!< DWT CTR
 959:Drivers/CMSIS/Include/core_cm4.h **** 
 960:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_FOLDEVTENA_Pos            21U                                         /*!< DWT CTR
 961:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_FOLDEVTENA_Msk            (0x1UL << DWT_CTRL_FOLDEVTENA_Pos)          /*!< DWT CTR
 962:Drivers/CMSIS/Include/core_cm4.h **** 
 963:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_LSUEVTENA_Pos             20U                                         /*!< DWT CTR
 964:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_LSUEVTENA_Msk             (0x1UL << DWT_CTRL_LSUEVTENA_Pos)           /*!< DWT CTR
 965:Drivers/CMSIS/Include/core_cm4.h **** 
 966:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_SLEEPEVTENA_Pos           19U                                         /*!< DWT CTR
 967:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_SLEEPEVTENA_Msk           (0x1UL << DWT_CTRL_SLEEPEVTENA_Pos)         /*!< DWT CTR
 968:Drivers/CMSIS/Include/core_cm4.h **** 
 969:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_EXCEVTENA_Pos             18U                                         /*!< DWT CTR
 970:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_EXCEVTENA_Msk             (0x1UL << DWT_CTRL_EXCEVTENA_Pos)           /*!< DWT CTR
 971:Drivers/CMSIS/Include/core_cm4.h **** 
 972:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CPIEVTENA_Pos             17U                                         /*!< DWT CTR
 973:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CPIEVTENA_Msk             (0x1UL << DWT_CTRL_CPIEVTENA_Pos)           /*!< DWT CTR
 974:Drivers/CMSIS/Include/core_cm4.h **** 
 975:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_EXCTRCENA_Pos             16U                                         /*!< DWT CTR
 976:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_EXCTRCENA_Msk             (0x1UL << DWT_CTRL_EXCTRCENA_Pos)           /*!< DWT CTR
 977:Drivers/CMSIS/Include/core_cm4.h **** 
 978:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_PCSAMPLENA_Pos            12U                                         /*!< DWT CTR
 979:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_PCSAMPLENA_Msk            (0x1UL << DWT_CTRL_PCSAMPLENA_Pos)          /*!< DWT CTR
 980:Drivers/CMSIS/Include/core_cm4.h **** 
 981:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_SYNCTAP_Pos               10U                                         /*!< DWT CTR
 982:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_SYNCTAP_Msk               (0x3UL << DWT_CTRL_SYNCTAP_Pos)             /*!< DWT CTR
 983:Drivers/CMSIS/Include/core_cm4.h **** 
 984:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CYCTAP_Pos                 9U                                         /*!< DWT CTR
 985:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CYCTAP_Msk                (0x1UL << DWT_CTRL_CYCTAP_Pos)              /*!< DWT CTR
 986:Drivers/CMSIS/Include/core_cm4.h **** 
 987:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_POSTINIT_Pos               5U                                         /*!< DWT CTR
 988:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_POSTINIT_Msk              (0xFUL << DWT_CTRL_POSTINIT_Pos)            /*!< DWT CTR
 989:Drivers/CMSIS/Include/core_cm4.h **** 
 990:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_POSTPRESET_Pos             1U                                         /*!< DWT CTR
 991:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_POSTPRESET_Msk            (0xFUL << DWT_CTRL_POSTPRESET_Pos)          /*!< DWT CTR
 992:Drivers/CMSIS/Include/core_cm4.h **** 
 993:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CYCCNTENA_Pos              0U                                         /*!< DWT CTR
 994:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CTRL_CYCCNTENA_Msk             (0x1UL /*<< DWT_CTRL_CYCCNTENA_Pos*/)       /*!< DWT CTR
 995:Drivers/CMSIS/Include/core_cm4.h **** 
 996:Drivers/CMSIS/Include/core_cm4.h **** /* DWT CPI Count Register Definitions */
 997:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CPICNT_CPICNT_Pos               0U                                         /*!< DWT CPI
 998:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_CPICNT_CPICNT_Msk              (0xFFUL /*<< DWT_CPICNT_CPICNT_Pos*/)       /*!< DWT CPI
 999:Drivers/CMSIS/Include/core_cm4.h **** 
1000:Drivers/CMSIS/Include/core_cm4.h **** /* DWT Exception Overhead Count Register Definitions */
1001:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_EXCCNT_EXCCNT_Pos               0U                                         /*!< DWT EXC
1002:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_EXCCNT_EXCCNT_Msk              (0xFFUL /*<< DWT_EXCCNT_EXCCNT_Pos*/)       /*!< DWT EXC
1003:Drivers/CMSIS/Include/core_cm4.h **** 
1004:Drivers/CMSIS/Include/core_cm4.h **** /* DWT Sleep Count Register Definitions */
1005:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_SLEEPCNT_SLEEPCNT_Pos           0U                                         /*!< DWT SLE
1006:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_SLEEPCNT_SLEEPCNT_Msk          (0xFFUL /*<< DWT_SLEEPCNT_SLEEPCNT_Pos*/)   /*!< DWT SLE
1007:Drivers/CMSIS/Include/core_cm4.h **** 
1008:Drivers/CMSIS/Include/core_cm4.h **** /* DWT LSU Count Register Definitions */
1009:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_LSUCNT_LSUCNT_Pos               0U                                         /*!< DWT LSU
1010:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_LSUCNT_LSUCNT_Msk              (0xFFUL /*<< DWT_LSUCNT_LSUCNT_Pos*/)       /*!< DWT LSU
ARM GAS  /tmp/ccPRqU3T.s 			page 22


1011:Drivers/CMSIS/Include/core_cm4.h **** 
1012:Drivers/CMSIS/Include/core_cm4.h **** /* DWT Folded-instruction Count Register Definitions */
1013:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FOLDCNT_FOLDCNT_Pos             0U                                         /*!< DWT FOL
1014:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FOLDCNT_FOLDCNT_Msk            (0xFFUL /*<< DWT_FOLDCNT_FOLDCNT_Pos*/)     /*!< DWT FOL
1015:Drivers/CMSIS/Include/core_cm4.h **** 
1016:Drivers/CMSIS/Include/core_cm4.h **** /* DWT Comparator Mask Register Definitions */
1017:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_MASK_MASK_Pos                   0U                                         /*!< DWT MAS
1018:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_MASK_MASK_Msk                  (0x1FUL /*<< DWT_MASK_MASK_Pos*/)           /*!< DWT MAS
1019:Drivers/CMSIS/Include/core_cm4.h **** 
1020:Drivers/CMSIS/Include/core_cm4.h **** /* DWT Comparator Function Register Definitions */
1021:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_MATCHED_Pos           24U                                         /*!< DWT FUN
1022:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_MATCHED_Msk           (0x1UL << DWT_FUNCTION_MATCHED_Pos)         /*!< DWT FUN
1023:Drivers/CMSIS/Include/core_cm4.h **** 
1024:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVADDR1_Pos        16U                                         /*!< DWT FUN
1025:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVADDR1_Msk        (0xFUL << DWT_FUNCTION_DATAVADDR1_Pos)      /*!< DWT FUN
1026:Drivers/CMSIS/Include/core_cm4.h **** 
1027:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVADDR0_Pos        12U                                         /*!< DWT FUN
1028:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVADDR0_Msk        (0xFUL << DWT_FUNCTION_DATAVADDR0_Pos)      /*!< DWT FUN
1029:Drivers/CMSIS/Include/core_cm4.h **** 
1030:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVSIZE_Pos         10U                                         /*!< DWT FUN
1031:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVSIZE_Msk         (0x3UL << DWT_FUNCTION_DATAVSIZE_Pos)       /*!< DWT FUN
1032:Drivers/CMSIS/Include/core_cm4.h **** 
1033:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_LNK1ENA_Pos            9U                                         /*!< DWT FUN
1034:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_LNK1ENA_Msk           (0x1UL << DWT_FUNCTION_LNK1ENA_Pos)         /*!< DWT FUN
1035:Drivers/CMSIS/Include/core_cm4.h **** 
1036:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVMATCH_Pos         8U                                         /*!< DWT FUN
1037:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_DATAVMATCH_Msk        (0x1UL << DWT_FUNCTION_DATAVMATCH_Pos)      /*!< DWT FUN
1038:Drivers/CMSIS/Include/core_cm4.h **** 
1039:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_CYCMATCH_Pos           7U                                         /*!< DWT FUN
1040:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_CYCMATCH_Msk          (0x1UL << DWT_FUNCTION_CYCMATCH_Pos)        /*!< DWT FUN
1041:Drivers/CMSIS/Include/core_cm4.h **** 
1042:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_EMITRANGE_Pos          5U                                         /*!< DWT FUN
1043:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_EMITRANGE_Msk         (0x1UL << DWT_FUNCTION_EMITRANGE_Pos)       /*!< DWT FUN
1044:Drivers/CMSIS/Include/core_cm4.h **** 
1045:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_FUNCTION_Pos           0U                                         /*!< DWT FUN
1046:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_FUNCTION_FUNCTION_Msk          (0xFUL /*<< DWT_FUNCTION_FUNCTION_Pos*/)    /*!< DWT FUN
1047:Drivers/CMSIS/Include/core_cm4.h **** 
1048:Drivers/CMSIS/Include/core_cm4.h **** /*@}*/ /* end of group CMSIS_DWT */
1049:Drivers/CMSIS/Include/core_cm4.h **** 
1050:Drivers/CMSIS/Include/core_cm4.h **** 
1051:Drivers/CMSIS/Include/core_cm4.h **** /**
1052:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
1053:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_TPI     Trace Port Interface (TPI)
1054:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the Trace Port Interface (TPI)
1055:Drivers/CMSIS/Include/core_cm4.h ****   @{
1056:Drivers/CMSIS/Include/core_cm4.h ****  */
1057:Drivers/CMSIS/Include/core_cm4.h **** 
1058:Drivers/CMSIS/Include/core_cm4.h **** /**
1059:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Trace Port Interface Register (TPI).
1060:Drivers/CMSIS/Include/core_cm4.h ****  */
1061:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
1062:Drivers/CMSIS/Include/core_cm4.h **** {
1063:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t SSPSR;                  /*!< Offset: 0x000 (R/ )  Supported Parallel Port Size Reg
1064:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CSPSR;                  /*!< Offset: 0x004 (R/W)  Current Parallel Port Size Regis
1065:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[2U];
1066:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ACPR;                   /*!< Offset: 0x010 (R/W)  Asynchronous Clock Prescaler Reg
1067:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED1[55U];
ARM GAS  /tmp/ccPRqU3T.s 			page 23


1068:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t SPPR;                   /*!< Offset: 0x0F0 (R/W)  Selected Pin Protocol Register *
1069:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED2[131U];
1070:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t FFSR;                   /*!< Offset: 0x300 (R/ )  Formatter and Flush Status Regis
1071:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FFCR;                   /*!< Offset: 0x304 (R/W)  Formatter and Flush Control Regi
1072:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t FSCR;                   /*!< Offset: 0x308 (R/ )  Formatter Synchronization Counte
1073:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED3[759U];
1074:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t TRIGGER;                /*!< Offset: 0xEE8 (R/ )  TRIGGER Register */
1075:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t FIFO0;                  /*!< Offset: 0xEEC (R/ )  Integration ETM Data */
1076:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t ITATBCTR2;              /*!< Offset: 0xEF0 (R/ )  ITATBCTR2 */
1077:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED4[1U];
1078:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t ITATBCTR0;              /*!< Offset: 0xEF8 (R/ )  ITATBCTR0 */
1079:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t FIFO1;                  /*!< Offset: 0xEFC (R/ )  Integration ITM Data */
1080:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t ITCTRL;                 /*!< Offset: 0xF00 (R/W)  Integration Mode Control */
1081:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED5[39U];
1082:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CLAIMSET;               /*!< Offset: 0xFA0 (R/W)  Claim tag set */
1083:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CLAIMCLR;               /*!< Offset: 0xFA4 (R/W)  Claim tag clear */
1084:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED7[8U];
1085:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t DEVID;                  /*!< Offset: 0xFC8 (R/ )  TPIU_DEVID */
1086:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t DEVTYPE;                /*!< Offset: 0xFCC (R/ )  TPIU_DEVTYPE */
1087:Drivers/CMSIS/Include/core_cm4.h **** } TPI_Type;
1088:Drivers/CMSIS/Include/core_cm4.h **** 
1089:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Asynchronous Clock Prescaler Register Definitions */
1090:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ACPR_PRESCALER_Pos              0U                                         /*!< TPI ACP
1091:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ACPR_PRESCALER_Msk             (0x1FFFUL /*<< TPI_ACPR_PRESCALER_Pos*/)    /*!< TPI ACP
1092:Drivers/CMSIS/Include/core_cm4.h **** 
1093:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Selected Pin Protocol Register Definitions */
1094:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_SPPR_TXMODE_Pos                 0U                                         /*!< TPI SPP
1095:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_SPPR_TXMODE_Msk                (0x3UL /*<< TPI_SPPR_TXMODE_Pos*/)          /*!< TPI SPP
1096:Drivers/CMSIS/Include/core_cm4.h **** 
1097:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Formatter and Flush Status Register Definitions */
1098:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_FtNonStop_Pos              3U                                         /*!< TPI FFS
1099:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_FtNonStop_Msk             (0x1UL << TPI_FFSR_FtNonStop_Pos)           /*!< TPI FFS
1100:Drivers/CMSIS/Include/core_cm4.h **** 
1101:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_TCPresent_Pos              2U                                         /*!< TPI FFS
1102:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_TCPresent_Msk             (0x1UL << TPI_FFSR_TCPresent_Pos)           /*!< TPI FFS
1103:Drivers/CMSIS/Include/core_cm4.h **** 
1104:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_FtStopped_Pos              1U                                         /*!< TPI FFS
1105:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_FtStopped_Msk             (0x1UL << TPI_FFSR_FtStopped_Pos)           /*!< TPI FFS
1106:Drivers/CMSIS/Include/core_cm4.h **** 
1107:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_FlInProg_Pos               0U                                         /*!< TPI FFS
1108:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFSR_FlInProg_Msk              (0x1UL /*<< TPI_FFSR_FlInProg_Pos*/)        /*!< TPI FFS
1109:Drivers/CMSIS/Include/core_cm4.h **** 
1110:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Formatter and Flush Control Register Definitions */
1111:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFCR_TrigIn_Pos                 8U                                         /*!< TPI FFC
1112:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFCR_TrigIn_Msk                (0x1UL << TPI_FFCR_TrigIn_Pos)              /*!< TPI FFC
1113:Drivers/CMSIS/Include/core_cm4.h **** 
1114:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFCR_EnFCont_Pos                1U                                         /*!< TPI FFC
1115:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FFCR_EnFCont_Msk               (0x1UL << TPI_FFCR_EnFCont_Pos)             /*!< TPI FFC
1116:Drivers/CMSIS/Include/core_cm4.h **** 
1117:Drivers/CMSIS/Include/core_cm4.h **** /* TPI TRIGGER Register Definitions */
1118:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_TRIGGER_TRIGGER_Pos             0U                                         /*!< TPI TRI
1119:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_TRIGGER_TRIGGER_Msk            (0x1UL /*<< TPI_TRIGGER_TRIGGER_Pos*/)      /*!< TPI TRI
1120:Drivers/CMSIS/Include/core_cm4.h **** 
1121:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Integration ETM Data Register Definitions (FIFO0) */
1122:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ITM_ATVALID_Pos          29U                                         /*!< TPI FIF
1123:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ITM_ATVALID_Msk          (0x3UL << TPI_FIFO0_ITM_ATVALID_Pos)        /*!< TPI FIF
1124:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 24


1125:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ITM_bytecount_Pos        27U                                         /*!< TPI FIF
1126:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ITM_bytecount_Msk        (0x3UL << TPI_FIFO0_ITM_bytecount_Pos)      /*!< TPI FIF
1127:Drivers/CMSIS/Include/core_cm4.h **** 
1128:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM_ATVALID_Pos          26U                                         /*!< TPI FIF
1129:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM_ATVALID_Msk          (0x3UL << TPI_FIFO0_ETM_ATVALID_Pos)        /*!< TPI FIF
1130:Drivers/CMSIS/Include/core_cm4.h **** 
1131:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM_bytecount_Pos        24U                                         /*!< TPI FIF
1132:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM_bytecount_Msk        (0x3UL << TPI_FIFO0_ETM_bytecount_Pos)      /*!< TPI FIF
1133:Drivers/CMSIS/Include/core_cm4.h **** 
1134:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM2_Pos                 16U                                         /*!< TPI FIF
1135:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM2_Msk                 (0xFFUL << TPI_FIFO0_ETM2_Pos)              /*!< TPI FIF
1136:Drivers/CMSIS/Include/core_cm4.h **** 
1137:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM1_Pos                  8U                                         /*!< TPI FIF
1138:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM1_Msk                 (0xFFUL << TPI_FIFO0_ETM1_Pos)              /*!< TPI FIF
1139:Drivers/CMSIS/Include/core_cm4.h **** 
1140:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM0_Pos                  0U                                         /*!< TPI FIF
1141:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO0_ETM0_Msk                 (0xFFUL /*<< TPI_FIFO0_ETM0_Pos*/)          /*!< TPI FIF
1142:Drivers/CMSIS/Include/core_cm4.h **** 
1143:Drivers/CMSIS/Include/core_cm4.h **** /* TPI ITATBCTR2 Register Definitions */
1144:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR2_ATREADY2_Pos          0U                                         /*!< TPI ITA
1145:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR2_ATREADY2_Msk         (0x1UL /*<< TPI_ITATBCTR2_ATREADY2_Pos*/)   /*!< TPI ITA
1146:Drivers/CMSIS/Include/core_cm4.h **** 
1147:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR2_ATREADY1_Pos          0U                                         /*!< TPI ITA
1148:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR2_ATREADY1_Msk         (0x1UL /*<< TPI_ITATBCTR2_ATREADY1_Pos*/)   /*!< TPI ITA
1149:Drivers/CMSIS/Include/core_cm4.h **** 
1150:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Integration ITM Data Register Definitions (FIFO1) */
1151:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM_ATVALID_Pos          29U                                         /*!< TPI FIF
1152:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM_ATVALID_Msk          (0x3UL << TPI_FIFO1_ITM_ATVALID_Pos)        /*!< TPI FIF
1153:Drivers/CMSIS/Include/core_cm4.h **** 
1154:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM_bytecount_Pos        27U                                         /*!< TPI FIF
1155:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM_bytecount_Msk        (0x3UL << TPI_FIFO1_ITM_bytecount_Pos)      /*!< TPI FIF
1156:Drivers/CMSIS/Include/core_cm4.h **** 
1157:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ETM_ATVALID_Pos          26U                                         /*!< TPI FIF
1158:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ETM_ATVALID_Msk          (0x3UL << TPI_FIFO1_ETM_ATVALID_Pos)        /*!< TPI FIF
1159:Drivers/CMSIS/Include/core_cm4.h **** 
1160:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ETM_bytecount_Pos        24U                                         /*!< TPI FIF
1161:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ETM_bytecount_Msk        (0x3UL << TPI_FIFO1_ETM_bytecount_Pos)      /*!< TPI FIF
1162:Drivers/CMSIS/Include/core_cm4.h **** 
1163:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM2_Pos                 16U                                         /*!< TPI FIF
1164:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM2_Msk                 (0xFFUL << TPI_FIFO1_ITM2_Pos)              /*!< TPI FIF
1165:Drivers/CMSIS/Include/core_cm4.h **** 
1166:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM1_Pos                  8U                                         /*!< TPI FIF
1167:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM1_Msk                 (0xFFUL << TPI_FIFO1_ITM1_Pos)              /*!< TPI FIF
1168:Drivers/CMSIS/Include/core_cm4.h **** 
1169:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM0_Pos                  0U                                         /*!< TPI FIF
1170:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_FIFO1_ITM0_Msk                 (0xFFUL /*<< TPI_FIFO1_ITM0_Pos*/)          /*!< TPI FIF
1171:Drivers/CMSIS/Include/core_cm4.h **** 
1172:Drivers/CMSIS/Include/core_cm4.h **** /* TPI ITATBCTR0 Register Definitions */
1173:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR0_ATREADY2_Pos          0U                                         /*!< TPI ITA
1174:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR0_ATREADY2_Msk         (0x1UL /*<< TPI_ITATBCTR0_ATREADY2_Pos*/)   /*!< TPI ITA
1175:Drivers/CMSIS/Include/core_cm4.h **** 
1176:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR0_ATREADY1_Pos          0U                                         /*!< TPI ITA
1177:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITATBCTR0_ATREADY1_Msk         (0x1UL /*<< TPI_ITATBCTR0_ATREADY1_Pos*/)   /*!< TPI ITA
1178:Drivers/CMSIS/Include/core_cm4.h **** 
1179:Drivers/CMSIS/Include/core_cm4.h **** /* TPI Integration Mode Control Register Definitions */
1180:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITCTRL_Mode_Pos                 0U                                         /*!< TPI ITC
1181:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_ITCTRL_Mode_Msk                (0x3UL /*<< TPI_ITCTRL_Mode_Pos*/)          /*!< TPI ITC
ARM GAS  /tmp/ccPRqU3T.s 			page 25


1182:Drivers/CMSIS/Include/core_cm4.h **** 
1183:Drivers/CMSIS/Include/core_cm4.h **** /* TPI DEVID Register Definitions */
1184:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_NRZVALID_Pos             11U                                         /*!< TPI DEV
1185:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_NRZVALID_Msk             (0x1UL << TPI_DEVID_NRZVALID_Pos)           /*!< TPI DEV
1186:Drivers/CMSIS/Include/core_cm4.h **** 
1187:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_MANCVALID_Pos            10U                                         /*!< TPI DEV
1188:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_MANCVALID_Msk            (0x1UL << TPI_DEVID_MANCVALID_Pos)          /*!< TPI DEV
1189:Drivers/CMSIS/Include/core_cm4.h **** 
1190:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_PTINVALID_Pos             9U                                         /*!< TPI DEV
1191:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_PTINVALID_Msk            (0x1UL << TPI_DEVID_PTINVALID_Pos)          /*!< TPI DEV
1192:Drivers/CMSIS/Include/core_cm4.h **** 
1193:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_MinBufSz_Pos              6U                                         /*!< TPI DEV
1194:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_MinBufSz_Msk             (0x7UL << TPI_DEVID_MinBufSz_Pos)           /*!< TPI DEV
1195:Drivers/CMSIS/Include/core_cm4.h **** 
1196:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_AsynClkIn_Pos             5U                                         /*!< TPI DEV
1197:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_AsynClkIn_Msk            (0x1UL << TPI_DEVID_AsynClkIn_Pos)          /*!< TPI DEV
1198:Drivers/CMSIS/Include/core_cm4.h **** 
1199:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_NrTraceInput_Pos          0U                                         /*!< TPI DEV
1200:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVID_NrTraceInput_Msk         (0x1FUL /*<< TPI_DEVID_NrTraceInput_Pos*/)  /*!< TPI DEV
1201:Drivers/CMSIS/Include/core_cm4.h **** 
1202:Drivers/CMSIS/Include/core_cm4.h **** /* TPI DEVTYPE Register Definitions */
1203:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVTYPE_SubType_Pos             4U                                         /*!< TPI DEV
1204:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVTYPE_SubType_Msk            (0xFUL /*<< TPI_DEVTYPE_SubType_Pos*/)      /*!< TPI DEV
1205:Drivers/CMSIS/Include/core_cm4.h **** 
1206:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVTYPE_MajorType_Pos           0U                                         /*!< TPI DEV
1207:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_DEVTYPE_MajorType_Msk          (0xFUL << TPI_DEVTYPE_MajorType_Pos)        /*!< TPI DEV
1208:Drivers/CMSIS/Include/core_cm4.h **** 
1209:Drivers/CMSIS/Include/core_cm4.h **** /*@}*/ /* end of group CMSIS_TPI */
1210:Drivers/CMSIS/Include/core_cm4.h **** 
1211:Drivers/CMSIS/Include/core_cm4.h **** 
1212:Drivers/CMSIS/Include/core_cm4.h **** #if defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U)
1213:Drivers/CMSIS/Include/core_cm4.h **** /**
1214:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
1215:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_MPU     Memory Protection Unit (MPU)
1216:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the Memory Protection Unit (MPU)
1217:Drivers/CMSIS/Include/core_cm4.h ****   @{
1218:Drivers/CMSIS/Include/core_cm4.h ****  */
1219:Drivers/CMSIS/Include/core_cm4.h **** 
1220:Drivers/CMSIS/Include/core_cm4.h **** /**
1221:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Memory Protection Unit (MPU).
1222:Drivers/CMSIS/Include/core_cm4.h ****  */
1223:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
1224:Drivers/CMSIS/Include/core_cm4.h **** {
1225:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t TYPE;                   /*!< Offset: 0x000 (R/ )  MPU Type Register */
1226:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t CTRL;                   /*!< Offset: 0x004 (R/W)  MPU Control Register */
1227:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RNR;                    /*!< Offset: 0x008 (R/W)  MPU Region RNRber Register */
1228:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RBAR;                   /*!< Offset: 0x00C (R/W)  MPU Region Base Address Register
1229:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RASR;                   /*!< Offset: 0x010 (R/W)  MPU Region Attribute and Size Re
1230:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RBAR_A1;                /*!< Offset: 0x014 (R/W)  MPU Alias 1 Region Base Address 
1231:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RASR_A1;                /*!< Offset: 0x018 (R/W)  MPU Alias 1 Region Attribute and
1232:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RBAR_A2;                /*!< Offset: 0x01C (R/W)  MPU Alias 2 Region Base Address 
1233:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RASR_A2;                /*!< Offset: 0x020 (R/W)  MPU Alias 2 Region Attribute and
1234:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RBAR_A3;                /*!< Offset: 0x024 (R/W)  MPU Alias 3 Region Base Address 
1235:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t RASR_A3;                /*!< Offset: 0x028 (R/W)  MPU Alias 3 Region Attribute and
1236:Drivers/CMSIS/Include/core_cm4.h **** } MPU_Type;
1237:Drivers/CMSIS/Include/core_cm4.h **** 
1238:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_RALIASES                  4U
ARM GAS  /tmp/ccPRqU3T.s 			page 26


1239:Drivers/CMSIS/Include/core_cm4.h **** 
1240:Drivers/CMSIS/Include/core_cm4.h **** /* MPU Type Register Definitions */
1241:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_IREGION_Pos               16U                                            /*!< MPU 
1242:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_IREGION_Msk               (0xFFUL << MPU_TYPE_IREGION_Pos)               /*!< MPU 
1243:Drivers/CMSIS/Include/core_cm4.h **** 
1244:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_DREGION_Pos                8U                                            /*!< MPU 
1245:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_DREGION_Msk               (0xFFUL << MPU_TYPE_DREGION_Pos)               /*!< MPU 
1246:Drivers/CMSIS/Include/core_cm4.h **** 
1247:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_SEPARATE_Pos               0U                                            /*!< MPU 
1248:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_TYPE_SEPARATE_Msk              (1UL /*<< MPU_TYPE_SEPARATE_Pos*/)             /*!< MPU 
1249:Drivers/CMSIS/Include/core_cm4.h **** 
1250:Drivers/CMSIS/Include/core_cm4.h **** /* MPU Control Register Definitions */
1251:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_CTRL_PRIVDEFENA_Pos             2U                                            /*!< MPU 
1252:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_CTRL_PRIVDEFENA_Msk            (1UL << MPU_CTRL_PRIVDEFENA_Pos)               /*!< MPU 
1253:Drivers/CMSIS/Include/core_cm4.h **** 
1254:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_CTRL_HFNMIENA_Pos               1U                                            /*!< MPU 
1255:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_CTRL_HFNMIENA_Msk              (1UL << MPU_CTRL_HFNMIENA_Pos)                 /*!< MPU 
1256:Drivers/CMSIS/Include/core_cm4.h **** 
1257:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_CTRL_ENABLE_Pos                 0U                                            /*!< MPU 
1258:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_CTRL_ENABLE_Msk                (1UL /*<< MPU_CTRL_ENABLE_Pos*/)               /*!< MPU 
1259:Drivers/CMSIS/Include/core_cm4.h **** 
1260:Drivers/CMSIS/Include/core_cm4.h **** /* MPU Region Number Register Definitions */
1261:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RNR_REGION_Pos                  0U                                            /*!< MPU 
1262:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RNR_REGION_Msk                 (0xFFUL /*<< MPU_RNR_REGION_Pos*/)             /*!< MPU 
1263:Drivers/CMSIS/Include/core_cm4.h **** 
1264:Drivers/CMSIS/Include/core_cm4.h **** /* MPU Region Base Address Register Definitions */
1265:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RBAR_ADDR_Pos                   5U                                            /*!< MPU 
1266:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RBAR_ADDR_Msk                  (0x7FFFFFFUL << MPU_RBAR_ADDR_Pos)             /*!< MPU 
1267:Drivers/CMSIS/Include/core_cm4.h **** 
1268:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RBAR_VALID_Pos                  4U                                            /*!< MPU 
1269:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RBAR_VALID_Msk                 (1UL << MPU_RBAR_VALID_Pos)                    /*!< MPU 
1270:Drivers/CMSIS/Include/core_cm4.h **** 
1271:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RBAR_REGION_Pos                 0U                                            /*!< MPU 
1272:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RBAR_REGION_Msk                (0xFUL /*<< MPU_RBAR_REGION_Pos*/)             /*!< MPU 
1273:Drivers/CMSIS/Include/core_cm4.h **** 
1274:Drivers/CMSIS/Include/core_cm4.h **** /* MPU Region Attribute and Size Register Definitions */
1275:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_ATTRS_Pos                 16U                                            /*!< MPU 
1276:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_ATTRS_Msk                 (0xFFFFUL << MPU_RASR_ATTRS_Pos)               /*!< MPU 
1277:Drivers/CMSIS/Include/core_cm4.h **** 
1278:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_XN_Pos                    28U                                            /*!< MPU 
1279:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_XN_Msk                    (1UL << MPU_RASR_XN_Pos)                       /*!< MPU 
1280:Drivers/CMSIS/Include/core_cm4.h **** 
1281:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_AP_Pos                    24U                                            /*!< MPU 
1282:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_AP_Msk                    (0x7UL << MPU_RASR_AP_Pos)                     /*!< MPU 
1283:Drivers/CMSIS/Include/core_cm4.h **** 
1284:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_TEX_Pos                   19U                                            /*!< MPU 
1285:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_TEX_Msk                   (0x7UL << MPU_RASR_TEX_Pos)                    /*!< MPU 
1286:Drivers/CMSIS/Include/core_cm4.h **** 
1287:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_S_Pos                     18U                                            /*!< MPU 
1288:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_S_Msk                     (1UL << MPU_RASR_S_Pos)                        /*!< MPU 
1289:Drivers/CMSIS/Include/core_cm4.h **** 
1290:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_C_Pos                     17U                                            /*!< MPU 
1291:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_C_Msk                     (1UL << MPU_RASR_C_Pos)                        /*!< MPU 
1292:Drivers/CMSIS/Include/core_cm4.h **** 
1293:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_B_Pos                     16U                                            /*!< MPU 
1294:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_B_Msk                     (1UL << MPU_RASR_B_Pos)                        /*!< MPU 
1295:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 27


1296:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_SRD_Pos                    8U                                            /*!< MPU 
1297:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_SRD_Msk                   (0xFFUL << MPU_RASR_SRD_Pos)                   /*!< MPU 
1298:Drivers/CMSIS/Include/core_cm4.h **** 
1299:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_SIZE_Pos                   1U                                            /*!< MPU 
1300:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_SIZE_Msk                  (0x1FUL << MPU_RASR_SIZE_Pos)                  /*!< MPU 
1301:Drivers/CMSIS/Include/core_cm4.h **** 
1302:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_ENABLE_Pos                 0U                                            /*!< MPU 
1303:Drivers/CMSIS/Include/core_cm4.h **** #define MPU_RASR_ENABLE_Msk                (1UL /*<< MPU_RASR_ENABLE_Pos*/)               /*!< MPU 
1304:Drivers/CMSIS/Include/core_cm4.h **** 
1305:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_MPU */
1306:Drivers/CMSIS/Include/core_cm4.h **** #endif /* defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U) */
1307:Drivers/CMSIS/Include/core_cm4.h **** 
1308:Drivers/CMSIS/Include/core_cm4.h **** 
1309:Drivers/CMSIS/Include/core_cm4.h **** /**
1310:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
1311:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_FPU     Floating Point Unit (FPU)
1312:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the Floating Point Unit (FPU)
1313:Drivers/CMSIS/Include/core_cm4.h ****   @{
1314:Drivers/CMSIS/Include/core_cm4.h ****  */
1315:Drivers/CMSIS/Include/core_cm4.h **** 
1316:Drivers/CMSIS/Include/core_cm4.h **** /**
1317:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Floating Point Unit (FPU).
1318:Drivers/CMSIS/Include/core_cm4.h ****  */
1319:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
1320:Drivers/CMSIS/Include/core_cm4.h **** {
1321:Drivers/CMSIS/Include/core_cm4.h ****         uint32_t RESERVED0[1U];
1322:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FPCCR;                  /*!< Offset: 0x004 (R/W)  Floating-Point Context Control R
1323:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FPCAR;                  /*!< Offset: 0x008 (R/W)  Floating-Point Context Address R
1324:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t FPDSCR;                 /*!< Offset: 0x00C (R/W)  Floating-Point Default Status Co
1325:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t MVFR0;                  /*!< Offset: 0x010 (R/ )  Media and FP Feature Register 0 
1326:Drivers/CMSIS/Include/core_cm4.h ****   __IM  uint32_t MVFR1;                  /*!< Offset: 0x014 (R/ )  Media and FP Feature Register 1 
1327:Drivers/CMSIS/Include/core_cm4.h **** } FPU_Type;
1328:Drivers/CMSIS/Include/core_cm4.h **** 
1329:Drivers/CMSIS/Include/core_cm4.h **** /* Floating-Point Context Control Register Definitions */
1330:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_ASPEN_Pos                31U                                            /*!< FPCC
1331:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_ASPEN_Msk                (1UL << FPU_FPCCR_ASPEN_Pos)                   /*!< FPCC
1332:Drivers/CMSIS/Include/core_cm4.h **** 
1333:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_LSPEN_Pos                30U                                            /*!< FPCC
1334:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_LSPEN_Msk                (1UL << FPU_FPCCR_LSPEN_Pos)                   /*!< FPCC
1335:Drivers/CMSIS/Include/core_cm4.h **** 
1336:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_MONRDY_Pos                8U                                            /*!< FPCC
1337:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_MONRDY_Msk               (1UL << FPU_FPCCR_MONRDY_Pos)                  /*!< FPCC
1338:Drivers/CMSIS/Include/core_cm4.h **** 
1339:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_BFRDY_Pos                 6U                                            /*!< FPCC
1340:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_BFRDY_Msk                (1UL << FPU_FPCCR_BFRDY_Pos)                   /*!< FPCC
1341:Drivers/CMSIS/Include/core_cm4.h **** 
1342:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_MMRDY_Pos                 5U                                            /*!< FPCC
1343:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_MMRDY_Msk                (1UL << FPU_FPCCR_MMRDY_Pos)                   /*!< FPCC
1344:Drivers/CMSIS/Include/core_cm4.h **** 
1345:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_HFRDY_Pos                 4U                                            /*!< FPCC
1346:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_HFRDY_Msk                (1UL << FPU_FPCCR_HFRDY_Pos)                   /*!< FPCC
1347:Drivers/CMSIS/Include/core_cm4.h **** 
1348:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_THREAD_Pos                3U                                            /*!< FPCC
1349:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_THREAD_Msk               (1UL << FPU_FPCCR_THREAD_Pos)                  /*!< FPCC
1350:Drivers/CMSIS/Include/core_cm4.h **** 
1351:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_USER_Pos                  1U                                            /*!< FPCC
1352:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_USER_Msk                 (1UL << FPU_FPCCR_USER_Pos)                    /*!< FPCC
ARM GAS  /tmp/ccPRqU3T.s 			page 28


1353:Drivers/CMSIS/Include/core_cm4.h **** 
1354:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_LSPACT_Pos                0U                                            /*!< FPCC
1355:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCCR_LSPACT_Msk               (1UL /*<< FPU_FPCCR_LSPACT_Pos*/)              /*!< FPCC
1356:Drivers/CMSIS/Include/core_cm4.h **** 
1357:Drivers/CMSIS/Include/core_cm4.h **** /* Floating-Point Context Address Register Definitions */
1358:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCAR_ADDRESS_Pos               3U                                            /*!< FPCA
1359:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPCAR_ADDRESS_Msk              (0x1FFFFFFFUL << FPU_FPCAR_ADDRESS_Pos)        /*!< FPCA
1360:Drivers/CMSIS/Include/core_cm4.h **** 
1361:Drivers/CMSIS/Include/core_cm4.h **** /* Floating-Point Default Status Control Register Definitions */
1362:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_AHP_Pos                 26U                                            /*!< FPDS
1363:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_AHP_Msk                 (1UL << FPU_FPDSCR_AHP_Pos)                    /*!< FPDS
1364:Drivers/CMSIS/Include/core_cm4.h **** 
1365:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_DN_Pos                  25U                                            /*!< FPDS
1366:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_DN_Msk                  (1UL << FPU_FPDSCR_DN_Pos)                     /*!< FPDS
1367:Drivers/CMSIS/Include/core_cm4.h **** 
1368:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_FZ_Pos                  24U                                            /*!< FPDS
1369:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_FZ_Msk                  (1UL << FPU_FPDSCR_FZ_Pos)                     /*!< FPDS
1370:Drivers/CMSIS/Include/core_cm4.h **** 
1371:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_RMode_Pos               22U                                            /*!< FPDS
1372:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_FPDSCR_RMode_Msk               (3UL << FPU_FPDSCR_RMode_Pos)                  /*!< FPDS
1373:Drivers/CMSIS/Include/core_cm4.h **** 
1374:Drivers/CMSIS/Include/core_cm4.h **** /* Media and FP Feature Register 0 Definitions */
1375:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_FP_rounding_modes_Pos    28U                                            /*!< MVFR
1376:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_FP_rounding_modes_Msk    (0xFUL << FPU_MVFR0_FP_rounding_modes_Pos)     /*!< MVFR
1377:Drivers/CMSIS/Include/core_cm4.h **** 
1378:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Short_vectors_Pos        24U                                            /*!< MVFR
1379:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Short_vectors_Msk        (0xFUL << FPU_MVFR0_Short_vectors_Pos)         /*!< MVFR
1380:Drivers/CMSIS/Include/core_cm4.h **** 
1381:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Square_root_Pos          20U                                            /*!< MVFR
1382:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Square_root_Msk          (0xFUL << FPU_MVFR0_Square_root_Pos)           /*!< MVFR
1383:Drivers/CMSIS/Include/core_cm4.h **** 
1384:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Divide_Pos               16U                                            /*!< MVFR
1385:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Divide_Msk               (0xFUL << FPU_MVFR0_Divide_Pos)                /*!< MVFR
1386:Drivers/CMSIS/Include/core_cm4.h **** 
1387:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_FP_excep_trapping_Pos    12U                                            /*!< MVFR
1388:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_FP_excep_trapping_Msk    (0xFUL << FPU_MVFR0_FP_excep_trapping_Pos)     /*!< MVFR
1389:Drivers/CMSIS/Include/core_cm4.h **** 
1390:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Double_precision_Pos      8U                                            /*!< MVFR
1391:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Double_precision_Msk     (0xFUL << FPU_MVFR0_Double_precision_Pos)      /*!< MVFR
1392:Drivers/CMSIS/Include/core_cm4.h **** 
1393:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Single_precision_Pos      4U                                            /*!< MVFR
1394:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_Single_precision_Msk     (0xFUL << FPU_MVFR0_Single_precision_Pos)      /*!< MVFR
1395:Drivers/CMSIS/Include/core_cm4.h **** 
1396:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_A_SIMD_registers_Pos      0U                                            /*!< MVFR
1397:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR0_A_SIMD_registers_Msk     (0xFUL /*<< FPU_MVFR0_A_SIMD_registers_Pos*/)  /*!< MVFR
1398:Drivers/CMSIS/Include/core_cm4.h **** 
1399:Drivers/CMSIS/Include/core_cm4.h **** /* Media and FP Feature Register 1 Definitions */
1400:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_FP_fused_MAC_Pos         28U                                            /*!< MVFR
1401:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_FP_fused_MAC_Msk         (0xFUL << FPU_MVFR1_FP_fused_MAC_Pos)          /*!< MVFR
1402:Drivers/CMSIS/Include/core_cm4.h **** 
1403:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_FP_HPFP_Pos              24U                                            /*!< MVFR
1404:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_FP_HPFP_Msk              (0xFUL << FPU_MVFR1_FP_HPFP_Pos)               /*!< MVFR
1405:Drivers/CMSIS/Include/core_cm4.h **** 
1406:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_D_NaN_mode_Pos            4U                                            /*!< MVFR
1407:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_D_NaN_mode_Msk           (0xFUL << FPU_MVFR1_D_NaN_mode_Pos)            /*!< MVFR
1408:Drivers/CMSIS/Include/core_cm4.h **** 
1409:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_FtZ_mode_Pos              0U                                            /*!< MVFR
ARM GAS  /tmp/ccPRqU3T.s 			page 29


1410:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_MVFR1_FtZ_mode_Msk             (0xFUL /*<< FPU_MVFR1_FtZ_mode_Pos*/)          /*!< MVFR
1411:Drivers/CMSIS/Include/core_cm4.h **** 
1412:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_FPU */
1413:Drivers/CMSIS/Include/core_cm4.h **** 
1414:Drivers/CMSIS/Include/core_cm4.h **** 
1415:Drivers/CMSIS/Include/core_cm4.h **** /**
1416:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_core_register
1417:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_CoreDebug       Core Debug Registers (CoreDebug)
1418:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Type definitions for the Core Debug Registers
1419:Drivers/CMSIS/Include/core_cm4.h ****   @{
1420:Drivers/CMSIS/Include/core_cm4.h ****  */
1421:Drivers/CMSIS/Include/core_cm4.h **** 
1422:Drivers/CMSIS/Include/core_cm4.h **** /**
1423:Drivers/CMSIS/Include/core_cm4.h ****   \brief  Structure type to access the Core Debug Register (CoreDebug).
1424:Drivers/CMSIS/Include/core_cm4.h ****  */
1425:Drivers/CMSIS/Include/core_cm4.h **** typedef struct
1426:Drivers/CMSIS/Include/core_cm4.h **** {
1427:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t DHCSR;                  /*!< Offset: 0x000 (R/W)  Debug Halting Control and Status
1428:Drivers/CMSIS/Include/core_cm4.h ****   __OM  uint32_t DCRSR;                  /*!< Offset: 0x004 ( /W)  Debug Core Register Selector Reg
1429:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t DCRDR;                  /*!< Offset: 0x008 (R/W)  Debug Core Register Data Registe
1430:Drivers/CMSIS/Include/core_cm4.h ****   __IOM uint32_t DEMCR;                  /*!< Offset: 0x00C (R/W)  Debug Exception and Monitor Cont
1431:Drivers/CMSIS/Include/core_cm4.h **** } CoreDebug_Type;
1432:Drivers/CMSIS/Include/core_cm4.h **** 
1433:Drivers/CMSIS/Include/core_cm4.h **** /* Debug Halting Control and Status Register Definitions */
1434:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_DBGKEY_Pos         16U                                            /*!< Core
1435:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_DBGKEY_Msk         (0xFFFFUL << CoreDebug_DHCSR_DBGKEY_Pos)       /*!< Core
1436:Drivers/CMSIS/Include/core_cm4.h **** 
1437:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_RESET_ST_Pos     25U                                            /*!< Core
1438:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_RESET_ST_Msk     (1UL << CoreDebug_DHCSR_S_RESET_ST_Pos)        /*!< Core
1439:Drivers/CMSIS/Include/core_cm4.h **** 
1440:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_RETIRE_ST_Pos    24U                                            /*!< Core
1441:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_RETIRE_ST_Msk    (1UL << CoreDebug_DHCSR_S_RETIRE_ST_Pos)       /*!< Core
1442:Drivers/CMSIS/Include/core_cm4.h **** 
1443:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_LOCKUP_Pos       19U                                            /*!< Core
1444:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_LOCKUP_Msk       (1UL << CoreDebug_DHCSR_S_LOCKUP_Pos)          /*!< Core
1445:Drivers/CMSIS/Include/core_cm4.h **** 
1446:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_SLEEP_Pos        18U                                            /*!< Core
1447:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_SLEEP_Msk        (1UL << CoreDebug_DHCSR_S_SLEEP_Pos)           /*!< Core
1448:Drivers/CMSIS/Include/core_cm4.h **** 
1449:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_HALT_Pos         17U                                            /*!< Core
1450:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_HALT_Msk         (1UL << CoreDebug_DHCSR_S_HALT_Pos)            /*!< Core
1451:Drivers/CMSIS/Include/core_cm4.h **** 
1452:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_REGRDY_Pos       16U                                            /*!< Core
1453:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_S_REGRDY_Msk       (1UL << CoreDebug_DHCSR_S_REGRDY_Pos)          /*!< Core
1454:Drivers/CMSIS/Include/core_cm4.h **** 
1455:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_SNAPSTALL_Pos     5U                                            /*!< Core
1456:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_SNAPSTALL_Msk    (1UL << CoreDebug_DHCSR_C_SNAPSTALL_Pos)       /*!< Core
1457:Drivers/CMSIS/Include/core_cm4.h **** 
1458:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_MASKINTS_Pos      3U                                            /*!< Core
1459:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_MASKINTS_Msk     (1UL << CoreDebug_DHCSR_C_MASKINTS_Pos)        /*!< Core
1460:Drivers/CMSIS/Include/core_cm4.h **** 
1461:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_STEP_Pos          2U                                            /*!< Core
1462:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_STEP_Msk         (1UL << CoreDebug_DHCSR_C_STEP_Pos)            /*!< Core
1463:Drivers/CMSIS/Include/core_cm4.h **** 
1464:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_HALT_Pos          1U                                            /*!< Core
1465:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_HALT_Msk         (1UL << CoreDebug_DHCSR_C_HALT_Pos)            /*!< Core
1466:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 30


1467:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_DEBUGEN_Pos       0U                                            /*!< Core
1468:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DHCSR_C_DEBUGEN_Msk      (1UL /*<< CoreDebug_DHCSR_C_DEBUGEN_Pos*/)     /*!< Core
1469:Drivers/CMSIS/Include/core_cm4.h **** 
1470:Drivers/CMSIS/Include/core_cm4.h **** /* Debug Core Register Selector Register Definitions */
1471:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DCRSR_REGWnR_Pos         16U                                            /*!< Core
1472:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DCRSR_REGWnR_Msk         (1UL << CoreDebug_DCRSR_REGWnR_Pos)            /*!< Core
1473:Drivers/CMSIS/Include/core_cm4.h **** 
1474:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DCRSR_REGSEL_Pos          0U                                            /*!< Core
1475:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DCRSR_REGSEL_Msk         (0x1FUL /*<< CoreDebug_DCRSR_REGSEL_Pos*/)     /*!< Core
1476:Drivers/CMSIS/Include/core_cm4.h **** 
1477:Drivers/CMSIS/Include/core_cm4.h **** /* Debug Exception and Monitor Control Register Definitions */
1478:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_TRCENA_Pos         24U                                            /*!< Core
1479:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_TRCENA_Msk         (1UL << CoreDebug_DEMCR_TRCENA_Pos)            /*!< Core
1480:Drivers/CMSIS/Include/core_cm4.h **** 
1481:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_REQ_Pos        19U                                            /*!< Core
1482:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_REQ_Msk        (1UL << CoreDebug_DEMCR_MON_REQ_Pos)           /*!< Core
1483:Drivers/CMSIS/Include/core_cm4.h **** 
1484:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_STEP_Pos       18U                                            /*!< Core
1485:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_STEP_Msk       (1UL << CoreDebug_DEMCR_MON_STEP_Pos)          /*!< Core
1486:Drivers/CMSIS/Include/core_cm4.h **** 
1487:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_PEND_Pos       17U                                            /*!< Core
1488:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_PEND_Msk       (1UL << CoreDebug_DEMCR_MON_PEND_Pos)          /*!< Core
1489:Drivers/CMSIS/Include/core_cm4.h **** 
1490:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_EN_Pos         16U                                            /*!< Core
1491:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_MON_EN_Msk         (1UL << CoreDebug_DEMCR_MON_EN_Pos)            /*!< Core
1492:Drivers/CMSIS/Include/core_cm4.h **** 
1493:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_HARDERR_Pos     10U                                            /*!< Core
1494:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_HARDERR_Msk     (1UL << CoreDebug_DEMCR_VC_HARDERR_Pos)        /*!< Core
1495:Drivers/CMSIS/Include/core_cm4.h **** 
1496:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_INTERR_Pos       9U                                            /*!< Core
1497:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_INTERR_Msk      (1UL << CoreDebug_DEMCR_VC_INTERR_Pos)         /*!< Core
1498:Drivers/CMSIS/Include/core_cm4.h **** 
1499:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_BUSERR_Pos       8U                                            /*!< Core
1500:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_BUSERR_Msk      (1UL << CoreDebug_DEMCR_VC_BUSERR_Pos)         /*!< Core
1501:Drivers/CMSIS/Include/core_cm4.h **** 
1502:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_STATERR_Pos      7U                                            /*!< Core
1503:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_STATERR_Msk     (1UL << CoreDebug_DEMCR_VC_STATERR_Pos)        /*!< Core
1504:Drivers/CMSIS/Include/core_cm4.h **** 
1505:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_CHKERR_Pos       6U                                            /*!< Core
1506:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_CHKERR_Msk      (1UL << CoreDebug_DEMCR_VC_CHKERR_Pos)         /*!< Core
1507:Drivers/CMSIS/Include/core_cm4.h **** 
1508:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_NOCPERR_Pos      5U                                            /*!< Core
1509:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_NOCPERR_Msk     (1UL << CoreDebug_DEMCR_VC_NOCPERR_Pos)        /*!< Core
1510:Drivers/CMSIS/Include/core_cm4.h **** 
1511:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_MMERR_Pos        4U                                            /*!< Core
1512:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_MMERR_Msk       (1UL << CoreDebug_DEMCR_VC_MMERR_Pos)          /*!< Core
1513:Drivers/CMSIS/Include/core_cm4.h **** 
1514:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_CORERESET_Pos    0U                                            /*!< Core
1515:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_DEMCR_VC_CORERESET_Msk   (1UL /*<< CoreDebug_DEMCR_VC_CORERESET_Pos*/)  /*!< Core
1516:Drivers/CMSIS/Include/core_cm4.h **** 
1517:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_CoreDebug */
1518:Drivers/CMSIS/Include/core_cm4.h **** 
1519:Drivers/CMSIS/Include/core_cm4.h **** 
1520:Drivers/CMSIS/Include/core_cm4.h **** /**
1521:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup    CMSIS_core_register
1522:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup   CMSIS_core_bitfield     Core register bit field macros
1523:Drivers/CMSIS/Include/core_cm4.h ****   \brief      Macros for use with bit field definitions (xxx_Pos, xxx_Msk).
ARM GAS  /tmp/ccPRqU3T.s 			page 31


1524:Drivers/CMSIS/Include/core_cm4.h ****   @{
1525:Drivers/CMSIS/Include/core_cm4.h ****  */
1526:Drivers/CMSIS/Include/core_cm4.h **** 
1527:Drivers/CMSIS/Include/core_cm4.h **** /**
1528:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Mask and shift a bit field value for use in a register bit range.
1529:Drivers/CMSIS/Include/core_cm4.h ****   \param[in] field  Name of the register bit field.
1530:Drivers/CMSIS/Include/core_cm4.h ****   \param[in] value  Value of the bit field. This parameter is interpreted as an uint32_t type.
1531:Drivers/CMSIS/Include/core_cm4.h ****   \return           Masked and shifted value.
1532:Drivers/CMSIS/Include/core_cm4.h **** */
1533:Drivers/CMSIS/Include/core_cm4.h **** #define _VAL2FLD(field, value)    (((uint32_t)(value) << field ## _Pos) & field ## _Msk)
1534:Drivers/CMSIS/Include/core_cm4.h **** 
1535:Drivers/CMSIS/Include/core_cm4.h **** /**
1536:Drivers/CMSIS/Include/core_cm4.h ****   \brief     Mask and shift a register value to extract a bit filed value.
1537:Drivers/CMSIS/Include/core_cm4.h ****   \param[in] field  Name of the register bit field.
1538:Drivers/CMSIS/Include/core_cm4.h ****   \param[in] value  Value of register. This parameter is interpreted as an uint32_t type.
1539:Drivers/CMSIS/Include/core_cm4.h ****   \return           Masked and shifted bit field value.
1540:Drivers/CMSIS/Include/core_cm4.h **** */
1541:Drivers/CMSIS/Include/core_cm4.h **** #define _FLD2VAL(field, value)    (((uint32_t)(value) & field ## _Msk) >> field ## _Pos)
1542:Drivers/CMSIS/Include/core_cm4.h **** 
1543:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of group CMSIS_core_bitfield */
1544:Drivers/CMSIS/Include/core_cm4.h **** 
1545:Drivers/CMSIS/Include/core_cm4.h **** 
1546:Drivers/CMSIS/Include/core_cm4.h **** /**
1547:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup    CMSIS_core_register
1548:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup   CMSIS_core_base     Core Definitions
1549:Drivers/CMSIS/Include/core_cm4.h ****   \brief      Definitions for base addresses, unions, and structures.
1550:Drivers/CMSIS/Include/core_cm4.h ****   @{
1551:Drivers/CMSIS/Include/core_cm4.h ****  */
1552:Drivers/CMSIS/Include/core_cm4.h **** 
1553:Drivers/CMSIS/Include/core_cm4.h **** /* Memory mapping of Core Hardware */
1554:Drivers/CMSIS/Include/core_cm4.h **** #define SCS_BASE            (0xE000E000UL)                            /*!< System Control Space Bas
1555:Drivers/CMSIS/Include/core_cm4.h **** #define ITM_BASE            (0xE0000000UL)                            /*!< ITM Base Address */
1556:Drivers/CMSIS/Include/core_cm4.h **** #define DWT_BASE            (0xE0001000UL)                            /*!< DWT Base Address */
1557:Drivers/CMSIS/Include/core_cm4.h **** #define TPI_BASE            (0xE0040000UL)                            /*!< TPI Base Address */
1558:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug_BASE      (0xE000EDF0UL)                            /*!< Core Debug Base Address 
1559:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick_BASE        (SCS_BASE +  0x0010UL)                    /*!< SysTick Base Address */
1560:Drivers/CMSIS/Include/core_cm4.h **** #define NVIC_BASE           (SCS_BASE +  0x0100UL)                    /*!< NVIC Base Address */
1561:Drivers/CMSIS/Include/core_cm4.h **** #define SCB_BASE            (SCS_BASE +  0x0D00UL)                    /*!< System Control Block Bas
1562:Drivers/CMSIS/Include/core_cm4.h **** 
1563:Drivers/CMSIS/Include/core_cm4.h **** #define SCnSCB              ((SCnSCB_Type    *)     SCS_BASE      )   /*!< System control Register 
1564:Drivers/CMSIS/Include/core_cm4.h **** #define SCB                 ((SCB_Type       *)     SCB_BASE      )   /*!< SCB configuration struct
1565:Drivers/CMSIS/Include/core_cm4.h **** #define SysTick             ((SysTick_Type   *)     SysTick_BASE  )   /*!< SysTick configuration st
1566:Drivers/CMSIS/Include/core_cm4.h **** #define NVIC                ((NVIC_Type      *)     NVIC_BASE     )   /*!< NVIC configuration struc
1567:Drivers/CMSIS/Include/core_cm4.h **** #define ITM                 ((ITM_Type       *)     ITM_BASE      )   /*!< ITM configuration struct
1568:Drivers/CMSIS/Include/core_cm4.h **** #define DWT                 ((DWT_Type       *)     DWT_BASE      )   /*!< DWT configuration struct
1569:Drivers/CMSIS/Include/core_cm4.h **** #define TPI                 ((TPI_Type       *)     TPI_BASE      )   /*!< TPI configuration struct
1570:Drivers/CMSIS/Include/core_cm4.h **** #define CoreDebug           ((CoreDebug_Type *)     CoreDebug_BASE)   /*!< Core Debug configuration
1571:Drivers/CMSIS/Include/core_cm4.h **** 
1572:Drivers/CMSIS/Include/core_cm4.h **** #if defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U)
1573:Drivers/CMSIS/Include/core_cm4.h ****   #define MPU_BASE          (SCS_BASE +  0x0D90UL)                    /*!< Memory Protection Unit *
1574:Drivers/CMSIS/Include/core_cm4.h ****   #define MPU               ((MPU_Type       *)     MPU_BASE      )   /*!< Memory Protection Unit *
1575:Drivers/CMSIS/Include/core_cm4.h **** #endif
1576:Drivers/CMSIS/Include/core_cm4.h **** 
1577:Drivers/CMSIS/Include/core_cm4.h **** #define FPU_BASE            (SCS_BASE +  0x0F30UL)                    /*!< Floating Point Unit */
1578:Drivers/CMSIS/Include/core_cm4.h **** #define FPU                 ((FPU_Type       *)     FPU_BASE      )   /*!< Floating Point Unit */
1579:Drivers/CMSIS/Include/core_cm4.h **** 
1580:Drivers/CMSIS/Include/core_cm4.h **** /*@} */
ARM GAS  /tmp/ccPRqU3T.s 			page 32


1581:Drivers/CMSIS/Include/core_cm4.h **** 
1582:Drivers/CMSIS/Include/core_cm4.h **** 
1583:Drivers/CMSIS/Include/core_cm4.h **** 
1584:Drivers/CMSIS/Include/core_cm4.h **** /*******************************************************************************
1585:Drivers/CMSIS/Include/core_cm4.h ****  *                Hardware Abstraction Layer
1586:Drivers/CMSIS/Include/core_cm4.h ****   Core Function Interface contains:
1587:Drivers/CMSIS/Include/core_cm4.h ****   - Core NVIC Functions
1588:Drivers/CMSIS/Include/core_cm4.h ****   - Core SysTick Functions
1589:Drivers/CMSIS/Include/core_cm4.h ****   - Core Debug Functions
1590:Drivers/CMSIS/Include/core_cm4.h ****   - Core Register Access Functions
1591:Drivers/CMSIS/Include/core_cm4.h ****  ******************************************************************************/
1592:Drivers/CMSIS/Include/core_cm4.h **** /**
1593:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_Core_FunctionInterface Functions and Instructions Reference
1594:Drivers/CMSIS/Include/core_cm4.h **** */
1595:Drivers/CMSIS/Include/core_cm4.h **** 
1596:Drivers/CMSIS/Include/core_cm4.h **** 
1597:Drivers/CMSIS/Include/core_cm4.h **** 
1598:Drivers/CMSIS/Include/core_cm4.h **** /* ##########################   NVIC functions  #################################### */
1599:Drivers/CMSIS/Include/core_cm4.h **** /**
1600:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_Core_FunctionInterface
1601:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_Core_NVICFunctions NVIC Functions
1602:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Functions that manage interrupts and exceptions via the NVIC.
1603:Drivers/CMSIS/Include/core_cm4.h ****   @{
1604:Drivers/CMSIS/Include/core_cm4.h ****  */
1605:Drivers/CMSIS/Include/core_cm4.h **** 
1606:Drivers/CMSIS/Include/core_cm4.h **** #ifdef CMSIS_NVIC_VIRTUAL
1607:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef CMSIS_NVIC_VIRTUAL_HEADER_FILE
1608:Drivers/CMSIS/Include/core_cm4.h ****     #define CMSIS_NVIC_VIRTUAL_HEADER_FILE "cmsis_nvic_virtual.h"
1609:Drivers/CMSIS/Include/core_cm4.h ****   #endif
1610:Drivers/CMSIS/Include/core_cm4.h ****   #include CMSIS_NVIC_VIRTUAL_HEADER_FILE
1611:Drivers/CMSIS/Include/core_cm4.h **** #else
1612:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_SetPriorityGrouping    __NVIC_SetPriorityGrouping
1613:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_GetPriorityGrouping    __NVIC_GetPriorityGrouping
1614:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_EnableIRQ              __NVIC_EnableIRQ
1615:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_GetEnableIRQ           __NVIC_GetEnableIRQ
1616:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_DisableIRQ             __NVIC_DisableIRQ
1617:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_GetPendingIRQ          __NVIC_GetPendingIRQ
1618:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_SetPendingIRQ          __NVIC_SetPendingIRQ
1619:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_ClearPendingIRQ        __NVIC_ClearPendingIRQ
1620:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_GetActive              __NVIC_GetActive
1621:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_SetPriority            __NVIC_SetPriority
1622:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_GetPriority            __NVIC_GetPriority
1623:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_SystemReset            __NVIC_SystemReset
1624:Drivers/CMSIS/Include/core_cm4.h **** #endif /* CMSIS_NVIC_VIRTUAL */
1625:Drivers/CMSIS/Include/core_cm4.h **** 
1626:Drivers/CMSIS/Include/core_cm4.h **** #ifdef CMSIS_VECTAB_VIRTUAL
1627:Drivers/CMSIS/Include/core_cm4.h ****   #ifndef CMSIS_VECTAB_VIRTUAL_HEADER_FILE
1628:Drivers/CMSIS/Include/core_cm4.h ****    #define CMSIS_VECTAB_VIRTUAL_HEADER_FILE "cmsis_vectab_virtual.h"
1629:Drivers/CMSIS/Include/core_cm4.h ****   #endif
1630:Drivers/CMSIS/Include/core_cm4.h ****   #include CMSIS_VECTAB_VIRTUAL_HEADER_FILE
1631:Drivers/CMSIS/Include/core_cm4.h **** #else
1632:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_SetVector              __NVIC_SetVector
1633:Drivers/CMSIS/Include/core_cm4.h ****   #define NVIC_GetVector              __NVIC_GetVector
1634:Drivers/CMSIS/Include/core_cm4.h **** #endif  /* (CMSIS_VECTAB_VIRTUAL) */
1635:Drivers/CMSIS/Include/core_cm4.h **** 
1636:Drivers/CMSIS/Include/core_cm4.h **** #define NVIC_USER_IRQ_OFFSET          16
1637:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 33


1638:Drivers/CMSIS/Include/core_cm4.h **** 
1639:Drivers/CMSIS/Include/core_cm4.h **** /* The following EXC_RETURN values are saved the LR on exception entry */
1640:Drivers/CMSIS/Include/core_cm4.h **** #define EXC_RETURN_HANDLER         (0xFFFFFFF1UL)     /* return to Handler mode, uses MSP after ret
1641:Drivers/CMSIS/Include/core_cm4.h **** #define EXC_RETURN_THREAD_MSP      (0xFFFFFFF9UL)     /* return to Thread mode, uses MSP after retu
1642:Drivers/CMSIS/Include/core_cm4.h **** #define EXC_RETURN_THREAD_PSP      (0xFFFFFFFDUL)     /* return to Thread mode, uses PSP after retu
1643:Drivers/CMSIS/Include/core_cm4.h **** #define EXC_RETURN_HANDLER_FPU     (0xFFFFFFE1UL)     /* return to Handler mode, uses MSP after ret
1644:Drivers/CMSIS/Include/core_cm4.h **** #define EXC_RETURN_THREAD_MSP_FPU  (0xFFFFFFE9UL)     /* return to Thread mode, uses MSP after retu
1645:Drivers/CMSIS/Include/core_cm4.h **** #define EXC_RETURN_THREAD_PSP_FPU  (0xFFFFFFEDUL)     /* return to Thread mode, uses PSP after retu
1646:Drivers/CMSIS/Include/core_cm4.h **** 
1647:Drivers/CMSIS/Include/core_cm4.h **** 
1648:Drivers/CMSIS/Include/core_cm4.h **** /**
1649:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Set Priority Grouping
1650:Drivers/CMSIS/Include/core_cm4.h ****   \details Sets the priority grouping field using the required unlock sequence.
1651:Drivers/CMSIS/Include/core_cm4.h ****            The parameter PriorityGroup is assigned to the field SCB->AIRCR [10:8] PRIGROUP field.
1652:Drivers/CMSIS/Include/core_cm4.h ****            Only values from 0..7 are used.
1653:Drivers/CMSIS/Include/core_cm4.h ****            In case of a conflict between priority grouping and available
1654:Drivers/CMSIS/Include/core_cm4.h ****            priority bits (__NVIC_PRIO_BITS), the smallest possible priority group is set.
1655:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      PriorityGroup  Priority grouping field.
1656:Drivers/CMSIS/Include/core_cm4.h ****  */
1657:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_SetPriorityGrouping(uint32_t PriorityGroup)
  40              		.loc 2 1657 22 view .LVU3
  41              	.LBB39:
1658:Drivers/CMSIS/Include/core_cm4.h **** {
1659:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t reg_value;
  42              		.loc 2 1659 3 view .LVU4
1660:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PriorityGroupTmp = (PriorityGroup & (uint32_t)0x07UL);             /* only values 0..7 a
  43              		.loc 2 1660 3 view .LVU5
1661:Drivers/CMSIS/Include/core_cm4.h **** 
1662:Drivers/CMSIS/Include/core_cm4.h ****   reg_value  =  SCB->AIRCR;                                                   /* read old register 
  44              		.loc 2 1662 3 view .LVU6
  45              		.loc 2 1662 14 is_stmt 0 view .LVU7
  46 0000 074A     		ldr	r2, .L2
  47 0002 D368     		ldr	r3, [r2, #12]
  48              	.LVL1:
1663:Drivers/CMSIS/Include/core_cm4.h ****   reg_value &= ~((uint32_t)(SCB_AIRCR_VECTKEY_Msk | SCB_AIRCR_PRIGROUP_Msk)); /* clear bits to chan
  49              		.loc 2 1663 3 is_stmt 1 view .LVU8
  50              		.loc 2 1663 13 is_stmt 0 view .LVU9
  51 0004 23F4E063 		bic	r3, r3, #1792
  52              	.LVL2:
  53              		.loc 2 1663 13 view .LVU10
  54 0008 1B04     		lsls	r3, r3, #16
  55 000a 1B0C     		lsrs	r3, r3, #16
  56              	.LVL3:
1664:Drivers/CMSIS/Include/core_cm4.h ****   reg_value  =  (reg_value                                   |
  57              		.loc 2 1664 3 is_stmt 1 view .LVU11
1665:Drivers/CMSIS/Include/core_cm4.h ****                 ((uint32_t)0x5FAUL << SCB_AIRCR_VECTKEY_Pos) |
1666:Drivers/CMSIS/Include/core_cm4.h ****                 (PriorityGroupTmp << SCB_AIRCR_PRIGROUP_Pos)  );              /* Insert write key a
  58              		.loc 2 1666 35 is_stmt 0 view .LVU12
  59 000c 0002     		lsls	r0, r0, #8
  60              	.LVL4:
  61              		.loc 2 1666 35 view .LVU13
  62 000e 00F4E060 		and	r0, r0, #1792
1665:Drivers/CMSIS/Include/core_cm4.h ****                 ((uint32_t)0x5FAUL << SCB_AIRCR_VECTKEY_Pos) |
  63              		.loc 2 1665 62 view .LVU14
  64 0012 0343     		orrs	r3, r3, r0
  65              	.LVL5:
1664:Drivers/CMSIS/Include/core_cm4.h ****   reg_value  =  (reg_value                                   |
ARM GAS  /tmp/ccPRqU3T.s 			page 34


  66              		.loc 2 1664 14 view .LVU15
  67 0014 43F0BF63 		orr	r3, r3, #100139008
  68 0018 43F40033 		orr	r3, r3, #131072
  69              	.LVL6:
1667:Drivers/CMSIS/Include/core_cm4.h ****   SCB->AIRCR =  reg_value;
  70              		.loc 2 1667 3 is_stmt 1 view .LVU16
  71              		.loc 2 1667 14 is_stmt 0 view .LVU17
  72 001c D360     		str	r3, [r2, #12]
  73              	.LVL7:
  74              		.loc 2 1667 14 view .LVU18
  75              	.LBE39:
  76              	.LBE38:
 150:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
  77              		.loc 1 150 1 view .LVU19
  78 001e 7047     		bx	lr
  79              	.L3:
  80              		.align	2
  81              	.L2:
  82 0020 00ED00E0 		.word	-536810240
  83              		.cfi_endproc
  84              	.LFE130:
  86              		.section	.text.HAL_NVIC_SetPriority,"ax",%progbits
  87              		.align	1
  88              		.global	HAL_NVIC_SetPriority
  89              		.syntax unified
  90              		.thumb
  91              		.thumb_func
  93              	HAL_NVIC_SetPriority:
  94              	.LVL8:
  95              	.LFB131:
 151:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 152:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 153:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Sets the priority of an interrupt.
 154:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number.
 155:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 156:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 157:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  PreemptPriority The preemption priority for the IRQn channel.
 158:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be a value between 0 and 15
 159:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         A lower priority value indicates a higher priority 
 160:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  SubPriority the subpriority level for the IRQ channel.
 161:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be a value between 0 and 15
 162:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         A lower priority value indicates a higher priority.          
 163:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 164:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 165:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_SetPriority(IRQn_Type IRQn, uint32_t PreemptPriority, uint32_t SubPriority)
 166:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** { 
  96              		.loc 1 166 1 is_stmt 1 view -0
  97              		.cfi_startproc
  98              		@ args = 0, pretend = 0, frame = 0
  99              		@ frame_needed = 0, uses_anonymous_args = 0
 100              		.loc 1 166 1 is_stmt 0 view .LVU21
 101 0000 00B5     		push	{lr}
 102              	.LCFI0:
 103              		.cfi_def_cfa_offset 4
 104              		.cfi_offset 14, -4
 167:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   uint32_t prioritygroup = 0x00U;
 105              		.loc 1 167 3 is_stmt 1 view .LVU22
ARM GAS  /tmp/ccPRqU3T.s 			page 35


 106              	.LVL9:
 168:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 169:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 170:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_SUB_PRIORITY(SubPriority));
 107              		.loc 1 170 3 view .LVU23
 171:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_PREEMPTION_PRIORITY(PreemptPriority));
 108              		.loc 1 171 3 view .LVU24
 172:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 173:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   prioritygroup = NVIC_GetPriorityGrouping();
 109              		.loc 1 173 3 view .LVU25
 110              	.LBB46:
 111              	.LBI46:
1668:Drivers/CMSIS/Include/core_cm4.h **** }
1669:Drivers/CMSIS/Include/core_cm4.h **** 
1670:Drivers/CMSIS/Include/core_cm4.h **** 
1671:Drivers/CMSIS/Include/core_cm4.h **** /**
1672:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Get Priority Grouping
1673:Drivers/CMSIS/Include/core_cm4.h ****   \details Reads the priority grouping field from the NVIC Interrupt Controller.
1674:Drivers/CMSIS/Include/core_cm4.h ****   \return                Priority grouping field (SCB->AIRCR [10:8] PRIGROUP field).
1675:Drivers/CMSIS/Include/core_cm4.h ****  */
1676:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t __NVIC_GetPriorityGrouping(void)
 112              		.loc 2 1676 26 view .LVU26
 113              	.LBB47:
1677:Drivers/CMSIS/Include/core_cm4.h **** {
1678:Drivers/CMSIS/Include/core_cm4.h ****   return ((uint32_t)((SCB->AIRCR & SCB_AIRCR_PRIGROUP_Msk) >> SCB_AIRCR_PRIGROUP_Pos));
 114              		.loc 2 1678 3 view .LVU27
 115              		.loc 2 1678 26 is_stmt 0 view .LVU28
 116 0002 194B     		ldr	r3, .L10
 117 0004 DB68     		ldr	r3, [r3, #12]
 118              		.loc 2 1678 11 view .LVU29
 119 0006 C3F30223 		ubfx	r3, r3, #8, #3
 120              	.LVL10:
 121              		.loc 2 1678 11 view .LVU30
 122              	.LBE47:
 123              	.LBE46:
 174:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 175:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_SetPriority(IRQn, NVIC_EncodePriority(prioritygroup, PreemptPriority, SubPriority));
 124              		.loc 1 175 3 is_stmt 1 view .LVU31
 125              	.LBB48:
 126              	.LBI48:
1679:Drivers/CMSIS/Include/core_cm4.h **** }
1680:Drivers/CMSIS/Include/core_cm4.h **** 
1681:Drivers/CMSIS/Include/core_cm4.h **** 
1682:Drivers/CMSIS/Include/core_cm4.h **** /**
1683:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Enable Interrupt
1684:Drivers/CMSIS/Include/core_cm4.h ****   \details Enables a device specific interrupt in the NVIC interrupt controller.
1685:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1686:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1687:Drivers/CMSIS/Include/core_cm4.h ****  */
1688:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_EnableIRQ(IRQn_Type IRQn)
1689:Drivers/CMSIS/Include/core_cm4.h **** {
1690:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1691:Drivers/CMSIS/Include/core_cm4.h ****   {
1692:Drivers/CMSIS/Include/core_cm4.h ****     NVIC->ISER[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1693:Drivers/CMSIS/Include/core_cm4.h ****   }
1694:Drivers/CMSIS/Include/core_cm4.h **** }
1695:Drivers/CMSIS/Include/core_cm4.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 36


1696:Drivers/CMSIS/Include/core_cm4.h **** 
1697:Drivers/CMSIS/Include/core_cm4.h **** /**
1698:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Get Interrupt Enable status
1699:Drivers/CMSIS/Include/core_cm4.h ****   \details Returns a device specific interrupt enable status from the NVIC interrupt controller.
1700:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1701:Drivers/CMSIS/Include/core_cm4.h ****   \return             0  Interrupt is not enabled.
1702:Drivers/CMSIS/Include/core_cm4.h ****   \return             1  Interrupt is enabled.
1703:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1704:Drivers/CMSIS/Include/core_cm4.h ****  */
1705:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t __NVIC_GetEnableIRQ(IRQn_Type IRQn)
1706:Drivers/CMSIS/Include/core_cm4.h **** {
1707:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1708:Drivers/CMSIS/Include/core_cm4.h ****   {
1709:Drivers/CMSIS/Include/core_cm4.h ****     return((uint32_t)(((NVIC->ISER[(((uint32_t)IRQn) >> 5UL)] & (1UL << (((uint32_t)IRQn) & 0x1FUL)
1710:Drivers/CMSIS/Include/core_cm4.h ****   }
1711:Drivers/CMSIS/Include/core_cm4.h ****   else
1712:Drivers/CMSIS/Include/core_cm4.h ****   {
1713:Drivers/CMSIS/Include/core_cm4.h ****     return(0U);
1714:Drivers/CMSIS/Include/core_cm4.h ****   }
1715:Drivers/CMSIS/Include/core_cm4.h **** }
1716:Drivers/CMSIS/Include/core_cm4.h **** 
1717:Drivers/CMSIS/Include/core_cm4.h **** 
1718:Drivers/CMSIS/Include/core_cm4.h **** /**
1719:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Disable Interrupt
1720:Drivers/CMSIS/Include/core_cm4.h ****   \details Disables a device specific interrupt in the NVIC interrupt controller.
1721:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1722:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1723:Drivers/CMSIS/Include/core_cm4.h ****  */
1724:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_DisableIRQ(IRQn_Type IRQn)
1725:Drivers/CMSIS/Include/core_cm4.h **** {
1726:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1727:Drivers/CMSIS/Include/core_cm4.h ****   {
1728:Drivers/CMSIS/Include/core_cm4.h ****     NVIC->ICER[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1729:Drivers/CMSIS/Include/core_cm4.h ****     __DSB();
1730:Drivers/CMSIS/Include/core_cm4.h ****     __ISB();
1731:Drivers/CMSIS/Include/core_cm4.h ****   }
1732:Drivers/CMSIS/Include/core_cm4.h **** }
1733:Drivers/CMSIS/Include/core_cm4.h **** 
1734:Drivers/CMSIS/Include/core_cm4.h **** 
1735:Drivers/CMSIS/Include/core_cm4.h **** /**
1736:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Get Pending Interrupt
1737:Drivers/CMSIS/Include/core_cm4.h ****   \details Reads the NVIC pending register and returns the pending bit for the specified device spe
1738:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1739:Drivers/CMSIS/Include/core_cm4.h ****   \return             0  Interrupt status is not pending.
1740:Drivers/CMSIS/Include/core_cm4.h ****   \return             1  Interrupt status is pending.
1741:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1742:Drivers/CMSIS/Include/core_cm4.h ****  */
1743:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t __NVIC_GetPendingIRQ(IRQn_Type IRQn)
1744:Drivers/CMSIS/Include/core_cm4.h **** {
1745:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1746:Drivers/CMSIS/Include/core_cm4.h ****   {
1747:Drivers/CMSIS/Include/core_cm4.h ****     return((uint32_t)(((NVIC->ISPR[(((uint32_t)IRQn) >> 5UL)] & (1UL << (((uint32_t)IRQn) & 0x1FUL)
1748:Drivers/CMSIS/Include/core_cm4.h ****   }
1749:Drivers/CMSIS/Include/core_cm4.h ****   else
1750:Drivers/CMSIS/Include/core_cm4.h ****   {
1751:Drivers/CMSIS/Include/core_cm4.h ****     return(0U);
1752:Drivers/CMSIS/Include/core_cm4.h ****   }
ARM GAS  /tmp/ccPRqU3T.s 			page 37


1753:Drivers/CMSIS/Include/core_cm4.h **** }
1754:Drivers/CMSIS/Include/core_cm4.h **** 
1755:Drivers/CMSIS/Include/core_cm4.h **** 
1756:Drivers/CMSIS/Include/core_cm4.h **** /**
1757:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Set Pending Interrupt
1758:Drivers/CMSIS/Include/core_cm4.h ****   \details Sets the pending bit of a device specific interrupt in the NVIC pending register.
1759:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1760:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1761:Drivers/CMSIS/Include/core_cm4.h ****  */
1762:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_SetPendingIRQ(IRQn_Type IRQn)
1763:Drivers/CMSIS/Include/core_cm4.h **** {
1764:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1765:Drivers/CMSIS/Include/core_cm4.h ****   {
1766:Drivers/CMSIS/Include/core_cm4.h ****     NVIC->ISPR[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1767:Drivers/CMSIS/Include/core_cm4.h ****   }
1768:Drivers/CMSIS/Include/core_cm4.h **** }
1769:Drivers/CMSIS/Include/core_cm4.h **** 
1770:Drivers/CMSIS/Include/core_cm4.h **** 
1771:Drivers/CMSIS/Include/core_cm4.h **** /**
1772:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Clear Pending Interrupt
1773:Drivers/CMSIS/Include/core_cm4.h ****   \details Clears the pending bit of a device specific interrupt in the NVIC pending register.
1774:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1775:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1776:Drivers/CMSIS/Include/core_cm4.h ****  */
1777:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_ClearPendingIRQ(IRQn_Type IRQn)
1778:Drivers/CMSIS/Include/core_cm4.h **** {
1779:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1780:Drivers/CMSIS/Include/core_cm4.h ****   {
1781:Drivers/CMSIS/Include/core_cm4.h ****     NVIC->ICPR[(((uint32_t)IRQn) >> 5UL)] = (uint32_t)(1UL << (((uint32_t)IRQn) & 0x1FUL));
1782:Drivers/CMSIS/Include/core_cm4.h ****   }
1783:Drivers/CMSIS/Include/core_cm4.h **** }
1784:Drivers/CMSIS/Include/core_cm4.h **** 
1785:Drivers/CMSIS/Include/core_cm4.h **** 
1786:Drivers/CMSIS/Include/core_cm4.h **** /**
1787:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Get Active Interrupt
1788:Drivers/CMSIS/Include/core_cm4.h ****   \details Reads the active register in the NVIC and returns the active bit for the device specific
1789:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Device specific interrupt number.
1790:Drivers/CMSIS/Include/core_cm4.h ****   \return             0  Interrupt status is not active.
1791:Drivers/CMSIS/Include/core_cm4.h ****   \return             1  Interrupt status is active.
1792:Drivers/CMSIS/Include/core_cm4.h ****   \note    IRQn must not be negative.
1793:Drivers/CMSIS/Include/core_cm4.h ****  */
1794:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t __NVIC_GetActive(IRQn_Type IRQn)
1795:Drivers/CMSIS/Include/core_cm4.h **** {
1796:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1797:Drivers/CMSIS/Include/core_cm4.h ****   {
1798:Drivers/CMSIS/Include/core_cm4.h ****     return((uint32_t)(((NVIC->IABR[(((uint32_t)IRQn) >> 5UL)] & (1UL << (((uint32_t)IRQn) & 0x1FUL)
1799:Drivers/CMSIS/Include/core_cm4.h ****   }
1800:Drivers/CMSIS/Include/core_cm4.h ****   else
1801:Drivers/CMSIS/Include/core_cm4.h ****   {
1802:Drivers/CMSIS/Include/core_cm4.h ****     return(0U);
1803:Drivers/CMSIS/Include/core_cm4.h ****   }
1804:Drivers/CMSIS/Include/core_cm4.h **** }
1805:Drivers/CMSIS/Include/core_cm4.h **** 
1806:Drivers/CMSIS/Include/core_cm4.h **** 
1807:Drivers/CMSIS/Include/core_cm4.h **** /**
1808:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Set Interrupt Priority
1809:Drivers/CMSIS/Include/core_cm4.h ****   \details Sets the priority of a device specific interrupt or a processor exception.
ARM GAS  /tmp/ccPRqU3T.s 			page 38


1810:Drivers/CMSIS/Include/core_cm4.h ****            The interrupt number can be positive to specify a device specific interrupt,
1811:Drivers/CMSIS/Include/core_cm4.h ****            or negative to specify a processor exception.
1812:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]      IRQn  Interrupt number.
1813:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]  priority  Priority to set.
1814:Drivers/CMSIS/Include/core_cm4.h ****   \note    The priority cannot be set for every processor exception.
1815:Drivers/CMSIS/Include/core_cm4.h ****  */
1816:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_SetPriority(IRQn_Type IRQn, uint32_t priority)
1817:Drivers/CMSIS/Include/core_cm4.h **** {
1818:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1819:Drivers/CMSIS/Include/core_cm4.h ****   {
1820:Drivers/CMSIS/Include/core_cm4.h ****     NVIC->IP[((uint32_t)IRQn)]               = (uint8_t)((priority << (8U - __NVIC_PRIO_BITS)) & (u
1821:Drivers/CMSIS/Include/core_cm4.h ****   }
1822:Drivers/CMSIS/Include/core_cm4.h ****   else
1823:Drivers/CMSIS/Include/core_cm4.h ****   {
1824:Drivers/CMSIS/Include/core_cm4.h ****     SCB->SHP[(((uint32_t)IRQn) & 0xFUL)-4UL] = (uint8_t)((priority << (8U - __NVIC_PRIO_BITS)) & (u
1825:Drivers/CMSIS/Include/core_cm4.h ****   }
1826:Drivers/CMSIS/Include/core_cm4.h **** }
1827:Drivers/CMSIS/Include/core_cm4.h **** 
1828:Drivers/CMSIS/Include/core_cm4.h **** 
1829:Drivers/CMSIS/Include/core_cm4.h **** /**
1830:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Get Interrupt Priority
1831:Drivers/CMSIS/Include/core_cm4.h ****   \details Reads the priority of a device specific interrupt or a processor exception.
1832:Drivers/CMSIS/Include/core_cm4.h ****            The interrupt number can be positive to specify a device specific interrupt,
1833:Drivers/CMSIS/Include/core_cm4.h ****            or negative to specify a processor exception.
1834:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]   IRQn  Interrupt number.
1835:Drivers/CMSIS/Include/core_cm4.h ****   \return             Interrupt Priority.
1836:Drivers/CMSIS/Include/core_cm4.h ****                       Value is aligned automatically to the implemented priority bits of the microc
1837:Drivers/CMSIS/Include/core_cm4.h ****  */
1838:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t __NVIC_GetPriority(IRQn_Type IRQn)
1839:Drivers/CMSIS/Include/core_cm4.h **** {
1840:Drivers/CMSIS/Include/core_cm4.h **** 
1841:Drivers/CMSIS/Include/core_cm4.h ****   if ((int32_t)(IRQn) >= 0)
1842:Drivers/CMSIS/Include/core_cm4.h ****   {
1843:Drivers/CMSIS/Include/core_cm4.h ****     return(((uint32_t)NVIC->IP[((uint32_t)IRQn)]               >> (8U - __NVIC_PRIO_BITS)));
1844:Drivers/CMSIS/Include/core_cm4.h ****   }
1845:Drivers/CMSIS/Include/core_cm4.h ****   else
1846:Drivers/CMSIS/Include/core_cm4.h ****   {
1847:Drivers/CMSIS/Include/core_cm4.h ****     return(((uint32_t)SCB->SHP[(((uint32_t)IRQn) & 0xFUL)-4UL] >> (8U - __NVIC_PRIO_BITS)));
1848:Drivers/CMSIS/Include/core_cm4.h ****   }
1849:Drivers/CMSIS/Include/core_cm4.h **** }
1850:Drivers/CMSIS/Include/core_cm4.h **** 
1851:Drivers/CMSIS/Include/core_cm4.h **** 
1852:Drivers/CMSIS/Include/core_cm4.h **** /**
1853:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Encode Priority
1854:Drivers/CMSIS/Include/core_cm4.h ****   \details Encodes the priority for an interrupt with the given priority group,
1855:Drivers/CMSIS/Include/core_cm4.h ****            preemptive priority value, and subpriority value.
1856:Drivers/CMSIS/Include/core_cm4.h ****            In case of a conflict between priority grouping and available
1857:Drivers/CMSIS/Include/core_cm4.h ****            priority bits (__NVIC_PRIO_BITS), the smallest possible priority group is set.
1858:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]     PriorityGroup  Used priority group.
1859:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]   PreemptPriority  Preemptive priority value (starting from 0).
1860:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]       SubPriority  Subpriority value (starting from 0).
1861:Drivers/CMSIS/Include/core_cm4.h ****   \return                        Encoded priority. Value can be used in the function \ref NVIC_SetP
1862:Drivers/CMSIS/Include/core_cm4.h ****  */
1863:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t NVIC_EncodePriority (uint32_t PriorityGroup, uint32_t PreemptPriority, uin
 127              		.loc 2 1863 26 view .LVU32
 128              	.LBB49:
1864:Drivers/CMSIS/Include/core_cm4.h **** {
ARM GAS  /tmp/ccPRqU3T.s 			page 39


1865:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PriorityGroupTmp = (PriorityGroup & (uint32_t)0x07UL);   /* only values 0..7 are used   
 129              		.loc 2 1865 3 view .LVU33
1866:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PreemptPriorityBits;
 130              		.loc 2 1866 3 view .LVU34
1867:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t SubPriorityBits;
 131              		.loc 2 1867 3 view .LVU35
1868:Drivers/CMSIS/Include/core_cm4.h **** 
1869:Drivers/CMSIS/Include/core_cm4.h ****   PreemptPriorityBits = ((7UL - PriorityGroupTmp) > (uint32_t)(__NVIC_PRIO_BITS)) ? (uint32_t)(__NV
 132              		.loc 2 1869 3 view .LVU36
 133              		.loc 2 1869 31 is_stmt 0 view .LVU37
 134 000a C3F1070C 		rsb	ip, r3, #7
 135              		.loc 2 1869 23 view .LVU38
 136 000e BCF1040F 		cmp	ip, #4
 137 0012 28BF     		it	cs
 138 0014 4FF0040C 		movcs	ip, #4
 139              	.LVL11:
1870:Drivers/CMSIS/Include/core_cm4.h ****   SubPriorityBits     = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint
 140              		.loc 2 1870 3 is_stmt 1 view .LVU39
 141              		.loc 2 1870 44 is_stmt 0 view .LVU40
 142 0018 03F1040E 		add	lr, r3, #4
 143              		.loc 2 1870 109 view .LVU41
 144 001c BEF1060F 		cmp	lr, #6
 145 0020 18D9     		bls	.L8
 146 0022 033B     		subs	r3, r3, #3
 147              	.LVL12:
 148              	.L5:
1871:Drivers/CMSIS/Include/core_cm4.h **** 
1872:Drivers/CMSIS/Include/core_cm4.h ****   return (
 149              		.loc 2 1872 3 is_stmt 1 view .LVU42
1873:Drivers/CMSIS/Include/core_cm4.h ****            ((PreemptPriority & (uint32_t)((1UL << (PreemptPriorityBits)) - 1UL)) << SubPriorityBits
 150              		.loc 2 1873 30 is_stmt 0 view .LVU43
 151 0024 4FF0FF3E 		mov	lr, #-1
 152              	.LVL13:
 153              		.loc 2 1873 30 view .LVU44
 154 0028 0EFA0CFC 		lsl	ip, lr, ip
 155              	.LVL14:
 156              		.loc 2 1873 30 view .LVU45
 157 002c 21EA0C01 		bic	r1, r1, ip
 158              	.LVL15:
 159              		.loc 2 1873 82 view .LVU46
 160 0030 9940     		lsls	r1, r1, r3
1874:Drivers/CMSIS/Include/core_cm4.h ****            ((SubPriority     & (uint32_t)((1UL << (SubPriorityBits    )) - 1UL)))
 161              		.loc 2 1874 30 view .LVU47
 162 0032 0EFA03F3 		lsl	r3, lr, r3
 163              	.LVL16:
 164              		.loc 2 1874 30 view .LVU48
 165 0036 22EA0303 		bic	r3, r2, r3
1873:Drivers/CMSIS/Include/core_cm4.h ****            ((PreemptPriority & (uint32_t)((1UL << (PreemptPriorityBits)) - 1UL)) << SubPriorityBits
 166              		.loc 2 1873 102 view .LVU49
 167 003a 1943     		orrs	r1, r1, r3
 168              	.LVL17:
1873:Drivers/CMSIS/Include/core_cm4.h ****            ((PreemptPriority & (uint32_t)((1UL << (PreemptPriorityBits)) - 1UL)) << SubPriorityBits
 169              		.loc 2 1873 102 view .LVU50
 170              	.LBE49:
 171              	.LBE48:
 172              	.LBB51:
 173              	.LBI51:
ARM GAS  /tmp/ccPRqU3T.s 			page 40


1816:Drivers/CMSIS/Include/core_cm4.h **** {
 174              		.loc 2 1816 22 is_stmt 1 view .LVU51
 175              	.LBB52:
1818:Drivers/CMSIS/Include/core_cm4.h ****   {
 176              		.loc 2 1818 3 view .LVU52
1818:Drivers/CMSIS/Include/core_cm4.h ****   {
 177              		.loc 2 1818 6 is_stmt 0 view .LVU53
 178 003c 0028     		cmp	r0, #0
 179 003e 0BDB     		blt	.L6
1820:Drivers/CMSIS/Include/core_cm4.h ****   }
 180              		.loc 2 1820 5 is_stmt 1 view .LVU54
1820:Drivers/CMSIS/Include/core_cm4.h ****   }
 181              		.loc 2 1820 48 is_stmt 0 view .LVU55
 182 0040 0901     		lsls	r1, r1, #4
 183              	.LVL18:
1820:Drivers/CMSIS/Include/core_cm4.h ****   }
 184              		.loc 2 1820 48 view .LVU56
 185 0042 C9B2     		uxtb	r1, r1
1820:Drivers/CMSIS/Include/core_cm4.h ****   }
 186              		.loc 2 1820 46 view .LVU57
 187 0044 00F16040 		add	r0, r0, #-536870912
 188              	.LVL19:
1820:Drivers/CMSIS/Include/core_cm4.h ****   }
 189              		.loc 2 1820 46 view .LVU58
 190 0048 00F56140 		add	r0, r0, #57600
 191 004c 80F80013 		strb	r1, [r0, #768]
 192              	.LVL20:
 193              	.L4:
1820:Drivers/CMSIS/Include/core_cm4.h ****   }
 194              		.loc 2 1820 46 view .LVU59
 195              	.LBE52:
 196              	.LBE51:
 176:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 197              		.loc 1 176 1 view .LVU60
 198 0050 5DF804FB 		ldr	pc, [sp], #4
 199              	.LVL21:
 200              	.L8:
 201              	.LBB54:
 202              	.LBB50:
1870:Drivers/CMSIS/Include/core_cm4.h **** 
 203              		.loc 2 1870 109 view .LVU61
 204 0054 0023     		movs	r3, #0
 205              	.LVL22:
1870:Drivers/CMSIS/Include/core_cm4.h **** 
 206              		.loc 2 1870 109 view .LVU62
 207 0056 E5E7     		b	.L5
 208              	.LVL23:
 209              	.L6:
1870:Drivers/CMSIS/Include/core_cm4.h **** 
 210              		.loc 2 1870 109 view .LVU63
 211              	.LBE50:
 212              	.LBE54:
 213              	.LBB55:
 214              	.LBB53:
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 215              		.loc 2 1824 5 is_stmt 1 view .LVU64
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
ARM GAS  /tmp/ccPRqU3T.s 			page 41


 216              		.loc 2 1824 32 is_stmt 0 view .LVU65
 217 0058 00F00F00 		and	r0, r0, #15
 218              	.LVL24:
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 219              		.loc 2 1824 48 view .LVU66
 220 005c 0901     		lsls	r1, r1, #4
 221              	.LVL25:
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 222              		.loc 2 1824 48 view .LVU67
 223 005e C9B2     		uxtb	r1, r1
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 224              		.loc 2 1824 46 view .LVU68
 225 0060 024B     		ldr	r3, .L10+4
 226 0062 1954     		strb	r1, [r3, r0]
 227              	.LVL26:
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 228              		.loc 2 1824 46 view .LVU69
 229              	.LBE53:
 230              	.LBE55:
 231              		.loc 1 176 1 view .LVU70
 232 0064 F4E7     		b	.L4
 233              	.L11:
 234 0066 00BF     		.align	2
 235              	.L10:
 236 0068 00ED00E0 		.word	-536810240
 237 006c 14ED00E0 		.word	-536810220
 238              		.cfi_endproc
 239              	.LFE131:
 241              		.section	.text.HAL_NVIC_EnableIRQ,"ax",%progbits
 242              		.align	1
 243              		.global	HAL_NVIC_EnableIRQ
 244              		.syntax unified
 245              		.thumb
 246              		.thumb_func
 248              	HAL_NVIC_EnableIRQ:
 249              	.LVL27:
 250              	.LFB132:
 177:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 178:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 179:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Enables a device specific interrupt in the NVIC interrupt controller.
 180:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @note   To configure interrupts priority correctly, the NVIC_PriorityGroupConfig()
 181:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         function should be called before. 
 182:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number.
 183:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 184:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 185:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 186:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 187:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_EnableIRQ(IRQn_Type IRQn)
 188:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 251              		.loc 1 188 1 is_stmt 1 view -0
 252              		.cfi_startproc
 253              		@ args = 0, pretend = 0, frame = 0
 254              		@ frame_needed = 0, uses_anonymous_args = 0
 255              		@ link register save eliminated.
 189:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 190:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_DEVICE_IRQ(IRQn));
 256              		.loc 1 190 3 view .LVU72
ARM GAS  /tmp/ccPRqU3T.s 			page 42


 191:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 192:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Enable interrupt */
 193:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_EnableIRQ(IRQn);
 257              		.loc 1 193 3 view .LVU73
 258              	.LBB56:
 259              	.LBI56:
1688:Drivers/CMSIS/Include/core_cm4.h **** {
 260              		.loc 2 1688 22 view .LVU74
 261              	.LBB57:
1690:Drivers/CMSIS/Include/core_cm4.h ****   {
 262              		.loc 2 1690 3 view .LVU75
1690:Drivers/CMSIS/Include/core_cm4.h ****   {
 263              		.loc 2 1690 6 is_stmt 0 view .LVU76
 264 0000 0028     		cmp	r0, #0
 265              	.LVL28:
1690:Drivers/CMSIS/Include/core_cm4.h ****   {
 266              		.loc 2 1690 6 view .LVU77
 267 0002 07DB     		blt	.L12
1692:Drivers/CMSIS/Include/core_cm4.h ****   }
 268              		.loc 2 1692 5 is_stmt 1 view .LVU78
1692:Drivers/CMSIS/Include/core_cm4.h ****   }
 269              		.loc 2 1692 81 is_stmt 0 view .LVU79
 270 0004 00F01F02 		and	r2, r0, #31
1692:Drivers/CMSIS/Include/core_cm4.h ****   }
 271              		.loc 2 1692 34 view .LVU80
 272 0008 4009     		lsrs	r0, r0, #5
1692:Drivers/CMSIS/Include/core_cm4.h ****   }
 273              		.loc 2 1692 45 view .LVU81
 274 000a 0123     		movs	r3, #1
 275 000c 9340     		lsls	r3, r3, r2
1692:Drivers/CMSIS/Include/core_cm4.h ****   }
 276              		.loc 2 1692 43 view .LVU82
 277 000e 024A     		ldr	r2, .L14
 278 0010 42F82030 		str	r3, [r2, r0, lsl #2]
 279              	.LVL29:
 280              	.L12:
1692:Drivers/CMSIS/Include/core_cm4.h ****   }
 281              		.loc 2 1692 43 view .LVU83
 282              	.LBE57:
 283              	.LBE56:
 194:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 284              		.loc 1 194 1 view .LVU84
 285 0014 7047     		bx	lr
 286              	.L15:
 287 0016 00BF     		.align	2
 288              	.L14:
 289 0018 00E100E0 		.word	-536813312
 290              		.cfi_endproc
 291              	.LFE132:
 293              		.section	.text.HAL_NVIC_DisableIRQ,"ax",%progbits
 294              		.align	1
 295              		.global	HAL_NVIC_DisableIRQ
 296              		.syntax unified
 297              		.thumb
 298              		.thumb_func
 300              	HAL_NVIC_DisableIRQ:
 301              	.LVL30:
ARM GAS  /tmp/ccPRqU3T.s 			page 43


 302              	.LFB133:
 195:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 196:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 197:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Disables a device specific interrupt in the NVIC interrupt controller.
 198:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number.
 199:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 200:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 201:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 202:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 203:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_DisableIRQ(IRQn_Type IRQn)
 204:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 303              		.loc 1 204 1 is_stmt 1 view -0
 304              		.cfi_startproc
 305              		@ args = 0, pretend = 0, frame = 0
 306              		@ frame_needed = 0, uses_anonymous_args = 0
 307              		@ link register save eliminated.
 205:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 206:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_DEVICE_IRQ(IRQn));
 308              		.loc 1 206 3 view .LVU86
 207:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 208:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Disable interrupt */
 209:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_DisableIRQ(IRQn);
 309              		.loc 1 209 3 view .LVU87
 310              	.LBB64:
 311              	.LBI64:
1724:Drivers/CMSIS/Include/core_cm4.h **** {
 312              		.loc 2 1724 22 view .LVU88
 313              	.LBB65:
1726:Drivers/CMSIS/Include/core_cm4.h ****   {
 314              		.loc 2 1726 3 view .LVU89
1726:Drivers/CMSIS/Include/core_cm4.h ****   {
 315              		.loc 2 1726 6 is_stmt 0 view .LVU90
 316 0000 0028     		cmp	r0, #0
 317              	.LVL31:
1726:Drivers/CMSIS/Include/core_cm4.h ****   {
 318              		.loc 2 1726 6 view .LVU91
 319 0002 0CDB     		blt	.L16
1728:Drivers/CMSIS/Include/core_cm4.h ****     __DSB();
 320              		.loc 2 1728 5 is_stmt 1 view .LVU92
1728:Drivers/CMSIS/Include/core_cm4.h ****     __DSB();
 321              		.loc 2 1728 81 is_stmt 0 view .LVU93
 322 0004 00F01F02 		and	r2, r0, #31
1728:Drivers/CMSIS/Include/core_cm4.h ****     __DSB();
 323              		.loc 2 1728 34 view .LVU94
 324 0008 4009     		lsrs	r0, r0, #5
1728:Drivers/CMSIS/Include/core_cm4.h ****     __DSB();
 325              		.loc 2 1728 45 view .LVU95
 326 000a 0123     		movs	r3, #1
 327 000c 9340     		lsls	r3, r3, r2
1728:Drivers/CMSIS/Include/core_cm4.h ****     __DSB();
 328              		.loc 2 1728 43 view .LVU96
 329 000e 2030     		adds	r0, r0, #32
 330 0010 034A     		ldr	r2, .L18
 331 0012 42F82030 		str	r3, [r2, r0, lsl #2]
1729:Drivers/CMSIS/Include/core_cm4.h ****     __ISB();
 332              		.loc 2 1729 5 is_stmt 1 view .LVU97
 333              	.LBB66:
ARM GAS  /tmp/ccPRqU3T.s 			page 44


 334              	.LBI66:
 335              		.file 3 "Drivers/CMSIS/Include/cmsis_gcc.h"
   1:Drivers/CMSIS/Include/cmsis_gcc.h **** /**************************************************************************//**
   2:Drivers/CMSIS/Include/cmsis_gcc.h ****  * @file     cmsis_gcc.h
   3:Drivers/CMSIS/Include/cmsis_gcc.h ****  * @brief    CMSIS compiler GCC header file
   4:Drivers/CMSIS/Include/cmsis_gcc.h ****  * @version  V5.0.4
   5:Drivers/CMSIS/Include/cmsis_gcc.h ****  * @date     09. April 2018
   6:Drivers/CMSIS/Include/cmsis_gcc.h ****  ******************************************************************************/
   7:Drivers/CMSIS/Include/cmsis_gcc.h **** /*
   8:Drivers/CMSIS/Include/cmsis_gcc.h ****  * Copyright (c) 2009-2018 Arm Limited. All rights reserved.
   9:Drivers/CMSIS/Include/cmsis_gcc.h ****  *
  10:Drivers/CMSIS/Include/cmsis_gcc.h ****  * SPDX-License-Identifier: Apache-2.0
  11:Drivers/CMSIS/Include/cmsis_gcc.h ****  *
  12:Drivers/CMSIS/Include/cmsis_gcc.h ****  * Licensed under the Apache License, Version 2.0 (the License); you may
  13:Drivers/CMSIS/Include/cmsis_gcc.h ****  * not use this file except in compliance with the License.
  14:Drivers/CMSIS/Include/cmsis_gcc.h ****  * You may obtain a copy of the License at
  15:Drivers/CMSIS/Include/cmsis_gcc.h ****  *
  16:Drivers/CMSIS/Include/cmsis_gcc.h ****  * www.apache.org/licenses/LICENSE-2.0
  17:Drivers/CMSIS/Include/cmsis_gcc.h ****  *
  18:Drivers/CMSIS/Include/cmsis_gcc.h ****  * Unless required by applicable law or agreed to in writing, software
  19:Drivers/CMSIS/Include/cmsis_gcc.h ****  * distributed under the License is distributed on an AS IS BASIS, WITHOUT
  20:Drivers/CMSIS/Include/cmsis_gcc.h ****  * WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  21:Drivers/CMSIS/Include/cmsis_gcc.h ****  * See the License for the specific language governing permissions and
  22:Drivers/CMSIS/Include/cmsis_gcc.h ****  * limitations under the License.
  23:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
  24:Drivers/CMSIS/Include/cmsis_gcc.h **** 
  25:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef __CMSIS_GCC_H
  26:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_H
  27:Drivers/CMSIS/Include/cmsis_gcc.h **** 
  28:Drivers/CMSIS/Include/cmsis_gcc.h **** /* ignore some GCC warnings */
  29:Drivers/CMSIS/Include/cmsis_gcc.h **** #pragma GCC diagnostic push
  30:Drivers/CMSIS/Include/cmsis_gcc.h **** #pragma GCC diagnostic ignored "-Wsign-conversion"
  31:Drivers/CMSIS/Include/cmsis_gcc.h **** #pragma GCC diagnostic ignored "-Wconversion"
  32:Drivers/CMSIS/Include/cmsis_gcc.h **** #pragma GCC diagnostic ignored "-Wunused-parameter"
  33:Drivers/CMSIS/Include/cmsis_gcc.h **** 
  34:Drivers/CMSIS/Include/cmsis_gcc.h **** /* Fallback for __has_builtin */
  35:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef __has_builtin
  36:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __has_builtin(x) (0)
  37:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  38:Drivers/CMSIS/Include/cmsis_gcc.h **** 
  39:Drivers/CMSIS/Include/cmsis_gcc.h **** /* CMSIS compiler specific defines */
  40:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __ASM
  41:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __ASM                                  __asm
  42:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  43:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __INLINE
  44:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __INLINE                               inline
  45:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  46:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __STATIC_INLINE
  47:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __STATIC_INLINE                        static inline
  48:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  49:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __STATIC_FORCEINLINE                 
  50:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __STATIC_FORCEINLINE                   __attribute__((always_inline)) static inline
  51:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif                                           
  52:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __NO_RETURN
  53:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __NO_RETURN                            __attribute__((__noreturn__))
  54:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  55:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __USED
ARM GAS  /tmp/ccPRqU3T.s 			page 45


  56:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __USED                                 __attribute__((used))
  57:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  58:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __WEAK
  59:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __WEAK                                 __attribute__((weak))
  60:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  61:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __PACKED
  62:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __PACKED                               __attribute__((packed, aligned(1)))
  63:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  64:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __PACKED_STRUCT
  65:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __PACKED_STRUCT                        struct __attribute__((packed, aligned(1)))
  66:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  67:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __PACKED_UNION
  68:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __PACKED_UNION                         union __attribute__((packed, aligned(1)))
  69:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  70:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __UNALIGNED_UINT32        /* deprecated */
  71:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic push
  72:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wpacked"
  73:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wattributes"
  74:Drivers/CMSIS/Include/cmsis_gcc.h ****   struct __attribute__((packed)) T_UINT32 { uint32_t v; };
  75:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic pop
  76:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __UNALIGNED_UINT32(x)                  (((struct T_UINT32 *)(x))->v)
  77:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  78:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __UNALIGNED_UINT16_WRITE
  79:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic push
  80:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wpacked"
  81:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wattributes"
  82:Drivers/CMSIS/Include/cmsis_gcc.h ****   __PACKED_STRUCT T_UINT16_WRITE { uint16_t v; };
  83:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic pop
  84:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __UNALIGNED_UINT16_WRITE(addr, val)    (void)((((struct T_UINT16_WRITE *)(void *)(addr))-
  85:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  86:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __UNALIGNED_UINT16_READ
  87:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic push
  88:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wpacked"
  89:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wattributes"
  90:Drivers/CMSIS/Include/cmsis_gcc.h ****   __PACKED_STRUCT T_UINT16_READ { uint16_t v; };
  91:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic pop
  92:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __UNALIGNED_UINT16_READ(addr)          (((const struct T_UINT16_READ *)(const void *)(add
  93:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
  94:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __UNALIGNED_UINT32_WRITE
  95:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic push
  96:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wpacked"
  97:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wattributes"
  98:Drivers/CMSIS/Include/cmsis_gcc.h ****   __PACKED_STRUCT T_UINT32_WRITE { uint32_t v; };
  99:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic pop
 100:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __UNALIGNED_UINT32_WRITE(addr, val)    (void)((((struct T_UINT32_WRITE *)(void *)(addr))-
 101:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 102:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __UNALIGNED_UINT32_READ
 103:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic push
 104:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wpacked"
 105:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic ignored "-Wattributes"
 106:Drivers/CMSIS/Include/cmsis_gcc.h ****   __PACKED_STRUCT T_UINT32_READ { uint32_t v; };
 107:Drivers/CMSIS/Include/cmsis_gcc.h ****   #pragma GCC diagnostic pop
 108:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __UNALIGNED_UINT32_READ(addr)          (((const struct T_UINT32_READ *)(const void *)(add
 109:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 110:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __ALIGNED
 111:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __ALIGNED(x)                           __attribute__((aligned(x)))
 112:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
ARM GAS  /tmp/ccPRqU3T.s 			page 46


 113:Drivers/CMSIS/Include/cmsis_gcc.h **** #ifndef   __RESTRICT
 114:Drivers/CMSIS/Include/cmsis_gcc.h ****   #define __RESTRICT                             __restrict
 115:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 116:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 117:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 118:Drivers/CMSIS/Include/cmsis_gcc.h **** /* ###########################  Core Function Access  ########################### */
 119:Drivers/CMSIS/Include/cmsis_gcc.h **** /** \ingroup  CMSIS_Core_FunctionInterface
 120:Drivers/CMSIS/Include/cmsis_gcc.h ****     \defgroup CMSIS_Core_RegAccFunctions CMSIS Core Register Access Functions
 121:Drivers/CMSIS/Include/cmsis_gcc.h ****   @{
 122:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 123:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 124:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 125:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Enable IRQ Interrupts
 126:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Enables IRQ interrupts by clearing the I-bit in the CPSR.
 127:Drivers/CMSIS/Include/cmsis_gcc.h ****            Can only be executed in Privileged modes.
 128:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 129:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __enable_irq(void)
 130:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 131:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("cpsie i" : : : "memory");
 132:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 133:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 134:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 135:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 136:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Disable IRQ Interrupts
 137:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Disables IRQ interrupts by setting the I-bit in the CPSR.
 138:Drivers/CMSIS/Include/cmsis_gcc.h ****            Can only be executed in Privileged modes.
 139:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 140:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __disable_irq(void)
 141:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 142:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("cpsid i" : : : "memory");
 143:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 144:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 145:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 146:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 147:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Control Register
 148:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the content of the Control Register.
 149:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Control Register value
 150:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 151:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_CONTROL(void)
 152:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 153:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 154:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 155:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, control" : "=r" (result) );
 156:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 157:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 158:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 159:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 160:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 161:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 162:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Control Register (non-secure)
 163:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the content of the non-secure Control Register when in secure mode.
 164:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               non-secure Control Register value
 165:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 166:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_CONTROL_NS(void)
 167:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 168:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 169:Drivers/CMSIS/Include/cmsis_gcc.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 47


 170:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, control_ns" : "=r" (result) );
 171:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 172:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 173:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 174:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 175:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 176:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 177:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Control Register
 178:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Writes the given value to the Control Register.
 179:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    control  Control Register value to set
 180:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 181:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_CONTROL(uint32_t control)
 182:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 183:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR control, %0" : : "r" (control) : "memory");
 184:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 185:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 186:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 187:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 188:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 189:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Control Register (non-secure)
 190:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Writes the given value to the non-secure Control Register when in secure state.
 191:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    control  Control Register value to set
 192:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 193:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_CONTROL_NS(uint32_t control)
 194:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 195:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR control_ns, %0" : : "r" (control) : "memory");
 196:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 197:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 198:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 199:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 200:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 201:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get IPSR Register
 202:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the content of the IPSR Register.
 203:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               IPSR Register value
 204:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 205:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_IPSR(void)
 206:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 207:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 208:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 209:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, ipsr" : "=r" (result) );
 210:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 211:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 212:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 213:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 214:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 215:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get APSR Register
 216:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the content of the APSR Register.
 217:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               APSR Register value
 218:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 219:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_APSR(void)
 220:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 221:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 222:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 223:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, apsr" : "=r" (result) );
 224:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 225:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 226:Drivers/CMSIS/Include/cmsis_gcc.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 48


 227:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 228:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 229:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get xPSR Register
 230:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the content of the xPSR Register.
 231:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               xPSR Register value
 232:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 233:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_xPSR(void)
 234:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 235:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 236:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 237:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, xpsr" : "=r" (result) );
 238:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 239:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 240:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 241:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 242:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 243:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Process Stack Pointer
 244:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Process Stack Pointer (PSP).
 245:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               PSP Register value
 246:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 247:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_PSP(void)
 248:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 249:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 250:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 251:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, psp"  : "=r" (result) );
 252:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 253:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 254:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 255:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 256:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 257:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 258:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Process Stack Pointer (non-secure)
 259:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Process Stack Pointer (PSP) when in secure s
 260:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               PSP Register value
 261:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 262:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_PSP_NS(void)
 263:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 264:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 265:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 266:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, psp_ns"  : "=r" (result) );
 267:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 268:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 269:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 270:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 271:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 272:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 273:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Process Stack Pointer
 274:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Process Stack Pointer (PSP).
 275:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    topOfProcStack  Process Stack Pointer value to set
 276:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 277:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_PSP(uint32_t topOfProcStack)
 278:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 279:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR psp, %0" : : "r" (topOfProcStack) : );
 280:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 281:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 282:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 283:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
ARM GAS  /tmp/ccPRqU3T.s 			page 49


 284:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 285:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Process Stack Pointer (non-secure)
 286:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Process Stack Pointer (PSP) when in secure sta
 287:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    topOfProcStack  Process Stack Pointer value to set
 288:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 289:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_PSP_NS(uint32_t topOfProcStack)
 290:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 291:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR psp_ns, %0" : : "r" (topOfProcStack) : );
 292:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 293:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 294:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 295:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 296:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 297:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Main Stack Pointer
 298:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Main Stack Pointer (MSP).
 299:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               MSP Register value
 300:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 301:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_MSP(void)
 302:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 303:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 304:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 305:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, msp" : "=r" (result) );
 306:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 307:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 308:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 309:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 310:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 311:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 312:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Main Stack Pointer (non-secure)
 313:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Main Stack Pointer (MSP) when in secure stat
 314:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               MSP Register value
 315:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 316:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_MSP_NS(void)
 317:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 318:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 319:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 320:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, msp_ns" : "=r" (result) );
 321:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 322:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 323:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 324:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 325:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 326:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 327:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Main Stack Pointer
 328:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Main Stack Pointer (MSP).
 329:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    topOfMainStack  Main Stack Pointer value to set
 330:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 331:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_MSP(uint32_t topOfMainStack)
 332:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 333:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR msp, %0" : : "r" (topOfMainStack) : );
 334:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 335:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 336:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 337:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 338:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 339:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Main Stack Pointer (non-secure)
 340:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Main Stack Pointer (MSP) when in secure state.
ARM GAS  /tmp/ccPRqU3T.s 			page 50


 341:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    topOfMainStack  Main Stack Pointer value to set
 342:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 343:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_MSP_NS(uint32_t topOfMainStack)
 344:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 345:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR msp_ns, %0" : : "r" (topOfMainStack) : );
 346:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 347:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 348:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 349:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 350:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 351:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 352:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Stack Pointer (non-secure)
 353:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Stack Pointer (SP) when in secure state.
 354:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               SP Register value
 355:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 356:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_SP_NS(void)
 357:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 358:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 359:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 360:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, sp_ns" : "=r" (result) );
 361:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 362:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 363:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 364:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 365:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 366:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Stack Pointer (non-secure)
 367:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Stack Pointer (SP) when in secure state.
 368:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    topOfStack  Stack Pointer value to set
 369:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 370:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_SP_NS(uint32_t topOfStack)
 371:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 372:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR sp_ns, %0" : : "r" (topOfStack) : );
 373:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 374:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 375:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 376:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 377:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 378:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Priority Mask
 379:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current state of the priority mask bit from the Priority Mask Register.
 380:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Priority Mask value
 381:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 382:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_PRIMASK(void)
 383:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 384:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 385:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 386:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, primask" : "=r" (result) :: "memory");
 387:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 388:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 389:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 390:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 391:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 392:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 393:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Priority Mask (non-secure)
 394:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current state of the non-secure priority mask bit from the Priority Mask Reg
 395:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Priority Mask value
 396:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 397:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_PRIMASK_NS(void)
ARM GAS  /tmp/ccPRqU3T.s 			page 51


 398:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 399:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 400:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 401:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, primask_ns" : "=r" (result) :: "memory");
 402:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 403:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 404:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 405:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 406:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 407:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 408:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Priority Mask
 409:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Priority Mask Register.
 410:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    priMask  Priority Mask
 411:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 412:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_PRIMASK(uint32_t priMask)
 413:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 414:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR primask, %0" : : "r" (priMask) : "memory");
 415:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 416:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 417:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 418:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 419:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 420:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Priority Mask (non-secure)
 421:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Priority Mask Register when in secure state.
 422:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    priMask  Priority Mask
 423:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 424:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_PRIMASK_NS(uint32_t priMask)
 425:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 426:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR primask_ns, %0" : : "r" (priMask) : "memory");
 427:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 428:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 429:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 430:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 431:Drivers/CMSIS/Include/cmsis_gcc.h **** #if ((defined (__ARM_ARCH_7M__      ) && (__ARM_ARCH_7M__      == 1)) || \
 432:Drivers/CMSIS/Include/cmsis_gcc.h ****      (defined (__ARM_ARCH_7EM__     ) && (__ARM_ARCH_7EM__     == 1)) || \
 433:Drivers/CMSIS/Include/cmsis_gcc.h ****      (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1))    )
 434:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 435:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Enable FIQ
 436:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Enables FIQ interrupts by clearing the F-bit in the CPSR.
 437:Drivers/CMSIS/Include/cmsis_gcc.h ****            Can only be executed in Privileged modes.
 438:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 439:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __enable_fault_irq(void)
 440:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 441:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("cpsie f" : : : "memory");
 442:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 443:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 444:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 445:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 446:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Disable FIQ
 447:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Disables FIQ interrupts by setting the F-bit in the CPSR.
 448:Drivers/CMSIS/Include/cmsis_gcc.h ****            Can only be executed in Privileged modes.
 449:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 450:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __disable_fault_irq(void)
 451:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 452:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("cpsid f" : : : "memory");
 453:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 454:Drivers/CMSIS/Include/cmsis_gcc.h **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 52


 455:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 456:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 457:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Base Priority
 458:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Base Priority register.
 459:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Base Priority register value
 460:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 461:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_BASEPRI(void)
 462:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 463:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 464:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 465:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, basepri" : "=r" (result) );
 466:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 467:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 468:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 469:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 470:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 471:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 472:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Base Priority (non-secure)
 473:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Base Priority register when in secure state.
 474:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Base Priority register value
 475:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 476:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_BASEPRI_NS(void)
 477:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 478:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 479:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 480:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, basepri_ns" : "=r" (result) );
 481:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 482:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 483:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 484:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 485:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 486:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 487:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Base Priority
 488:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Base Priority register.
 489:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    basePri  Base Priority value to set
 490:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 491:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_BASEPRI(uint32_t basePri)
 492:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 493:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR basepri, %0" : : "r" (basePri) : "memory");
 494:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 495:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 496:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 497:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 498:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 499:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Base Priority (non-secure)
 500:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Base Priority register when in secure state.
 501:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    basePri  Base Priority value to set
 502:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 503:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_BASEPRI_NS(uint32_t basePri)
 504:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 505:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR basepri_ns, %0" : : "r" (basePri) : "memory");
 506:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 507:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 508:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 509:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 510:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 511:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Base Priority with condition
ARM GAS  /tmp/ccPRqU3T.s 			page 53


 512:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Base Priority register only if BASEPRI masking is disable
 513:Drivers/CMSIS/Include/cmsis_gcc.h ****            or the new value increases the BASEPRI priority level.
 514:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    basePri  Base Priority value to set
 515:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 516:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_BASEPRI_MAX(uint32_t basePri)
 517:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 518:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR basepri_max, %0" : : "r" (basePri) : "memory");
 519:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 520:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 521:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 522:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 523:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Fault Mask
 524:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Fault Mask register.
 525:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Fault Mask register value
 526:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 527:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_FAULTMASK(void)
 528:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 529:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 530:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 531:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, faultmask" : "=r" (result) );
 532:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 533:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 534:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 535:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 536:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 537:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 538:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Fault Mask (non-secure)
 539:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Fault Mask register when in secure state.
 540:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Fault Mask register value
 541:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 542:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_FAULTMASK_NS(void)
 543:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 544:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 545:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 546:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, faultmask_ns" : "=r" (result) );
 547:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 548:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 549:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 550:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 551:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 552:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 553:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Fault Mask
 554:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Fault Mask register.
 555:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    faultMask  Fault Mask value to set
 556:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 557:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_FAULTMASK(uint32_t faultMask)
 558:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 559:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR faultmask, %0" : : "r" (faultMask) : "memory");
 560:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 561:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 562:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 563:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE ) && (__ARM_FEATURE_CMSE == 3))
 564:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 565:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Fault Mask (non-secure)
 566:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Fault Mask register when in secure state.
 567:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    faultMask  Fault Mask value to set
 568:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
ARM GAS  /tmp/ccPRqU3T.s 			page 54


 569:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_FAULTMASK_NS(uint32_t faultMask)
 570:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 571:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR faultmask_ns, %0" : : "r" (faultMask) : "memory");
 572:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 573:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 574:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 575:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif /* ((defined (__ARM_ARCH_7M__      ) && (__ARM_ARCH_7M__      == 1)) || \
 576:Drivers/CMSIS/Include/cmsis_gcc.h ****            (defined (__ARM_ARCH_7EM__     ) && (__ARM_ARCH_7EM__     == 1)) || \
 577:Drivers/CMSIS/Include/cmsis_gcc.h ****            (defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1))    ) */
 578:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 579:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 580:Drivers/CMSIS/Include/cmsis_gcc.h **** #if ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
 581:Drivers/CMSIS/Include/cmsis_gcc.h ****      (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1))    )
 582:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 583:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 584:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Process Stack Pointer Limit
 585:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 586:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence zero is returned always in non-secure
 587:Drivers/CMSIS/Include/cmsis_gcc.h ****   mode.
 588:Drivers/CMSIS/Include/cmsis_gcc.h ****   
 589:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Process Stack Pointer Limit (PSPLIM).
 590:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               PSPLIM Register value
 591:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 592:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_PSPLIM(void)
 593:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 594:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
 595:Drivers/CMSIS/Include/cmsis_gcc.h ****     (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
 596:Drivers/CMSIS/Include/cmsis_gcc.h ****     // without main extensions, the non-secure PSPLIM is RAZ/WI
 597:Drivers/CMSIS/Include/cmsis_gcc.h ****   return 0U;
 598:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 599:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 600:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, psplim"  : "=r" (result) );
 601:Drivers/CMSIS/Include/cmsis_gcc.h ****   return result;
 602:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 603:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 604:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 605:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE) && (__ARM_FEATURE_CMSE == 3))
 606:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 607:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Process Stack Pointer Limit (non-secure)
 608:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 609:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence zero is returned always.
 610:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 611:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Process Stack Pointer Limit (PSPLIM) when in
 612:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               PSPLIM Register value
 613:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 614:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_PSPLIM_NS(void)
 615:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 616:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
 617:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure PSPLIM is RAZ/WI
 618:Drivers/CMSIS/Include/cmsis_gcc.h ****   return 0U;
 619:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 620:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 621:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, psplim_ns"  : "=r" (result) );
 622:Drivers/CMSIS/Include/cmsis_gcc.h ****   return result;
 623:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 624:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 625:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
ARM GAS  /tmp/ccPRqU3T.s 			page 55


 626:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 627:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 628:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 629:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Process Stack Pointer Limit
 630:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 631:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence the write is silently ignored in non-secure
 632:Drivers/CMSIS/Include/cmsis_gcc.h ****   mode.
 633:Drivers/CMSIS/Include/cmsis_gcc.h ****   
 634:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Process Stack Pointer Limit (PSPLIM).
 635:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    ProcStackPtrLimit  Process Stack Pointer Limit value to set
 636:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 637:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_PSPLIM(uint32_t ProcStackPtrLimit)
 638:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 639:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
 640:Drivers/CMSIS/Include/cmsis_gcc.h ****     (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
 641:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure PSPLIM is RAZ/WI
 642:Drivers/CMSIS/Include/cmsis_gcc.h ****   (void)ProcStackPtrLimit;
 643:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 644:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR psplim, %0" : : "r" (ProcStackPtrLimit));
 645:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 646:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 647:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 648:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 649:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE  ) && (__ARM_FEATURE_CMSE   == 3))
 650:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 651:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Process Stack Pointer (non-secure)
 652:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 653:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence the write is silently ignored.
 654:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 655:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Process Stack Pointer Limit (PSPLIM) when in s
 656:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    ProcStackPtrLimit  Process Stack Pointer Limit value to set
 657:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 658:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_PSPLIM_NS(uint32_t ProcStackPtrLimit)
 659:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 660:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
 661:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure PSPLIM is RAZ/WI
 662:Drivers/CMSIS/Include/cmsis_gcc.h ****   (void)ProcStackPtrLimit;
 663:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 664:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR psplim_ns, %0\n" : : "r" (ProcStackPtrLimit));
 665:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 666:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 667:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 668:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 669:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 670:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 671:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Main Stack Pointer Limit
 672:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 673:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence zero is returned always in non-secure
 674:Drivers/CMSIS/Include/cmsis_gcc.h ****   mode.
 675:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 676:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Main Stack Pointer Limit (MSPLIM).
 677:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               MSPLIM Register value
 678:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 679:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_MSPLIM(void)
 680:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 681:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
 682:Drivers/CMSIS/Include/cmsis_gcc.h ****     (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
ARM GAS  /tmp/ccPRqU3T.s 			page 56


 683:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure MSPLIM is RAZ/WI
 684:Drivers/CMSIS/Include/cmsis_gcc.h ****   return 0U;
 685:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 686:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 687:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, msplim" : "=r" (result) );
 688:Drivers/CMSIS/Include/cmsis_gcc.h ****   return result;
 689:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 690:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 691:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 692:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 693:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE  ) && (__ARM_FEATURE_CMSE   == 3))
 694:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 695:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get Main Stack Pointer Limit (non-secure)
 696:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 697:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence zero is returned always.
 698:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 699:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the non-secure Main Stack Pointer Limit(MSPLIM) when in sec
 700:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               MSPLIM Register value
 701:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 702:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __TZ_get_MSPLIM_NS(void)
 703:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 704:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
 705:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure MSPLIM is RAZ/WI
 706:Drivers/CMSIS/Include/cmsis_gcc.h ****   return 0U;
 707:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 708:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 709:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MRS %0, msplim_ns" : "=r" (result) );
 710:Drivers/CMSIS/Include/cmsis_gcc.h ****   return result;
 711:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 712:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 713:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 714:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 715:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 716:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 717:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Main Stack Pointer Limit
 718:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 719:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence the write is silently ignored in non-secure
 720:Drivers/CMSIS/Include/cmsis_gcc.h ****   mode.
 721:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 722:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Main Stack Pointer Limit (MSPLIM).
 723:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    MainStackPtrLimit  Main Stack Pointer Limit value to set
 724:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 725:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_MSPLIM(uint32_t MainStackPtrLimit)
 726:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 727:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) && \
 728:Drivers/CMSIS/Include/cmsis_gcc.h ****     (!defined (__ARM_FEATURE_CMSE) || (__ARM_FEATURE_CMSE < 3)))
 729:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure MSPLIM is RAZ/WI
 730:Drivers/CMSIS/Include/cmsis_gcc.h ****   (void)MainStackPtrLimit;
 731:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 732:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR msplim, %0" : : "r" (MainStackPtrLimit));
 733:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 734:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 735:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 736:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 737:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (defined (__ARM_FEATURE_CMSE  ) && (__ARM_FEATURE_CMSE   == 3))
 738:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 739:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set Main Stack Pointer Limit (non-secure)
ARM GAS  /tmp/ccPRqU3T.s 			page 57


 740:Drivers/CMSIS/Include/cmsis_gcc.h ****   Devices without ARMv8-M Main Extensions (i.e. Cortex-M23) lack the non-secure
 741:Drivers/CMSIS/Include/cmsis_gcc.h ****   Stack Pointer Limit register hence the write is silently ignored.
 742:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 743:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the non-secure Main Stack Pointer Limit (MSPLIM) when in secu
 744:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    MainStackPtrLimit  Main Stack Pointer value to set
 745:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 746:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __TZ_set_MSPLIM_NS(uint32_t MainStackPtrLimit)
 747:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 748:Drivers/CMSIS/Include/cmsis_gcc.h **** #if (!(defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)))
 749:Drivers/CMSIS/Include/cmsis_gcc.h ****   // without main extensions, the non-secure MSPLIM is RAZ/WI
 750:Drivers/CMSIS/Include/cmsis_gcc.h ****   (void)MainStackPtrLimit;
 751:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 752:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("MSR msplim_ns, %0" : : "r" (MainStackPtrLimit));
 753:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 754:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 755:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 756:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 757:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif /* ((defined (__ARM_ARCH_8M_MAIN__ ) && (__ARM_ARCH_8M_MAIN__ == 1)) || \
 758:Drivers/CMSIS/Include/cmsis_gcc.h ****            (defined (__ARM_ARCH_8M_BASE__ ) && (__ARM_ARCH_8M_BASE__ == 1))    ) */
 759:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 760:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 761:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 762:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Get FPSCR
 763:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Returns the current value of the Floating Point Status/Control register.
 764:Drivers/CMSIS/Include/cmsis_gcc.h ****   \return               Floating Point Status/Control register value
 765:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 766:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE uint32_t __get_FPSCR(void)
 767:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 768:Drivers/CMSIS/Include/cmsis_gcc.h **** #if ((defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)) && \
 769:Drivers/CMSIS/Include/cmsis_gcc.h ****      (defined (__FPU_USED   ) && (__FPU_USED    == 1U))     )
 770:Drivers/CMSIS/Include/cmsis_gcc.h **** #if __has_builtin(__builtin_arm_get_fpscr) 
 771:Drivers/CMSIS/Include/cmsis_gcc.h **** // Re-enable using built-in when GCC has been fixed
 772:Drivers/CMSIS/Include/cmsis_gcc.h **** // || (__GNUC__ > 7) || (__GNUC__ == 7 && __GNUC_MINOR__ >= 2)
 773:Drivers/CMSIS/Include/cmsis_gcc.h ****   /* see https://gcc.gnu.org/ml/gcc-patches/2017-04/msg00443.html */
 774:Drivers/CMSIS/Include/cmsis_gcc.h ****   return __builtin_arm_get_fpscr();
 775:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 776:Drivers/CMSIS/Include/cmsis_gcc.h ****   uint32_t result;
 777:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 778:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("VMRS %0, fpscr" : "=r" (result) );
 779:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(result);
 780:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 781:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 782:Drivers/CMSIS/Include/cmsis_gcc.h ****   return(0U);
 783:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 784:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 785:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 786:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 787:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 788:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Set FPSCR
 789:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Assigns the given value to the Floating Point Status/Control register.
 790:Drivers/CMSIS/Include/cmsis_gcc.h ****   \param [in]    fpscr  Floating Point Status/Control value to set
 791:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 792:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __set_FPSCR(uint32_t fpscr)
 793:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 794:Drivers/CMSIS/Include/cmsis_gcc.h **** #if ((defined (__FPU_PRESENT) && (__FPU_PRESENT == 1U)) && \
 795:Drivers/CMSIS/Include/cmsis_gcc.h ****      (defined (__FPU_USED   ) && (__FPU_USED    == 1U))     )
 796:Drivers/CMSIS/Include/cmsis_gcc.h **** #if __has_builtin(__builtin_arm_set_fpscr)
ARM GAS  /tmp/ccPRqU3T.s 			page 58


 797:Drivers/CMSIS/Include/cmsis_gcc.h **** // Re-enable using built-in when GCC has been fixed
 798:Drivers/CMSIS/Include/cmsis_gcc.h **** // || (__GNUC__ > 7) || (__GNUC__ == 7 && __GNUC_MINOR__ >= 2)
 799:Drivers/CMSIS/Include/cmsis_gcc.h ****   /* see https://gcc.gnu.org/ml/gcc-patches/2017-04/msg00443.html */
 800:Drivers/CMSIS/Include/cmsis_gcc.h ****   __builtin_arm_set_fpscr(fpscr);
 801:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 802:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("VMSR fpscr, %0" : : "r" (fpscr) : "vfpcc", "memory");
 803:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 804:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 805:Drivers/CMSIS/Include/cmsis_gcc.h ****   (void)fpscr;
 806:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 807:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 808:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 809:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 810:Drivers/CMSIS/Include/cmsis_gcc.h **** /*@} end of CMSIS_Core_RegAccFunctions */
 811:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 812:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 813:Drivers/CMSIS/Include/cmsis_gcc.h **** /* ##########################  Core Instruction Access  ######################### */
 814:Drivers/CMSIS/Include/cmsis_gcc.h **** /** \defgroup CMSIS_Core_InstructionInterface CMSIS Core Instruction Interface
 815:Drivers/CMSIS/Include/cmsis_gcc.h ****   Access to dedicated instructions
 816:Drivers/CMSIS/Include/cmsis_gcc.h ****   @{
 817:Drivers/CMSIS/Include/cmsis_gcc.h **** */
 818:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 819:Drivers/CMSIS/Include/cmsis_gcc.h **** /* Define macros for porting to both thumb1 and thumb2.
 820:Drivers/CMSIS/Include/cmsis_gcc.h ****  * For thumb1, use low register (r0-r7), specified by constraint "l"
 821:Drivers/CMSIS/Include/cmsis_gcc.h ****  * Otherwise, use general registers, specified by constraint "r" */
 822:Drivers/CMSIS/Include/cmsis_gcc.h **** #if defined (__thumb__) && !defined (__thumb2__)
 823:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_OUT_REG(r) "=l" (r)
 824:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_RW_REG(r) "+l" (r)
 825:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_USE_REG(r) "l" (r)
 826:Drivers/CMSIS/Include/cmsis_gcc.h **** #else
 827:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_OUT_REG(r) "=r" (r)
 828:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_RW_REG(r) "+r" (r)
 829:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __CMSIS_GCC_USE_REG(r) "r" (r)
 830:Drivers/CMSIS/Include/cmsis_gcc.h **** #endif
 831:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 832:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 833:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   No Operation
 834:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details No Operation does nothing. This instruction can be used for code alignment purposes.
 835:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 836:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __NOP()                             __ASM volatile ("nop")
 837:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 838:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 839:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Wait For Interrupt
 840:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Wait For Interrupt is a hint instruction that suspends execution until one of a number o
 841:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 842:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __WFI()                             __ASM volatile ("wfi")
 843:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 844:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 845:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 846:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Wait For Event
 847:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Wait For Event is a hint instruction that permits the processor to enter
 848:Drivers/CMSIS/Include/cmsis_gcc.h ****            a low-power state until one of a number of events occurs.
 849:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 850:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __WFE()                             __ASM volatile ("wfe")
 851:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 852:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 853:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
ARM GAS  /tmp/ccPRqU3T.s 			page 59


 854:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Send Event
 855:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Send Event is a hint instruction. It causes an event to be signaled to the CPU.
 856:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 857:Drivers/CMSIS/Include/cmsis_gcc.h **** #define __SEV()                             __ASM volatile ("sev")
 858:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 859:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 860:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 861:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Instruction Synchronization Barrier
 862:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Instruction Synchronization Barrier flushes the pipeline in the processor,
 863:Drivers/CMSIS/Include/cmsis_gcc.h ****            so that all instructions following the ISB are fetched from cache or memory,
 864:Drivers/CMSIS/Include/cmsis_gcc.h ****            after the instruction has been completed.
 865:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 866:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __ISB(void)
 867:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 868:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("isb 0xF":::"memory");
 869:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 870:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 871:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 872:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 873:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Data Synchronization Barrier
 874:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Acts as a special kind of Data Memory Barrier.
 875:Drivers/CMSIS/Include/cmsis_gcc.h ****            It completes when all explicit memory accesses before this instruction complete.
 876:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 877:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __DSB(void)
 336              		.loc 3 877 27 view .LVU98
 337              	.LBB67:
 878:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 879:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("dsb 0xF":::"memory");
 338              		.loc 3 879 3 view .LVU99
 339              		.syntax unified
 340              	@ 879 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 341 0016 BFF34F8F 		dsb 0xF
 342              	@ 0 "" 2
 343              		.thumb
 344              		.syntax unified
 345              	.LBE67:
 346              	.LBE66:
1730:Drivers/CMSIS/Include/core_cm4.h ****   }
 347              		.loc 2 1730 5 view .LVU100
 348              	.LBB68:
 349              	.LBI68:
 866:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 350              		.loc 3 866 27 view .LVU101
 351              	.LBB69:
 868:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 352              		.loc 3 868 3 view .LVU102
 353              		.syntax unified
 354              	@ 868 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 355 001a BFF36F8F 		isb 0xF
 356              	@ 0 "" 2
 357              	.LVL32:
 358              		.thumb
 359              		.syntax unified
 360              	.L16:
 868:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 361              		.loc 3 868 3 is_stmt 0 view .LVU103
 362              	.LBE69:
ARM GAS  /tmp/ccPRqU3T.s 			page 60


 363              	.LBE68:
 364              	.LBE65:
 365              	.LBE64:
 210:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 366              		.loc 1 210 1 view .LVU104
 367 001e 7047     		bx	lr
 368              	.L19:
 369              		.align	2
 370              	.L18:
 371 0020 00E100E0 		.word	-536813312
 372              		.cfi_endproc
 373              	.LFE133:
 375              		.section	.text.HAL_NVIC_SystemReset,"ax",%progbits
 376              		.align	1
 377              		.global	HAL_NVIC_SystemReset
 378              		.syntax unified
 379              		.thumb
 380              		.thumb_func
 382              	HAL_NVIC_SystemReset:
 383              	.LFB134:
 211:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 212:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 213:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Initiates a system reset request to reset the MCU.
 214:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 215:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 216:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_SystemReset(void)
 217:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 384              		.loc 1 217 1 is_stmt 1 view -0
 385              		.cfi_startproc
 386              		@ Volatile: function does not return.
 387              		@ args = 0, pretend = 0, frame = 0
 388              		@ frame_needed = 0, uses_anonymous_args = 0
 389              		@ link register save eliminated.
 218:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* System Reset */
 219:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_SystemReset();
 390              		.loc 1 219 3 view .LVU106
 391              	.LBB76:
 392              	.LBI76:
1875:Drivers/CMSIS/Include/core_cm4.h ****          );
1876:Drivers/CMSIS/Include/core_cm4.h **** }
1877:Drivers/CMSIS/Include/core_cm4.h **** 
1878:Drivers/CMSIS/Include/core_cm4.h **** 
1879:Drivers/CMSIS/Include/core_cm4.h **** /**
1880:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Decode Priority
1881:Drivers/CMSIS/Include/core_cm4.h ****   \details Decodes an interrupt priority value with a given priority group to
1882:Drivers/CMSIS/Include/core_cm4.h ****            preemptive priority value and subpriority value.
1883:Drivers/CMSIS/Include/core_cm4.h ****            In case of a conflict between priority grouping and available
1884:Drivers/CMSIS/Include/core_cm4.h ****            priority bits (__NVIC_PRIO_BITS) the smallest possible priority group is set.
1885:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]         Priority   Priority value, which can be retrieved with the function \ref NVIC
1886:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]     PriorityGroup  Used priority group.
1887:Drivers/CMSIS/Include/core_cm4.h ****   \param [out] pPreemptPriority  Preemptive priority value (starting from 0).
1888:Drivers/CMSIS/Include/core_cm4.h ****   \param [out]     pSubPriority  Subpriority value (starting from 0).
1889:Drivers/CMSIS/Include/core_cm4.h ****  */
1890:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void NVIC_DecodePriority (uint32_t Priority, uint32_t PriorityGroup, uint32_t* cons
1891:Drivers/CMSIS/Include/core_cm4.h **** {
1892:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PriorityGroupTmp = (PriorityGroup & (uint32_t)0x07UL);   /* only values 0..7 are used   
1893:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PreemptPriorityBits;
ARM GAS  /tmp/ccPRqU3T.s 			page 61


1894:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t SubPriorityBits;
1895:Drivers/CMSIS/Include/core_cm4.h **** 
1896:Drivers/CMSIS/Include/core_cm4.h ****   PreemptPriorityBits = ((7UL - PriorityGroupTmp) > (uint32_t)(__NVIC_PRIO_BITS)) ? (uint32_t)(__NV
1897:Drivers/CMSIS/Include/core_cm4.h ****   SubPriorityBits     = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint
1898:Drivers/CMSIS/Include/core_cm4.h **** 
1899:Drivers/CMSIS/Include/core_cm4.h ****   *pPreemptPriority = (Priority >> SubPriorityBits) & (uint32_t)((1UL << (PreemptPriorityBits)) - 1
1900:Drivers/CMSIS/Include/core_cm4.h ****   *pSubPriority     = (Priority                   ) & (uint32_t)((1UL << (SubPriorityBits    )) - 1
1901:Drivers/CMSIS/Include/core_cm4.h **** }
1902:Drivers/CMSIS/Include/core_cm4.h **** 
1903:Drivers/CMSIS/Include/core_cm4.h **** 
1904:Drivers/CMSIS/Include/core_cm4.h **** /**
1905:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Set Interrupt Vector
1906:Drivers/CMSIS/Include/core_cm4.h ****   \details Sets an interrupt vector in SRAM based interrupt vector table.
1907:Drivers/CMSIS/Include/core_cm4.h ****            The interrupt number can be positive to specify a device specific interrupt,
1908:Drivers/CMSIS/Include/core_cm4.h ****            or negative to specify a processor exception.
1909:Drivers/CMSIS/Include/core_cm4.h ****            VTOR must been relocated to SRAM before.
1910:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]   IRQn      Interrupt number
1911:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]   vector    Address of interrupt handler function
1912:Drivers/CMSIS/Include/core_cm4.h ****  */
1913:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE void __NVIC_SetVector(IRQn_Type IRQn, uint32_t vector)
1914:Drivers/CMSIS/Include/core_cm4.h **** {
1915:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t *vectors = (uint32_t *)SCB->VTOR;
1916:Drivers/CMSIS/Include/core_cm4.h ****   vectors[(int32_t)IRQn + NVIC_USER_IRQ_OFFSET] = vector;
1917:Drivers/CMSIS/Include/core_cm4.h **** }
1918:Drivers/CMSIS/Include/core_cm4.h **** 
1919:Drivers/CMSIS/Include/core_cm4.h **** 
1920:Drivers/CMSIS/Include/core_cm4.h **** /**
1921:Drivers/CMSIS/Include/core_cm4.h ****   \brief   Get Interrupt Vector
1922:Drivers/CMSIS/Include/core_cm4.h ****   \details Reads an interrupt vector from interrupt vector table.
1923:Drivers/CMSIS/Include/core_cm4.h ****            The interrupt number can be positive to specify a device specific interrupt,
1924:Drivers/CMSIS/Include/core_cm4.h ****            or negative to specify a processor exception.
1925:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]   IRQn      Interrupt number.
1926:Drivers/CMSIS/Include/core_cm4.h ****   \return                 Address of interrupt handler function
1927:Drivers/CMSIS/Include/core_cm4.h ****  */
1928:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t __NVIC_GetVector(IRQn_Type IRQn)
1929:Drivers/CMSIS/Include/core_cm4.h **** {
1930:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t *vectors = (uint32_t *)SCB->VTOR;
1931:Drivers/CMSIS/Include/core_cm4.h ****   return vectors[(int32_t)IRQn + NVIC_USER_IRQ_OFFSET];
1932:Drivers/CMSIS/Include/core_cm4.h **** }
1933:Drivers/CMSIS/Include/core_cm4.h **** 
1934:Drivers/CMSIS/Include/core_cm4.h **** 
1935:Drivers/CMSIS/Include/core_cm4.h **** /**
1936:Drivers/CMSIS/Include/core_cm4.h ****   \brief   System Reset
1937:Drivers/CMSIS/Include/core_cm4.h ****   \details Initiates a system reset request to reset the MCU.
1938:Drivers/CMSIS/Include/core_cm4.h ****  */
1939:Drivers/CMSIS/Include/core_cm4.h **** __NO_RETURN __STATIC_INLINE void __NVIC_SystemReset(void)
 393              		.loc 2 1939 34 view .LVU107
 394              	.LBB77:
1940:Drivers/CMSIS/Include/core_cm4.h **** {
1941:Drivers/CMSIS/Include/core_cm4.h ****   __DSB();                                                          /* Ensure all outstanding memor
 395              		.loc 2 1941 3 view .LVU108
 396              	.LBB78:
 397              	.LBI78:
 877:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 398              		.loc 3 877 27 view .LVU109
 399              	.LBB79:
 400              		.loc 3 879 3 view .LVU110
ARM GAS  /tmp/ccPRqU3T.s 			page 62


 401              		.syntax unified
 402              	@ 879 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 403 0000 BFF34F8F 		dsb 0xF
 404              	@ 0 "" 2
 405              		.thumb
 406              		.syntax unified
 407              	.LBE79:
 408              	.LBE78:
1942:Drivers/CMSIS/Include/core_cm4.h ****                                                                        buffered write are completed
1943:Drivers/CMSIS/Include/core_cm4.h ****   SCB->AIRCR  = (uint32_t)((0x5FAUL << SCB_AIRCR_VECTKEY_Pos)    |
 409              		.loc 2 1943 3 view .LVU111
1944:Drivers/CMSIS/Include/core_cm4.h ****                            (SCB->AIRCR & SCB_AIRCR_PRIGROUP_Msk) |
 410              		.loc 2 1944 32 is_stmt 0 view .LVU112
 411 0004 0549     		ldr	r1, .L22
 412 0006 CA68     		ldr	r2, [r1, #12]
 413              		.loc 2 1944 40 view .LVU113
 414 0008 02F4E062 		and	r2, r2, #1792
1943:Drivers/CMSIS/Include/core_cm4.h ****                            (SCB->AIRCR & SCB_AIRCR_PRIGROUP_Msk) |
 415              		.loc 2 1943 17 view .LVU114
 416 000c 044B     		ldr	r3, .L22+4
 417 000e 1343     		orrs	r3, r3, r2
1943:Drivers/CMSIS/Include/core_cm4.h ****                            (SCB->AIRCR & SCB_AIRCR_PRIGROUP_Msk) |
 418              		.loc 2 1943 15 view .LVU115
 419 0010 CB60     		str	r3, [r1, #12]
1945:Drivers/CMSIS/Include/core_cm4.h ****                             SCB_AIRCR_SYSRESETREQ_Msk    );         /* Keep priority group unchange
1946:Drivers/CMSIS/Include/core_cm4.h ****   __DSB();                                                          /* Ensure completion of memory 
 420              		.loc 2 1946 3 is_stmt 1 view .LVU116
 421              	.LBB80:
 422              	.LBI80:
 877:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 423              		.loc 3 877 27 view .LVU117
 424              	.LBB81:
 425              		.loc 3 879 3 view .LVU118
 426              		.syntax unified
 427              	@ 879 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 428 0012 BFF34F8F 		dsb 0xF
 429              	@ 0 "" 2
 430              		.thumb
 431              		.syntax unified
 432              	.L21:
 433              	.LBE81:
 434              	.LBE80:
1947:Drivers/CMSIS/Include/core_cm4.h **** 
1948:Drivers/CMSIS/Include/core_cm4.h ****   for(;;)                                                           /* wait until reset */
 435              		.loc 2 1948 3 view .LVU119
1949:Drivers/CMSIS/Include/core_cm4.h ****   {
1950:Drivers/CMSIS/Include/core_cm4.h ****     __NOP();
 436              		.loc 2 1950 5 view .LVU120
 437              		.syntax unified
 438              	@ 1950 "Drivers/CMSIS/Include/core_cm4.h" 1
 439 0016 00BF     		nop
 440              	@ 0 "" 2
1948:Drivers/CMSIS/Include/core_cm4.h ****   {
 441              		.loc 2 1948 8 view .LVU121
 442              		.thumb
 443              		.syntax unified
 444 0018 FDE7     		b	.L21
ARM GAS  /tmp/ccPRqU3T.s 			page 63


 445              	.L23:
 446 001a 00BF     		.align	2
 447              	.L22:
 448 001c 00ED00E0 		.word	-536810240
 449 0020 0400FA05 		.word	100270084
 450              	.LBE77:
 451              	.LBE76:
 452              		.cfi_endproc
 453              	.LFE134:
 455              		.section	.text.HAL_SYSTICK_Config,"ax",%progbits
 456              		.align	1
 457              		.global	HAL_SYSTICK_Config
 458              		.syntax unified
 459              		.thumb
 460              		.thumb_func
 462              	HAL_SYSTICK_Config:
 463              	.LVL33:
 464              	.LFB135:
 220:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 221:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 222:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 223:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Initializes the System Timer and its interrupt, and starts the System Tick Timer.
 224:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         Counter is in free running mode to generate periodic interrupts.
 225:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  TicksNumb Specifies the ticks Number of ticks between two interrupts.
 226:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval status:  - 0  Function succeeded.
 227:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                  - 1  Function failed.
 228:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 229:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** uint32_t HAL_SYSTICK_Config(uint32_t TicksNumb)
 230:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 465              		.loc 1 230 1 view -0
 466              		.cfi_startproc
 467              		@ args = 0, pretend = 0, frame = 0
 468              		@ frame_needed = 0, uses_anonymous_args = 0
 469              		@ link register save eliminated.
 231:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    return SysTick_Config(TicksNumb);
 470              		.loc 1 231 4 view .LVU123
 471              	.LBB82:
 472              	.LBI82:
1951:Drivers/CMSIS/Include/core_cm4.h ****   }
1952:Drivers/CMSIS/Include/core_cm4.h **** }
1953:Drivers/CMSIS/Include/core_cm4.h **** 
1954:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of CMSIS_Core_NVICFunctions */
1955:Drivers/CMSIS/Include/core_cm4.h **** 
1956:Drivers/CMSIS/Include/core_cm4.h **** /* ##########################  MPU functions  #################################### */
1957:Drivers/CMSIS/Include/core_cm4.h **** 
1958:Drivers/CMSIS/Include/core_cm4.h **** #if defined (__MPU_PRESENT) && (__MPU_PRESENT == 1U)
1959:Drivers/CMSIS/Include/core_cm4.h **** 
1960:Drivers/CMSIS/Include/core_cm4.h **** #include "mpu_armv7.h"
1961:Drivers/CMSIS/Include/core_cm4.h **** 
1962:Drivers/CMSIS/Include/core_cm4.h **** #endif
1963:Drivers/CMSIS/Include/core_cm4.h **** 
1964:Drivers/CMSIS/Include/core_cm4.h **** 
1965:Drivers/CMSIS/Include/core_cm4.h **** /* ##########################  FPU functions  #################################### */
1966:Drivers/CMSIS/Include/core_cm4.h **** /**
1967:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_Core_FunctionInterface
1968:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_Core_FpuFunctions FPU Functions
1969:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Function that provides FPU type.
ARM GAS  /tmp/ccPRqU3T.s 			page 64


1970:Drivers/CMSIS/Include/core_cm4.h ****   @{
1971:Drivers/CMSIS/Include/core_cm4.h ****  */
1972:Drivers/CMSIS/Include/core_cm4.h **** 
1973:Drivers/CMSIS/Include/core_cm4.h **** /**
1974:Drivers/CMSIS/Include/core_cm4.h ****   \brief   get FPU type
1975:Drivers/CMSIS/Include/core_cm4.h ****   \details returns the FPU type
1976:Drivers/CMSIS/Include/core_cm4.h ****   \returns
1977:Drivers/CMSIS/Include/core_cm4.h ****    - \b  0: No FPU
1978:Drivers/CMSIS/Include/core_cm4.h ****    - \b  1: Single precision FPU
1979:Drivers/CMSIS/Include/core_cm4.h ****    - \b  2: Double + Single precision FPU
1980:Drivers/CMSIS/Include/core_cm4.h ****  */
1981:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t SCB_GetFPUType(void)
1982:Drivers/CMSIS/Include/core_cm4.h **** {
1983:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t mvfr0;
1984:Drivers/CMSIS/Include/core_cm4.h **** 
1985:Drivers/CMSIS/Include/core_cm4.h ****   mvfr0 = FPU->MVFR0;
1986:Drivers/CMSIS/Include/core_cm4.h ****   if      ((mvfr0 & (FPU_MVFR0_Single_precision_Msk | FPU_MVFR0_Double_precision_Msk)) == 0x020U)
1987:Drivers/CMSIS/Include/core_cm4.h ****   {
1988:Drivers/CMSIS/Include/core_cm4.h ****     return 1U;           /* Single precision FPU */
1989:Drivers/CMSIS/Include/core_cm4.h ****   }
1990:Drivers/CMSIS/Include/core_cm4.h ****   else
1991:Drivers/CMSIS/Include/core_cm4.h ****   {
1992:Drivers/CMSIS/Include/core_cm4.h ****     return 0U;           /* No FPU */
1993:Drivers/CMSIS/Include/core_cm4.h ****   }
1994:Drivers/CMSIS/Include/core_cm4.h **** }
1995:Drivers/CMSIS/Include/core_cm4.h **** 
1996:Drivers/CMSIS/Include/core_cm4.h **** 
1997:Drivers/CMSIS/Include/core_cm4.h **** /*@} end of CMSIS_Core_FpuFunctions */
1998:Drivers/CMSIS/Include/core_cm4.h **** 
1999:Drivers/CMSIS/Include/core_cm4.h **** 
2000:Drivers/CMSIS/Include/core_cm4.h **** 
2001:Drivers/CMSIS/Include/core_cm4.h **** /* ##################################    SysTick function  ########################################
2002:Drivers/CMSIS/Include/core_cm4.h **** /**
2003:Drivers/CMSIS/Include/core_cm4.h ****   \ingroup  CMSIS_Core_FunctionInterface
2004:Drivers/CMSIS/Include/core_cm4.h ****   \defgroup CMSIS_Core_SysTickFunctions SysTick Functions
2005:Drivers/CMSIS/Include/core_cm4.h ****   \brief    Functions that configure the System.
2006:Drivers/CMSIS/Include/core_cm4.h ****   @{
2007:Drivers/CMSIS/Include/core_cm4.h ****  */
2008:Drivers/CMSIS/Include/core_cm4.h **** 
2009:Drivers/CMSIS/Include/core_cm4.h **** #if defined (__Vendor_SysTickConfig) && (__Vendor_SysTickConfig == 0U)
2010:Drivers/CMSIS/Include/core_cm4.h **** 
2011:Drivers/CMSIS/Include/core_cm4.h **** /**
2012:Drivers/CMSIS/Include/core_cm4.h ****   \brief   System Tick Configuration
2013:Drivers/CMSIS/Include/core_cm4.h ****   \details Initializes the System Timer and its interrupt, and starts the System Tick Timer.
2014:Drivers/CMSIS/Include/core_cm4.h ****            Counter is in free running mode to generate periodic interrupts.
2015:Drivers/CMSIS/Include/core_cm4.h ****   \param [in]  ticks  Number of ticks between two interrupts.
2016:Drivers/CMSIS/Include/core_cm4.h ****   \return          0  Function succeeded.
2017:Drivers/CMSIS/Include/core_cm4.h ****   \return          1  Function failed.
2018:Drivers/CMSIS/Include/core_cm4.h ****   \note    When the variable <b>__Vendor_SysTickConfig</b> is set to 1, then the
2019:Drivers/CMSIS/Include/core_cm4.h ****            function <b>SysTick_Config</b> is not included. In this case, the file <b><i>device</i>.
2020:Drivers/CMSIS/Include/core_cm4.h ****            must contain a vendor-specific implementation of this function.
2021:Drivers/CMSIS/Include/core_cm4.h ****  */
2022:Drivers/CMSIS/Include/core_cm4.h **** __STATIC_INLINE uint32_t SysTick_Config(uint32_t ticks)
 473              		.loc 2 2022 26 view .LVU124
 474              	.LBB83:
2023:Drivers/CMSIS/Include/core_cm4.h **** {
2024:Drivers/CMSIS/Include/core_cm4.h ****   if ((ticks - 1UL) > SysTick_LOAD_RELOAD_Msk)
ARM GAS  /tmp/ccPRqU3T.s 			page 65


 475              		.loc 2 2024 3 view .LVU125
 476              		.loc 2 2024 14 is_stmt 0 view .LVU126
 477 0000 0138     		subs	r0, r0, #1
 478              	.LVL34:
 479              		.loc 2 2024 6 view .LVU127
 480 0002 B0F1807F 		cmp	r0, #16777216
 481 0006 0BD2     		bcs	.L26
2025:Drivers/CMSIS/Include/core_cm4.h ****   {
2026:Drivers/CMSIS/Include/core_cm4.h ****     return (1UL);                                                   /* Reload value impossible */
2027:Drivers/CMSIS/Include/core_cm4.h ****   }
2028:Drivers/CMSIS/Include/core_cm4.h **** 
2029:Drivers/CMSIS/Include/core_cm4.h ****   SysTick->LOAD  = (uint32_t)(ticks - 1UL);                         /* set reload register */
 482              		.loc 2 2029 3 is_stmt 1 view .LVU128
 483              		.loc 2 2029 18 is_stmt 0 view .LVU129
 484 0008 4FF0E023 		mov	r3, #-536813568
 485 000c 5861     		str	r0, [r3, #20]
2030:Drivers/CMSIS/Include/core_cm4.h ****   NVIC_SetPriority (SysTick_IRQn, (1UL << __NVIC_PRIO_BITS) - 1UL); /* set Priority for Systick Int
 486              		.loc 2 2030 3 is_stmt 1 view .LVU130
 487              	.LVL35:
 488              	.LBB84:
 489              	.LBI84:
1816:Drivers/CMSIS/Include/core_cm4.h **** {
 490              		.loc 2 1816 22 view .LVU131
 491              	.LBB85:
1818:Drivers/CMSIS/Include/core_cm4.h ****   {
 492              		.loc 2 1818 3 view .LVU132
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 493              		.loc 2 1824 5 view .LVU133
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 494              		.loc 2 1824 46 is_stmt 0 view .LVU134
 495 000e 054A     		ldr	r2, .L27
 496 0010 F021     		movs	r1, #240
 497 0012 82F82310 		strb	r1, [r2, #35]
 498              	.LVL36:
1824:Drivers/CMSIS/Include/core_cm4.h ****   }
 499              		.loc 2 1824 46 view .LVU135
 500              	.LBE85:
 501              	.LBE84:
2031:Drivers/CMSIS/Include/core_cm4.h ****   SysTick->VAL   = 0UL;                                             /* Load the SysTick Counter Val
 502              		.loc 2 2031 3 is_stmt 1 view .LVU136
 503              		.loc 2 2031 18 is_stmt 0 view .LVU137
 504 0016 0020     		movs	r0, #0
 505              	.LVL37:
 506              		.loc 2 2031 18 view .LVU138
 507 0018 9861     		str	r0, [r3, #24]
2032:Drivers/CMSIS/Include/core_cm4.h ****   SysTick->CTRL  = SysTick_CTRL_CLKSOURCE_Msk |
 508              		.loc 2 2032 3 is_stmt 1 view .LVU139
 509              		.loc 2 2032 18 is_stmt 0 view .LVU140
 510 001a 0722     		movs	r2, #7
 511 001c 1A61     		str	r2, [r3, #16]
2033:Drivers/CMSIS/Include/core_cm4.h ****                    SysTick_CTRL_TICKINT_Msk   |
2034:Drivers/CMSIS/Include/core_cm4.h ****                    SysTick_CTRL_ENABLE_Msk;                         /* Enable SysTick IRQ and SysTi
2035:Drivers/CMSIS/Include/core_cm4.h ****   return (0UL);                                                     /* Function successful */
 512              		.loc 2 2035 3 is_stmt 1 view .LVU141
 513              		.loc 2 2035 10 is_stmt 0 view .LVU142
 514 001e 7047     		bx	lr
 515              	.L26:
ARM GAS  /tmp/ccPRqU3T.s 			page 66


2026:Drivers/CMSIS/Include/core_cm4.h ****   }
 516              		.loc 2 2026 12 view .LVU143
 517 0020 0120     		movs	r0, #1
 518              	.LVL38:
2026:Drivers/CMSIS/Include/core_cm4.h ****   }
 519              		.loc 2 2026 12 view .LVU144
 520              	.LBE83:
 521              	.LBE82:
 232:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 522              		.loc 1 232 1 view .LVU145
 523 0022 7047     		bx	lr
 524              	.L28:
 525              		.align	2
 526              	.L27:
 527 0024 00ED00E0 		.word	-536810240
 528              		.cfi_endproc
 529              	.LFE135:
 531              		.section	.text.HAL_MPU_Disable,"ax",%progbits
 532              		.align	1
 533              		.global	HAL_MPU_Disable
 534              		.syntax unified
 535              		.thumb
 536              		.thumb_func
 538              	HAL_MPU_Disable:
 539              	.LFB136:
 233:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 234:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @}
 235:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 236:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 237:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /** @defgroup CORTEX_Exported_Functions_Group2 Peripheral Control functions
 238:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  *  @brief   Cortex control functions 
 239:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  *
 240:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** @verbatim   
 241:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ==============================================================================
 242:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                       ##### Peripheral Control functions #####
 243:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   ==============================================================================  
 244:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     [..]
 245:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****       This subsection provides a set of functions allowing to control the CORTEX
 246:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****       (NVIC, SYSTICK, MPU) functionalities. 
 247:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  
 248:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****       
 249:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** @endverbatim
 250:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @{
 251:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 252:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 253:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** #if (__MPU_PRESENT == 1U)
 254:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 255:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Disables the MPU
 256:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 257:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 258:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_MPU_Disable(void)
 259:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 540              		.loc 1 259 1 is_stmt 1 view -0
 541              		.cfi_startproc
 542              		@ args = 0, pretend = 0, frame = 0
 543              		@ frame_needed = 0, uses_anonymous_args = 0
 544              		@ link register save eliminated.
ARM GAS  /tmp/ccPRqU3T.s 			page 67


 260:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Make sure outstanding transfers are done */
 261:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   __DMB();
 545              		.loc 1 261 3 view .LVU147
 546              	.LBB86:
 547              	.LBI86:
 880:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 881:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 882:Drivers/CMSIS/Include/cmsis_gcc.h **** 
 883:Drivers/CMSIS/Include/cmsis_gcc.h **** /**
 884:Drivers/CMSIS/Include/cmsis_gcc.h ****   \brief   Data Memory Barrier
 885:Drivers/CMSIS/Include/cmsis_gcc.h ****   \details Ensures the apparent order of the explicit memory operations before
 886:Drivers/CMSIS/Include/cmsis_gcc.h ****            and after the instruction, without ensuring their completion.
 887:Drivers/CMSIS/Include/cmsis_gcc.h ****  */
 888:Drivers/CMSIS/Include/cmsis_gcc.h **** __STATIC_FORCEINLINE void __DMB(void)
 548              		.loc 3 888 27 view .LVU148
 549              	.LBB87:
 889:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 890:Drivers/CMSIS/Include/cmsis_gcc.h ****   __ASM volatile ("dmb 0xF":::"memory");
 550              		.loc 3 890 3 view .LVU149
 551              		.syntax unified
 552              	@ 890 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 553 0000 BFF35F8F 		dmb 0xF
 554              	@ 0 "" 2
 555              		.thumb
 556              		.syntax unified
 557              	.LBE87:
 558              	.LBE86:
 262:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 263:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Disable fault exceptions */
 264:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   SCB->SHCSR &= ~SCB_SHCSR_MEMFAULTENA_Msk;
 559              		.loc 1 264 3 view .LVU150
 560              		.loc 1 264 14 is_stmt 0 view .LVU151
 561 0004 044B     		ldr	r3, .L30
 562 0006 5A6A     		ldr	r2, [r3, #36]
 563 0008 22F48032 		bic	r2, r2, #65536
 564 000c 5A62     		str	r2, [r3, #36]
 265:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 266:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Disable the MPU and clear the control register*/
 267:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   MPU->CTRL = 0U;
 565              		.loc 1 267 3 is_stmt 1 view .LVU152
 566              		.loc 1 267 13 is_stmt 0 view .LVU153
 567 000e 0022     		movs	r2, #0
 568 0010 C3F89420 		str	r2, [r3, #148]
 268:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 569              		.loc 1 268 1 view .LVU154
 570 0014 7047     		bx	lr
 571              	.L31:
 572 0016 00BF     		.align	2
 573              	.L30:
 574 0018 00ED00E0 		.word	-536810240
 575              		.cfi_endproc
 576              	.LFE136:
 578              		.section	.text.HAL_MPU_Enable,"ax",%progbits
 579              		.align	1
 580              		.global	HAL_MPU_Enable
 581              		.syntax unified
 582              		.thumb
ARM GAS  /tmp/ccPRqU3T.s 			page 68


 583              		.thumb_func
 585              	HAL_MPU_Enable:
 586              	.LVL39:
 587              	.LFB137:
 269:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 270:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 271:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Enable the MPU.
 272:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  MPU_Control Specifies the control mode of the MPU during hard fault, 
 273:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *          NMI, FAULTMASK and privileged access to the default memory 
 274:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *          This parameter can be one of the following values:
 275:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *            @arg MPU_HFNMI_PRIVDEF_NONE
 276:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *            @arg MPU_HARDFAULT_NMI
 277:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *            @arg MPU_PRIVILEGED_DEFAULT
 278:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *            @arg MPU_HFNMI_PRIVDEF
 279:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 280:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 281:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_MPU_Enable(uint32_t MPU_Control)
 282:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 588              		.loc 1 282 1 is_stmt 1 view -0
 589              		.cfi_startproc
 590              		@ args = 0, pretend = 0, frame = 0
 591              		@ frame_needed = 0, uses_anonymous_args = 0
 592              		@ link register save eliminated.
 283:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Enable the MPU */
 284:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   MPU->CTRL = MPU_Control | MPU_CTRL_ENABLE_Msk;
 593              		.loc 1 284 3 view .LVU156
 594              		.loc 1 284 27 is_stmt 0 view .LVU157
 595 0000 40F00100 		orr	r0, r0, #1
 596              	.LVL40:
 597              		.loc 1 284 13 view .LVU158
 598 0004 054B     		ldr	r3, .L33
 599 0006 C3F89400 		str	r0, [r3, #148]
 285:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 286:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Enable fault exceptions */
 287:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   SCB->SHCSR |= SCB_SHCSR_MEMFAULTENA_Msk;
 600              		.loc 1 287 3 is_stmt 1 view .LVU159
 601              		.loc 1 287 14 is_stmt 0 view .LVU160
 602 000a 5A6A     		ldr	r2, [r3, #36]
 603 000c 42F48032 		orr	r2, r2, #65536
 604 0010 5A62     		str	r2, [r3, #36]
 288:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 289:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Ensure MPU setting take effects */
 290:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   __DSB();
 605              		.loc 1 290 3 is_stmt 1 view .LVU161
 606              	.LBB88:
 607              	.LBI88:
 877:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 608              		.loc 3 877 27 view .LVU162
 609              	.LBB89:
 879:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 610              		.loc 3 879 3 view .LVU163
 611              		.syntax unified
 612              	@ 879 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 613 0012 BFF34F8F 		dsb 0xF
 614              	@ 0 "" 2
 615              		.thumb
 616              		.syntax unified
ARM GAS  /tmp/ccPRqU3T.s 			page 69


 617              	.LBE89:
 618              	.LBE88:
 291:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   __ISB();
 619              		.loc 1 291 3 view .LVU164
 620              	.LBB90:
 621              	.LBI90:
 866:Drivers/CMSIS/Include/cmsis_gcc.h **** {
 622              		.loc 3 866 27 view .LVU165
 623              	.LBB91:
 868:Drivers/CMSIS/Include/cmsis_gcc.h **** }
 624              		.loc 3 868 3 view .LVU166
 625              		.syntax unified
 626              	@ 868 "Drivers/CMSIS/Include/cmsis_gcc.h" 1
 627 0016 BFF36F8F 		isb 0xF
 628              	@ 0 "" 2
 629              		.thumb
 630              		.syntax unified
 631              	.LBE91:
 632              	.LBE90:
 292:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 633              		.loc 1 292 1 is_stmt 0 view .LVU167
 634 001a 7047     		bx	lr
 635              	.L34:
 636              		.align	2
 637              	.L33:
 638 001c 00ED00E0 		.word	-536810240
 639              		.cfi_endproc
 640              	.LFE137:
 642              		.section	.text.HAL_MPU_ConfigRegion,"ax",%progbits
 643              		.align	1
 644              		.global	HAL_MPU_ConfigRegion
 645              		.syntax unified
 646              		.thumb
 647              		.thumb_func
 649              	HAL_MPU_ConfigRegion:
 650              	.LVL41:
 651              	.LFB138:
 293:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 294:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 295:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Initializes and configures the Region and the memory to be protected.
 296:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  MPU_Init Pointer to a MPU_Region_InitTypeDef structure that contains
 297:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                the initialization and configuration information.
 298:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 299:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 300:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_MPU_ConfigRegion(MPU_Region_InitTypeDef *MPU_Init)
 301:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 652              		.loc 1 301 1 is_stmt 1 view -0
 653              		.cfi_startproc
 654              		@ args = 0, pretend = 0, frame = 0
 655              		@ frame_needed = 0, uses_anonymous_args = 0
 656              		@ link register save eliminated.
 302:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 303:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_MPU_REGION_NUMBER(MPU_Init->Number));
 657              		.loc 1 303 3 view .LVU169
 304:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_MPU_REGION_ENABLE(MPU_Init->Enable));
 658              		.loc 1 304 3 view .LVU170
 305:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
ARM GAS  /tmp/ccPRqU3T.s 			page 70


 306:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Set the Region number */
 307:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   MPU->RNR = MPU_Init->Number;
 659              		.loc 1 307 3 view .LVU171
 660              		.loc 1 307 22 is_stmt 0 view .LVU172
 661 0000 4278     		ldrb	r2, [r0, #1]	@ zero_extendqisi2
 662              		.loc 1 307 12 view .LVU173
 663 0002 164B     		ldr	r3, .L38
 664 0004 C3F89820 		str	r2, [r3, #152]
 308:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 309:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   if ((MPU_Init->Enable) != RESET)
 665              		.loc 1 309 3 is_stmt 1 view .LVU174
 666              		.loc 1 309 16 is_stmt 0 view .LVU175
 667 0008 0378     		ldrb	r3, [r0]	@ zero_extendqisi2
 668              		.loc 1 309 6 view .LVU176
 669 000a FBB1     		cbz	r3, .L36
 310:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   {
 311:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     /* Check the parameters */
 312:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_INSTRUCTION_ACCESS(MPU_Init->DisableExec));
 670              		.loc 1 312 5 is_stmt 1 view .LVU177
 313:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_REGION_PERMISSION_ATTRIBUTE(MPU_Init->AccessPermission));
 671              		.loc 1 313 5 view .LVU178
 314:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_TEX_LEVEL(MPU_Init->TypeExtField));
 672              		.loc 1 314 5 view .LVU179
 315:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_ACCESS_SHAREABLE(MPU_Init->IsShareable));
 673              		.loc 1 315 5 view .LVU180
 316:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_ACCESS_CACHEABLE(MPU_Init->IsCacheable));
 674              		.loc 1 316 5 view .LVU181
 317:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_ACCESS_BUFFERABLE(MPU_Init->IsBufferable));
 675              		.loc 1 317 5 view .LVU182
 318:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_SUB_REGION_DISABLE(MPU_Init->SubRegionDisable));
 676              		.loc 1 318 5 view .LVU183
 319:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     assert_param(IS_MPU_REGION_SIZE(MPU_Init->Size));
 677              		.loc 1 319 5 view .LVU184
 320:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     
 321:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     MPU->RBAR = MPU_Init->BaseAddress;
 678              		.loc 1 321 5 view .LVU185
 679              		.loc 1 321 25 is_stmt 0 view .LVU186
 680 000c 4368     		ldr	r3, [r0, #4]
 681              		.loc 1 321 15 view .LVU187
 682 000e 134A     		ldr	r2, .L38
 683 0010 C2F89C30 		str	r3, [r2, #156]
 322:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     MPU->RASR = ((uint32_t)MPU_Init->DisableExec             << MPU_RASR_XN_Pos)   |
 684              		.loc 1 322 5 is_stmt 1 view .LVU188
 685              		.loc 1 322 36 is_stmt 0 view .LVU189
 686 0014 017B     		ldrb	r1, [r0, #12]	@ zero_extendqisi2
 323:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->AccessPermission        << MPU_RASR_AP_Pos)   |
 687              		.loc 1 323 36 view .LVU190
 688 0016 C37A     		ldrb	r3, [r0, #11]	@ zero_extendqisi2
 689              		.loc 1 323 62 view .LVU191
 690 0018 1B06     		lsls	r3, r3, #24
 322:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     MPU->RASR = ((uint32_t)MPU_Init->DisableExec             << MPU_RASR_XN_Pos)   |
 691              		.loc 1 322 84 view .LVU192
 692 001a 43EA0173 		orr	r3, r3, r1, lsl #28
 324:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->TypeExtField            << MPU_RASR_TEX_Pos)  |
 693              		.loc 1 324 36 view .LVU193
 694 001e 817A     		ldrb	r1, [r0, #10]	@ zero_extendqisi2
 323:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->AccessPermission        << MPU_RASR_AP_Pos)   |
ARM GAS  /tmp/ccPRqU3T.s 			page 71


 695              		.loc 1 323 84 view .LVU194
 696 0020 43EAC143 		orr	r3, r3, r1, lsl #19
 325:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->IsShareable             << MPU_RASR_S_Pos)    |
 697              		.loc 1 325 36 view .LVU195
 698 0024 417B     		ldrb	r1, [r0, #13]	@ zero_extendqisi2
 324:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->TypeExtField            << MPU_RASR_TEX_Pos)  |
 699              		.loc 1 324 84 view .LVU196
 700 0026 43EA8143 		orr	r3, r3, r1, lsl #18
 326:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->IsCacheable             << MPU_RASR_C_Pos)    |
 701              		.loc 1 326 36 view .LVU197
 702 002a 817B     		ldrb	r1, [r0, #14]	@ zero_extendqisi2
 325:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->IsShareable             << MPU_RASR_S_Pos)    |
 703              		.loc 1 325 84 view .LVU198
 704 002c 43EA4143 		orr	r3, r3, r1, lsl #17
 327:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->IsBufferable            << MPU_RASR_B_Pos)    |
 705              		.loc 1 327 36 view .LVU199
 706 0030 C17B     		ldrb	r1, [r0, #15]	@ zero_extendqisi2
 326:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->IsCacheable             << MPU_RASR_C_Pos)    |
 707              		.loc 1 326 84 view .LVU200
 708 0032 43EA0143 		orr	r3, r3, r1, lsl #16
 328:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->SubRegionDisable        << MPU_RASR_SRD_Pos)  |
 709              		.loc 1 328 36 view .LVU201
 710 0036 417A     		ldrb	r1, [r0, #9]	@ zero_extendqisi2
 327:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->IsBufferable            << MPU_RASR_B_Pos)    |
 711              		.loc 1 327 84 view .LVU202
 712 0038 43EA0123 		orr	r3, r3, r1, lsl #8
 329:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->Size                    << MPU_RASR_SIZE_Pos) |
 713              		.loc 1 329 36 view .LVU203
 714 003c 017A     		ldrb	r1, [r0, #8]	@ zero_extendqisi2
 328:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->SubRegionDisable        << MPU_RASR_SRD_Pos)  |
 715              		.loc 1 328 84 view .LVU204
 716 003e 43EA4103 		orr	r3, r3, r1, lsl #1
 330:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->Enable                  << MPU_RASR_ENABLE_Pos);
 717              		.loc 1 330 36 view .LVU205
 718 0042 0178     		ldrb	r1, [r0]	@ zero_extendqisi2
 329:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->Size                    << MPU_RASR_SIZE_Pos) |
 719              		.loc 1 329 84 view .LVU206
 720 0044 0B43     		orrs	r3, r3, r1
 322:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****                 ((uint32_t)MPU_Init->AccessPermission        << MPU_RASR_AP_Pos)   |
 721              		.loc 1 322 15 view .LVU207
 722 0046 C2F8A030 		str	r3, [r2, #160]
 723 004a 7047     		bx	lr
 724              	.L36:
 331:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   }
 332:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   else
 333:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   {
 334:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     MPU->RBAR = 0x00U;
 725              		.loc 1 334 5 is_stmt 1 view .LVU208
 726              		.loc 1 334 15 is_stmt 0 view .LVU209
 727 004c 034B     		ldr	r3, .L38
 728 004e 0022     		movs	r2, #0
 729 0050 C3F89C20 		str	r2, [r3, #156]
 335:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     MPU->RASR = 0x00U;
 730              		.loc 1 335 5 is_stmt 1 view .LVU210
 731              		.loc 1 335 15 is_stmt 0 view .LVU211
 732 0054 C3F8A020 		str	r2, [r3, #160]
 336:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   }
ARM GAS  /tmp/ccPRqU3T.s 			page 72


 337:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 733              		.loc 1 337 1 view .LVU212
 734 0058 7047     		bx	lr
 735              	.L39:
 736 005a 00BF     		.align	2
 737              	.L38:
 738 005c 00ED00E0 		.word	-536810240
 739              		.cfi_endproc
 740              	.LFE138:
 742              		.section	.text.HAL_NVIC_GetPriorityGrouping,"ax",%progbits
 743              		.align	1
 744              		.global	HAL_NVIC_GetPriorityGrouping
 745              		.syntax unified
 746              		.thumb
 747              		.thumb_func
 749              	HAL_NVIC_GetPriorityGrouping:
 750              	.LFB139:
 338:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** #endif /* __MPU_PRESENT */
 339:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 340:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 341:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Gets the priority grouping field from the NVIC Interrupt Controller.
 342:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval Priority grouping field (SCB->AIRCR [10:8] PRIGROUP field)
 343:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 344:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** uint32_t HAL_NVIC_GetPriorityGrouping(void)
 345:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 751              		.loc 1 345 1 is_stmt 1 view -0
 752              		.cfi_startproc
 753              		@ args = 0, pretend = 0, frame = 0
 754              		@ frame_needed = 0, uses_anonymous_args = 0
 755              		@ link register save eliminated.
 346:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Get the PRIGROUP[10:8] field value */
 347:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   return NVIC_GetPriorityGrouping();
 756              		.loc 1 347 3 view .LVU214
 757              	.LBB92:
 758              	.LBI92:
1676:Drivers/CMSIS/Include/core_cm4.h **** {
 759              		.loc 2 1676 26 view .LVU215
 760              	.LBB93:
1678:Drivers/CMSIS/Include/core_cm4.h **** }
 761              		.loc 2 1678 3 view .LVU216
1678:Drivers/CMSIS/Include/core_cm4.h **** }
 762              		.loc 2 1678 26 is_stmt 0 view .LVU217
 763 0000 024B     		ldr	r3, .L41
 764 0002 D868     		ldr	r0, [r3, #12]
 765              	.LBE93:
 766              	.LBE92:
 348:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 767              		.loc 1 348 1 view .LVU218
 768 0004 C0F30220 		ubfx	r0, r0, #8, #3
 769 0008 7047     		bx	lr
 770              	.L42:
 771 000a 00BF     		.align	2
 772              	.L41:
 773 000c 00ED00E0 		.word	-536810240
 774              		.cfi_endproc
 775              	.LFE139:
 777              		.section	.text.HAL_NVIC_GetPriority,"ax",%progbits
ARM GAS  /tmp/ccPRqU3T.s 			page 73


 778              		.align	1
 779              		.global	HAL_NVIC_GetPriority
 780              		.syntax unified
 781              		.thumb
 782              		.thumb_func
 784              	HAL_NVIC_GetPriority:
 785              	.LVL42:
 786              	.LFB140:
 349:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 350:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 351:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Gets the priority of an interrupt.
 352:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number.
 353:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 354:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 355:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param   PriorityGroup the priority grouping bits length.
 356:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be one of the following values:
 357:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           @arg NVIC_PRIORITYGROUP_0: 0 bits for preemption priority
 358:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                      4 bits for subpriority
 359:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           @arg NVIC_PRIORITYGROUP_1: 1 bits for preemption priority
 360:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                      3 bits for subpriority
 361:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           @arg NVIC_PRIORITYGROUP_2: 2 bits for preemption priority
 362:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                      2 bits for subpriority
 363:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           @arg NVIC_PRIORITYGROUP_3: 3 bits for preemption priority
 364:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                      1 bits for subpriority
 365:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *           @arg NVIC_PRIORITYGROUP_4: 4 bits for preemption priority
 366:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                                      0 bits for subpriority
 367:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  pPreemptPriority Pointer on the Preemptive priority value (starting from 0).
 368:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  pSubPriority Pointer on the Subpriority value (starting from 0).
 369:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 370:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 371:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_GetPriority(IRQn_Type IRQn, uint32_t PriorityGroup, uint32_t *pPreemptPriority, uint3
 372:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 787              		.loc 1 372 1 is_stmt 1 view -0
 788              		.cfi_startproc
 789              		@ args = 0, pretend = 0, frame = 0
 790              		@ frame_needed = 0, uses_anonymous_args = 0
 791              		.loc 1 372 1 is_stmt 0 view .LVU220
 792 0000 10B5     		push	{r4, lr}
 793              	.LCFI1:
 794              		.cfi_def_cfa_offset 8
 795              		.cfi_offset 4, -8
 796              		.cfi_offset 14, -4
 373:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 374:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_PRIORITY_GROUP(PriorityGroup));
 797              		.loc 1 374 3 is_stmt 1 view .LVU221
 375:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****  /* Get priority for Cortex-M system or device specific interrupts */
 376:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_DecodePriority(NVIC_GetPriority(IRQn), PriorityGroup, pPreemptPriority, pSubPriority);
 798              		.loc 1 376 3 view .LVU222
 799              	.LVL43:
 800              	.LBB98:
 801              	.LBI98:
1838:Drivers/CMSIS/Include/core_cm4.h **** {
 802              		.loc 2 1838 26 view .LVU223
 803              	.LBB99:
1841:Drivers/CMSIS/Include/core_cm4.h ****   {
 804              		.loc 2 1841 3 view .LVU224
1841:Drivers/CMSIS/Include/core_cm4.h ****   {
ARM GAS  /tmp/ccPRqU3T.s 			page 74


 805              		.loc 2 1841 6 is_stmt 0 view .LVU225
 806 0002 0028     		cmp	r0, #0
 807              	.LVL44:
1841:Drivers/CMSIS/Include/core_cm4.h ****   {
 808              		.loc 2 1841 6 view .LVU226
 809 0004 22DB     		blt	.L44
1843:Drivers/CMSIS/Include/core_cm4.h ****   }
 810              		.loc 2 1843 5 is_stmt 1 view .LVU227
1843:Drivers/CMSIS/Include/core_cm4.h ****   }
 811              		.loc 2 1843 31 is_stmt 0 view .LVU228
 812 0006 00F16040 		add	r0, r0, #-536870912
 813 000a 00F56140 		add	r0, r0, #57600
 814 000e 90F80003 		ldrb	r0, [r0, #768]	@ zero_extendqisi2
1843:Drivers/CMSIS/Include/core_cm4.h ****   }
 815              		.loc 2 1843 64 view .LVU229
 816 0012 0009     		lsrs	r0, r0, #4
 817              	.L45:
 818              	.LVL45:
1843:Drivers/CMSIS/Include/core_cm4.h ****   }
 819              		.loc 2 1843 64 view .LVU230
 820              	.LBE99:
 821              	.LBE98:
 822              	.LBB101:
 823              	.LBI101:
1890:Drivers/CMSIS/Include/core_cm4.h **** {
 824              		.loc 2 1890 22 is_stmt 1 view .LVU231
 825              	.LBB102:
1892:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PreemptPriorityBits;
 826              		.loc 2 1892 3 view .LVU232
1892:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t PreemptPriorityBits;
 827              		.loc 2 1892 12 is_stmt 0 view .LVU233
 828 0014 01F00701 		and	r1, r1, #7
 829              	.LVL46:
1893:Drivers/CMSIS/Include/core_cm4.h ****   uint32_t SubPriorityBits;
 830              		.loc 2 1893 3 is_stmt 1 view .LVU234
1894:Drivers/CMSIS/Include/core_cm4.h **** 
 831              		.loc 2 1894 3 view .LVU235
1896:Drivers/CMSIS/Include/core_cm4.h ****   SubPriorityBits     = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint
 832              		.loc 2 1896 3 view .LVU236
1896:Drivers/CMSIS/Include/core_cm4.h ****   SubPriorityBits     = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint
 833              		.loc 2 1896 31 is_stmt 0 view .LVU237
 834 0018 C1F1070C 		rsb	ip, r1, #7
1896:Drivers/CMSIS/Include/core_cm4.h ****   SubPriorityBits     = ((PriorityGroupTmp + (uint32_t)(__NVIC_PRIO_BITS)) < (uint32_t)7UL) ? (uint
 835              		.loc 2 1896 23 view .LVU238
 836 001c BCF1040F 		cmp	ip, #4
 837 0020 28BF     		it	cs
 838 0022 4FF0040C 		movcs	ip, #4
 839              	.LVL47:
1897:Drivers/CMSIS/Include/core_cm4.h **** 
 840              		.loc 2 1897 3 is_stmt 1 view .LVU239
1897:Drivers/CMSIS/Include/core_cm4.h **** 
 841              		.loc 2 1897 44 is_stmt 0 view .LVU240
 842 0026 0C1D     		adds	r4, r1, #4
1897:Drivers/CMSIS/Include/core_cm4.h **** 
 843              		.loc 2 1897 109 view .LVU241
 844 0028 062C     		cmp	r4, #6
 845 002a 15D9     		bls	.L47
ARM GAS  /tmp/ccPRqU3T.s 			page 75


 846 002c 0339     		subs	r1, r1, #3
 847              	.LVL48:
 848              	.L46:
1899:Drivers/CMSIS/Include/core_cm4.h ****   *pSubPriority     = (Priority                   ) & (uint32_t)((1UL << (SubPriorityBits    )) - 1
 849              		.loc 2 1899 3 is_stmt 1 view .LVU242
1899:Drivers/CMSIS/Include/core_cm4.h ****   *pSubPriority     = (Priority                   ) & (uint32_t)((1UL << (SubPriorityBits    )) - 1
 850              		.loc 2 1899 33 is_stmt 0 view .LVU243
 851 002e 20FA01F4 		lsr	r4, r0, r1
 852              	.LVL49:
1899:Drivers/CMSIS/Include/core_cm4.h ****   *pSubPriority     = (Priority                   ) & (uint32_t)((1UL << (SubPriorityBits    )) - 1
 853              		.loc 2 1899 53 view .LVU244
 854 0032 4FF0FF3E 		mov	lr, #-1
 855 0036 0EFA0CFC 		lsl	ip, lr, ip
 856              	.LVL50:
1899:Drivers/CMSIS/Include/core_cm4.h ****   *pSubPriority     = (Priority                   ) & (uint32_t)((1UL << (SubPriorityBits    )) - 1
 857              		.loc 2 1899 53 view .LVU245
 858 003a 24EA0C04 		bic	r4, r4, ip
1899:Drivers/CMSIS/Include/core_cm4.h ****   *pSubPriority     = (Priority                   ) & (uint32_t)((1UL << (SubPriorityBits    )) - 1
 859              		.loc 2 1899 21 view .LVU246
 860 003e 1460     		str	r4, [r2]
1900:Drivers/CMSIS/Include/core_cm4.h **** }
 861              		.loc 2 1900 3 is_stmt 1 view .LVU247
1900:Drivers/CMSIS/Include/core_cm4.h **** }
 862              		.loc 2 1900 53 is_stmt 0 view .LVU248
 863 0040 0EFA01F1 		lsl	r1, lr, r1
 864              	.LVL51:
1900:Drivers/CMSIS/Include/core_cm4.h **** }
 865              		.loc 2 1900 53 view .LVU249
 866 0044 20EA0100 		bic	r0, r0, r1
 867              	.LVL52:
1900:Drivers/CMSIS/Include/core_cm4.h **** }
 868              		.loc 2 1900 21 view .LVU250
 869 0048 1860     		str	r0, [r3]
 870              	.LVL53:
1900:Drivers/CMSIS/Include/core_cm4.h **** }
 871              		.loc 2 1900 21 view .LVU251
 872              	.LBE102:
 873              	.LBE101:
 377:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 874              		.loc 1 377 1 view .LVU252
 875 004a 10BD     		pop	{r4, pc}
 876              	.LVL54:
 877              	.L44:
 878              	.LBB104:
 879              	.LBB100:
1847:Drivers/CMSIS/Include/core_cm4.h ****   }
 880              		.loc 2 1847 5 is_stmt 1 view .LVU253
1847:Drivers/CMSIS/Include/core_cm4.h ****   }
 881              		.loc 2 1847 50 is_stmt 0 view .LVU254
 882 004c 00F00F00 		and	r0, r0, #15
1847:Drivers/CMSIS/Include/core_cm4.h ****   }
 883              		.loc 2 1847 31 view .LVU255
 884 0050 024C     		ldr	r4, .L49
 885 0052 205C     		ldrb	r0, [r4, r0]	@ zero_extendqisi2
1847:Drivers/CMSIS/Include/core_cm4.h ****   }
 886              		.loc 2 1847 64 view .LVU256
 887 0054 0009     		lsrs	r0, r0, #4
ARM GAS  /tmp/ccPRqU3T.s 			page 76


 888 0056 DDE7     		b	.L45
 889              	.LVL55:
 890              	.L47:
1847:Drivers/CMSIS/Include/core_cm4.h ****   }
 891              		.loc 2 1847 64 view .LVU257
 892              	.LBE100:
 893              	.LBE104:
 894              	.LBB105:
 895              	.LBB103:
1897:Drivers/CMSIS/Include/core_cm4.h **** 
 896              		.loc 2 1897 109 view .LVU258
 897 0058 0021     		movs	r1, #0
 898              	.LVL56:
1897:Drivers/CMSIS/Include/core_cm4.h **** 
 899              		.loc 2 1897 109 view .LVU259
 900 005a E8E7     		b	.L46
 901              	.L50:
 902              		.align	2
 903              	.L49:
 904 005c 14ED00E0 		.word	-536810220
 905              	.LBE103:
 906              	.LBE105:
 907              		.cfi_endproc
 908              	.LFE140:
 910              		.section	.text.HAL_NVIC_SetPendingIRQ,"ax",%progbits
 911              		.align	1
 912              		.global	HAL_NVIC_SetPendingIRQ
 913              		.syntax unified
 914              		.thumb
 915              		.thumb_func
 917              	HAL_NVIC_SetPendingIRQ:
 918              	.LVL57:
 919              	.LFB141:
 378:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 379:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 380:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Sets Pending bit of an external interrupt.
 381:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number
 382:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 383:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 384:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 385:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 386:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_SetPendingIRQ(IRQn_Type IRQn)
 387:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 920              		.loc 1 387 1 is_stmt 1 view -0
 921              		.cfi_startproc
 922              		@ args = 0, pretend = 0, frame = 0
 923              		@ frame_needed = 0, uses_anonymous_args = 0
 924              		@ link register save eliminated.
 388:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 389:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_DEVICE_IRQ(IRQn));
 925              		.loc 1 389 3 view .LVU261
 390:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 391:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Set interrupt pending */
 392:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_SetPendingIRQ(IRQn);
 926              		.loc 1 392 3 view .LVU262
 927              	.LBB106:
 928              	.LBI106:
ARM GAS  /tmp/ccPRqU3T.s 			page 77


1762:Drivers/CMSIS/Include/core_cm4.h **** {
 929              		.loc 2 1762 22 view .LVU263
 930              	.LBB107:
1764:Drivers/CMSIS/Include/core_cm4.h ****   {
 931              		.loc 2 1764 3 view .LVU264
1764:Drivers/CMSIS/Include/core_cm4.h ****   {
 932              		.loc 2 1764 6 is_stmt 0 view .LVU265
 933 0000 0028     		cmp	r0, #0
 934              	.LVL58:
1764:Drivers/CMSIS/Include/core_cm4.h ****   {
 935              		.loc 2 1764 6 view .LVU266
 936 0002 08DB     		blt	.L51
1766:Drivers/CMSIS/Include/core_cm4.h ****   }
 937              		.loc 2 1766 5 is_stmt 1 view .LVU267
1766:Drivers/CMSIS/Include/core_cm4.h ****   }
 938              		.loc 2 1766 81 is_stmt 0 view .LVU268
 939 0004 00F01F02 		and	r2, r0, #31
1766:Drivers/CMSIS/Include/core_cm4.h ****   }
 940              		.loc 2 1766 34 view .LVU269
 941 0008 4009     		lsrs	r0, r0, #5
1766:Drivers/CMSIS/Include/core_cm4.h ****   }
 942              		.loc 2 1766 45 view .LVU270
 943 000a 0123     		movs	r3, #1
 944 000c 9340     		lsls	r3, r3, r2
1766:Drivers/CMSIS/Include/core_cm4.h ****   }
 945              		.loc 2 1766 43 view .LVU271
 946 000e 4030     		adds	r0, r0, #64
 947 0010 014A     		ldr	r2, .L53
 948 0012 42F82030 		str	r3, [r2, r0, lsl #2]
 949              	.LVL59:
 950              	.L51:
1766:Drivers/CMSIS/Include/core_cm4.h ****   }
 951              		.loc 2 1766 43 view .LVU272
 952              	.LBE107:
 953              	.LBE106:
 393:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 954              		.loc 1 393 1 view .LVU273
 955 0016 7047     		bx	lr
 956              	.L54:
 957              		.align	2
 958              	.L53:
 959 0018 00E100E0 		.word	-536813312
 960              		.cfi_endproc
 961              	.LFE141:
 963              		.section	.text.HAL_NVIC_GetPendingIRQ,"ax",%progbits
 964              		.align	1
 965              		.global	HAL_NVIC_GetPendingIRQ
 966              		.syntax unified
 967              		.thumb
 968              		.thumb_func
 970              	HAL_NVIC_GetPendingIRQ:
 971              	.LVL60:
 972              	.LFB142:
 394:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 395:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 396:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Gets Pending Interrupt (reads the pending register in the NVIC 
 397:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         and returns the pending bit for the specified interrupt).
ARM GAS  /tmp/ccPRqU3T.s 			page 78


 398:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number.
 399:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *          This parameter can be an enumerator of IRQn_Type enumeration
 400:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 401:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval status: - 0  Interrupt status is not pending.
 402:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                 - 1  Interrupt status is pending.
 403:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 404:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** uint32_t HAL_NVIC_GetPendingIRQ(IRQn_Type IRQn)
 405:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 973              		.loc 1 405 1 is_stmt 1 view -0
 974              		.cfi_startproc
 975              		@ args = 0, pretend = 0, frame = 0
 976              		@ frame_needed = 0, uses_anonymous_args = 0
 977              		@ link register save eliminated.
 406:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 407:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_DEVICE_IRQ(IRQn));
 978              		.loc 1 407 3 view .LVU275
 408:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 409:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Return 1 if pending else 0 */
 410:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   return NVIC_GetPendingIRQ(IRQn);
 979              		.loc 1 410 3 view .LVU276
 980              	.LBB108:
 981              	.LBI108:
1743:Drivers/CMSIS/Include/core_cm4.h **** {
 982              		.loc 2 1743 26 view .LVU277
 983              	.LBB109:
1745:Drivers/CMSIS/Include/core_cm4.h ****   {
 984              		.loc 2 1745 3 view .LVU278
1745:Drivers/CMSIS/Include/core_cm4.h ****   {
 985              		.loc 2 1745 6 is_stmt 0 view .LVU279
 986 0000 0028     		cmp	r0, #0
 987              	.LVL61:
1745:Drivers/CMSIS/Include/core_cm4.h ****   {
 988              		.loc 2 1745 6 view .LVU280
 989 0002 0BDB     		blt	.L57
1747:Drivers/CMSIS/Include/core_cm4.h ****   }
 990              		.loc 2 1747 5 is_stmt 1 view .LVU281
1747:Drivers/CMSIS/Include/core_cm4.h ****   }
 991              		.loc 2 1747 54 is_stmt 0 view .LVU282
 992 0004 4309     		lsrs	r3, r0, #5
1747:Drivers/CMSIS/Include/core_cm4.h ****   }
 993              		.loc 2 1747 35 view .LVU283
 994 0006 4033     		adds	r3, r3, #64
 995 0008 054A     		ldr	r2, .L58
 996 000a 52F82330 		ldr	r3, [r2, r3, lsl #2]
1747:Drivers/CMSIS/Include/core_cm4.h ****   }
 997              		.loc 2 1747 91 view .LVU284
 998 000e 00F01F00 		and	r0, r0, #31
1747:Drivers/CMSIS/Include/core_cm4.h ****   }
 999              		.loc 2 1747 103 view .LVU285
 1000 0012 23FA00F0 		lsr	r0, r3, r0
1747:Drivers/CMSIS/Include/core_cm4.h ****   }
 1001              		.loc 2 1747 12 view .LVU286
 1002 0016 00F00100 		and	r0, r0, #1
 1003 001a 7047     		bx	lr
 1004              	.L57:
1751:Drivers/CMSIS/Include/core_cm4.h ****   }
 1005              		.loc 2 1751 11 view .LVU287
ARM GAS  /tmp/ccPRqU3T.s 			page 79


 1006 001c 0020     		movs	r0, #0
 1007              	.LVL62:
1751:Drivers/CMSIS/Include/core_cm4.h ****   }
 1008              		.loc 2 1751 11 view .LVU288
 1009              	.LBE109:
 1010              	.LBE108:
 411:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 1011              		.loc 1 411 1 view .LVU289
 1012 001e 7047     		bx	lr
 1013              	.L59:
 1014              		.align	2
 1015              	.L58:
 1016 0020 00E100E0 		.word	-536813312
 1017              		.cfi_endproc
 1018              	.LFE142:
 1020              		.section	.text.HAL_NVIC_ClearPendingIRQ,"ax",%progbits
 1021              		.align	1
 1022              		.global	HAL_NVIC_ClearPendingIRQ
 1023              		.syntax unified
 1024              		.thumb
 1025              		.thumb_func
 1027              	HAL_NVIC_ClearPendingIRQ:
 1028              	.LVL63:
 1029              	.LFB143:
 412:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 413:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 414:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Clears the pending bit of an external interrupt.
 415:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  IRQn External interrupt number.
 416:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 417:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 418:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 419:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 420:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_NVIC_ClearPendingIRQ(IRQn_Type IRQn)
 421:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 1030              		.loc 1 421 1 is_stmt 1 view -0
 1031              		.cfi_startproc
 1032              		@ args = 0, pretend = 0, frame = 0
 1033              		@ frame_needed = 0, uses_anonymous_args = 0
 1034              		@ link register save eliminated.
 422:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 423:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_DEVICE_IRQ(IRQn));
 1035              		.loc 1 423 3 view .LVU291
 424:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 425:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Clear pending interrupt */
 426:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   NVIC_ClearPendingIRQ(IRQn);
 1036              		.loc 1 426 3 view .LVU292
 1037              	.LBB110:
 1038              	.LBI110:
1777:Drivers/CMSIS/Include/core_cm4.h **** {
 1039              		.loc 2 1777 22 view .LVU293
 1040              	.LBB111:
1779:Drivers/CMSIS/Include/core_cm4.h ****   {
 1041              		.loc 2 1779 3 view .LVU294
1779:Drivers/CMSIS/Include/core_cm4.h ****   {
 1042              		.loc 2 1779 6 is_stmt 0 view .LVU295
 1043 0000 0028     		cmp	r0, #0
 1044              	.LVL64:
ARM GAS  /tmp/ccPRqU3T.s 			page 80


1779:Drivers/CMSIS/Include/core_cm4.h ****   {
 1045              		.loc 2 1779 6 view .LVU296
 1046 0002 08DB     		blt	.L60
1781:Drivers/CMSIS/Include/core_cm4.h ****   }
 1047              		.loc 2 1781 5 is_stmt 1 view .LVU297
1781:Drivers/CMSIS/Include/core_cm4.h ****   }
 1048              		.loc 2 1781 81 is_stmt 0 view .LVU298
 1049 0004 00F01F02 		and	r2, r0, #31
1781:Drivers/CMSIS/Include/core_cm4.h ****   }
 1050              		.loc 2 1781 34 view .LVU299
 1051 0008 4009     		lsrs	r0, r0, #5
1781:Drivers/CMSIS/Include/core_cm4.h ****   }
 1052              		.loc 2 1781 45 view .LVU300
 1053 000a 0123     		movs	r3, #1
 1054 000c 9340     		lsls	r3, r3, r2
1781:Drivers/CMSIS/Include/core_cm4.h ****   }
 1055              		.loc 2 1781 43 view .LVU301
 1056 000e 6030     		adds	r0, r0, #96
 1057 0010 014A     		ldr	r2, .L62
 1058 0012 42F82030 		str	r3, [r2, r0, lsl #2]
 1059              	.LVL65:
 1060              	.L60:
1781:Drivers/CMSIS/Include/core_cm4.h ****   }
 1061              		.loc 2 1781 43 view .LVU302
 1062              	.LBE111:
 1063              	.LBE110:
 427:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 1064              		.loc 1 427 1 view .LVU303
 1065 0016 7047     		bx	lr
 1066              	.L63:
 1067              		.align	2
 1068              	.L62:
 1069 0018 00E100E0 		.word	-536813312
 1070              		.cfi_endproc
 1071              	.LFE143:
 1073              		.section	.text.HAL_NVIC_GetActive,"ax",%progbits
 1074              		.align	1
 1075              		.global	HAL_NVIC_GetActive
 1076              		.syntax unified
 1077              		.thumb
 1078              		.thumb_func
 1080              	HAL_NVIC_GetActive:
 1081              	.LVL66:
 1082              	.LFB144:
 428:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 429:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 430:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief Gets active interrupt ( reads the active register in NVIC and returns the active bit).
 431:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param IRQn External interrupt number
 432:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         This parameter can be an enumerator of IRQn_Type enumeration
 433:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *         (For the complete STM32 Devices IRQ Channels list, please refer to the appropriate CMSI
 434:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval status: - 0  Interrupt status is not pending.
 435:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *                 - 1  Interrupt status is pending.
 436:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 437:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** uint32_t HAL_NVIC_GetActive(IRQn_Type IRQn)
 438:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 1083              		.loc 1 438 1 is_stmt 1 view -0
 1084              		.cfi_startproc
ARM GAS  /tmp/ccPRqU3T.s 			page 81


 1085              		@ args = 0, pretend = 0, frame = 0
 1086              		@ frame_needed = 0, uses_anonymous_args = 0
 1087              		@ link register save eliminated.
 439:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 440:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_NVIC_DEVICE_IRQ(IRQn));
 1088              		.loc 1 440 3 view .LVU305
 441:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   
 442:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Return 1 if active else 0 */
 443:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   return NVIC_GetActive(IRQn);
 1089              		.loc 1 443 3 view .LVU306
 1090              	.LBB112:
 1091              	.LBI112:
1794:Drivers/CMSIS/Include/core_cm4.h **** {
 1092              		.loc 2 1794 26 view .LVU307
 1093              	.LBB113:
1796:Drivers/CMSIS/Include/core_cm4.h ****   {
 1094              		.loc 2 1796 3 view .LVU308
1796:Drivers/CMSIS/Include/core_cm4.h ****   {
 1095              		.loc 2 1796 6 is_stmt 0 view .LVU309
 1096 0000 0028     		cmp	r0, #0
 1097              	.LVL67:
1796:Drivers/CMSIS/Include/core_cm4.h ****   {
 1098              		.loc 2 1796 6 view .LVU310
 1099 0002 0BDB     		blt	.L66
1798:Drivers/CMSIS/Include/core_cm4.h ****   }
 1100              		.loc 2 1798 5 is_stmt 1 view .LVU311
1798:Drivers/CMSIS/Include/core_cm4.h ****   }
 1101              		.loc 2 1798 54 is_stmt 0 view .LVU312
 1102 0004 4309     		lsrs	r3, r0, #5
1798:Drivers/CMSIS/Include/core_cm4.h ****   }
 1103              		.loc 2 1798 35 view .LVU313
 1104 0006 8033     		adds	r3, r3, #128
 1105 0008 054A     		ldr	r2, .L67
 1106 000a 52F82330 		ldr	r3, [r2, r3, lsl #2]
1798:Drivers/CMSIS/Include/core_cm4.h ****   }
 1107              		.loc 2 1798 91 view .LVU314
 1108 000e 00F01F00 		and	r0, r0, #31
1798:Drivers/CMSIS/Include/core_cm4.h ****   }
 1109              		.loc 2 1798 103 view .LVU315
 1110 0012 23FA00F0 		lsr	r0, r3, r0
1798:Drivers/CMSIS/Include/core_cm4.h ****   }
 1111              		.loc 2 1798 12 view .LVU316
 1112 0016 00F00100 		and	r0, r0, #1
 1113 001a 7047     		bx	lr
 1114              	.L66:
1802:Drivers/CMSIS/Include/core_cm4.h ****   }
 1115              		.loc 2 1802 11 view .LVU317
 1116 001c 0020     		movs	r0, #0
 1117              	.LVL68:
1802:Drivers/CMSIS/Include/core_cm4.h ****   }
 1118              		.loc 2 1802 11 view .LVU318
 1119              	.LBE113:
 1120              	.LBE112:
 444:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 1121              		.loc 1 444 1 view .LVU319
 1122 001e 7047     		bx	lr
 1123              	.L68:
ARM GAS  /tmp/ccPRqU3T.s 			page 82


 1124              		.align	2
 1125              	.L67:
 1126 0020 00E100E0 		.word	-536813312
 1127              		.cfi_endproc
 1128              	.LFE144:
 1130              		.section	.text.HAL_SYSTICK_CLKSourceConfig,"ax",%progbits
 1131              		.align	1
 1132              		.global	HAL_SYSTICK_CLKSourceConfig
 1133              		.syntax unified
 1134              		.thumb
 1135              		.thumb_func
 1137              	HAL_SYSTICK_CLKSourceConfig:
 1138              	.LVL69:
 1139              	.LFB145:
 445:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 446:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 447:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  Configures the SysTick clock source.
 448:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @param  CLKSource specifies the SysTick clock source.
 449:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *          This parameter can be one of the following values:
 450:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *             @arg SYSTICK_CLKSOURCE_HCLK_DIV8: AHB clock divided by 8 selected as SysTick clock 
 451:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   *             @arg SYSTICK_CLKSOURCE_HCLK: AHB clock selected as SysTick clock source.
 452:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 453:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 454:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_SYSTICK_CLKSourceConfig(uint32_t CLKSource)
 455:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 1140              		.loc 1 455 1 is_stmt 1 view -0
 1141              		.cfi_startproc
 1142              		@ args = 0, pretend = 0, frame = 0
 1143              		@ frame_needed = 0, uses_anonymous_args = 0
 1144              		@ link register save eliminated.
 456:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* Check the parameters */
 457:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   assert_param(IS_SYSTICK_CLK_SOURCE(CLKSource));
 1145              		.loc 1 457 3 view .LVU321
 458:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   if (CLKSource == SYSTICK_CLKSOURCE_HCLK)
 1146              		.loc 1 458 3 view .LVU322
 1147              		.loc 1 458 6 is_stmt 0 view .LVU323
 1148 0000 0428     		cmp	r0, #4
 1149 0002 06D0     		beq	.L72
 459:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   {
 460:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     SysTick->CTRL |= SYSTICK_CLKSOURCE_HCLK;
 461:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   }
 462:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   else
 463:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   {
 464:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****     SysTick->CTRL &= ~SYSTICK_CLKSOURCE_HCLK;
 1150              		.loc 1 464 5 is_stmt 1 view .LVU324
 1151              		.loc 1 464 19 is_stmt 0 view .LVU325
 1152 0004 4FF0E022 		mov	r2, #-536813568
 1153 0008 1369     		ldr	r3, [r2, #16]
 1154 000a 23F00403 		bic	r3, r3, #4
 1155 000e 1361     		str	r3, [r2, #16]
 465:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   }
 466:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 1156              		.loc 1 466 1 view .LVU326
 1157 0010 7047     		bx	lr
 1158              	.L72:
 460:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   }
 1159              		.loc 1 460 5 is_stmt 1 view .LVU327
ARM GAS  /tmp/ccPRqU3T.s 			page 83


 460:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   }
 1160              		.loc 1 460 19 is_stmt 0 view .LVU328
 1161 0012 4FF0E022 		mov	r2, #-536813568
 1162 0016 1369     		ldr	r3, [r2, #16]
 1163 0018 43F00403 		orr	r3, r3, #4
 1164 001c 1361     		str	r3, [r2, #16]
 1165 001e 7047     		bx	lr
 1166              		.cfi_endproc
 1167              	.LFE145:
 1169              		.section	.text.HAL_SYSTICK_Callback,"ax",%progbits
 1170              		.align	1
 1171              		.weak	HAL_SYSTICK_Callback
 1172              		.syntax unified
 1173              		.thumb
 1174              		.thumb_func
 1176              	HAL_SYSTICK_Callback:
 1177              	.LFB147:
 467:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 468:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 469:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  This function handles SYSTICK interrupt request.
 470:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 471:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 472:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** void HAL_SYSTICK_IRQHandler(void)
 473:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 474:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   HAL_SYSTICK_Callback();
 475:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 476:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 477:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** /**
 478:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @brief  SYSTICK callback.
 479:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   * @retval None
 480:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   */
 481:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** __weak void HAL_SYSTICK_Callback(void)
 482:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** {
 1178              		.loc 1 482 1 is_stmt 1 view -0
 1179              		.cfi_startproc
 1180              		@ args = 0, pretend = 0, frame = 0
 1181              		@ frame_needed = 0, uses_anonymous_args = 0
 1182              		@ link register save eliminated.
 483:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   /* NOTE : This function Should not be modified, when the callback is needed,
 484:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****             the HAL_SYSTICK_Callback could be implemented in the user file
 485:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****    */
 486:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 1183              		.loc 1 486 1 view .LVU330
 1184 0000 7047     		bx	lr
 1185              		.cfi_endproc
 1186              	.LFE147:
 1188              		.section	.text.HAL_SYSTICK_IRQHandler,"ax",%progbits
 1189              		.align	1
 1190              		.global	HAL_SYSTICK_IRQHandler
 1191              		.syntax unified
 1192              		.thumb
 1193              		.thumb_func
 1195              	HAL_SYSTICK_IRQHandler:
 1196              	.LFB146:
 473:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c ****   HAL_SYSTICK_Callback();
 1197              		.loc 1 473 1 view -0
 1198              		.cfi_startproc
ARM GAS  /tmp/ccPRqU3T.s 			page 84


 1199              		@ args = 0, pretend = 0, frame = 0
 1200              		@ frame_needed = 0, uses_anonymous_args = 0
 1201 0000 08B5     		push	{r3, lr}
 1202              	.LCFI2:
 1203              		.cfi_def_cfa_offset 8
 1204              		.cfi_offset 3, -8
 1205              		.cfi_offset 14, -4
 474:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** }
 1206              		.loc 1 474 3 view .LVU332
 1207 0002 FFF7FEFF 		bl	HAL_SYSTICK_Callback
 1208              	.LVL70:
 475:Drivers/STM32F4xx_HAL_Driver/Src/stm32f4xx_hal_cortex.c **** 
 1209              		.loc 1 475 1 is_stmt 0 view .LVU333
 1210 0006 08BD     		pop	{r3, pc}
 1211              		.cfi_endproc
 1212              	.LFE146:
 1214              		.text
 1215              	.Letext0:
 1216              		.file 4 "Drivers/CMSIS/Device/ST/STM32F4xx/Include/stm32f407xx.h"
 1217              		.file 5 "/home/gitc/\346\241\214\351\235\242/gcc-arm-none-eabi-10.3-2021.10/arm-none-eabi/include/
 1218              		.file 6 "/home/gitc/\346\241\214\351\235\242/gcc-arm-none-eabi-10.3-2021.10/arm-none-eabi/include/
 1219              		.file 7 "Drivers/CMSIS/Device/ST/STM32F4xx/Include/stm32f4xx.h"
 1220              		.file 8 "Drivers/STM32F4xx_HAL_Driver/Inc/stm32f4xx_hal_cortex.h"
ARM GAS  /tmp/ccPRqU3T.s 			page 85


DEFINED SYMBOLS
                            *ABS*:0000000000000000 stm32f4xx_hal_cortex.c
     /tmp/ccPRqU3T.s:20     .text.HAL_NVIC_SetPriorityGrouping:0000000000000000 $t
     /tmp/ccPRqU3T.s:26     .text.HAL_NVIC_SetPriorityGrouping:0000000000000000 HAL_NVIC_SetPriorityGrouping
     /tmp/ccPRqU3T.s:82     .text.HAL_NVIC_SetPriorityGrouping:0000000000000020 $d
     /tmp/ccPRqU3T.s:87     .text.HAL_NVIC_SetPriority:0000000000000000 $t
     /tmp/ccPRqU3T.s:93     .text.HAL_NVIC_SetPriority:0000000000000000 HAL_NVIC_SetPriority
     /tmp/ccPRqU3T.s:236    .text.HAL_NVIC_SetPriority:0000000000000068 $d
     /tmp/ccPRqU3T.s:242    .text.HAL_NVIC_EnableIRQ:0000000000000000 $t
     /tmp/ccPRqU3T.s:248    .text.HAL_NVIC_EnableIRQ:0000000000000000 HAL_NVIC_EnableIRQ
     /tmp/ccPRqU3T.s:289    .text.HAL_NVIC_EnableIRQ:0000000000000018 $d
     /tmp/ccPRqU3T.s:294    .text.HAL_NVIC_DisableIRQ:0000000000000000 $t
     /tmp/ccPRqU3T.s:300    .text.HAL_NVIC_DisableIRQ:0000000000000000 HAL_NVIC_DisableIRQ
     /tmp/ccPRqU3T.s:371    .text.HAL_NVIC_DisableIRQ:0000000000000020 $d
     /tmp/ccPRqU3T.s:376    .text.HAL_NVIC_SystemReset:0000000000000000 $t
     /tmp/ccPRqU3T.s:382    .text.HAL_NVIC_SystemReset:0000000000000000 HAL_NVIC_SystemReset
     /tmp/ccPRqU3T.s:448    .text.HAL_NVIC_SystemReset:000000000000001c $d
     /tmp/ccPRqU3T.s:456    .text.HAL_SYSTICK_Config:0000000000000000 $t
     /tmp/ccPRqU3T.s:462    .text.HAL_SYSTICK_Config:0000000000000000 HAL_SYSTICK_Config
     /tmp/ccPRqU3T.s:527    .text.HAL_SYSTICK_Config:0000000000000024 $d
     /tmp/ccPRqU3T.s:532    .text.HAL_MPU_Disable:0000000000000000 $t
     /tmp/ccPRqU3T.s:538    .text.HAL_MPU_Disable:0000000000000000 HAL_MPU_Disable
     /tmp/ccPRqU3T.s:574    .text.HAL_MPU_Disable:0000000000000018 $d
     /tmp/ccPRqU3T.s:579    .text.HAL_MPU_Enable:0000000000000000 $t
     /tmp/ccPRqU3T.s:585    .text.HAL_MPU_Enable:0000000000000000 HAL_MPU_Enable
     /tmp/ccPRqU3T.s:638    .text.HAL_MPU_Enable:000000000000001c $d
     /tmp/ccPRqU3T.s:643    .text.HAL_MPU_ConfigRegion:0000000000000000 $t
     /tmp/ccPRqU3T.s:649    .text.HAL_MPU_ConfigRegion:0000000000000000 HAL_MPU_ConfigRegion
     /tmp/ccPRqU3T.s:738    .text.HAL_MPU_ConfigRegion:000000000000005c $d
     /tmp/ccPRqU3T.s:743    .text.HAL_NVIC_GetPriorityGrouping:0000000000000000 $t
     /tmp/ccPRqU3T.s:749    .text.HAL_NVIC_GetPriorityGrouping:0000000000000000 HAL_NVIC_GetPriorityGrouping
     /tmp/ccPRqU3T.s:773    .text.HAL_NVIC_GetPriorityGrouping:000000000000000c $d
     /tmp/ccPRqU3T.s:778    .text.HAL_NVIC_GetPriority:0000000000000000 $t
     /tmp/ccPRqU3T.s:784    .text.HAL_NVIC_GetPriority:0000000000000000 HAL_NVIC_GetPriority
     /tmp/ccPRqU3T.s:904    .text.HAL_NVIC_GetPriority:000000000000005c $d
     /tmp/ccPRqU3T.s:911    .text.HAL_NVIC_SetPendingIRQ:0000000000000000 $t
     /tmp/ccPRqU3T.s:917    .text.HAL_NVIC_SetPendingIRQ:0000000000000000 HAL_NVIC_SetPendingIRQ
     /tmp/ccPRqU3T.s:959    .text.HAL_NVIC_SetPendingIRQ:0000000000000018 $d
     /tmp/ccPRqU3T.s:964    .text.HAL_NVIC_GetPendingIRQ:0000000000000000 $t
     /tmp/ccPRqU3T.s:970    .text.HAL_NVIC_GetPendingIRQ:0000000000000000 HAL_NVIC_GetPendingIRQ
     /tmp/ccPRqU3T.s:1016   .text.HAL_NVIC_GetPendingIRQ:0000000000000020 $d
     /tmp/ccPRqU3T.s:1021   .text.HAL_NVIC_ClearPendingIRQ:0000000000000000 $t
     /tmp/ccPRqU3T.s:1027   .text.HAL_NVIC_ClearPendingIRQ:0000000000000000 HAL_NVIC_ClearPendingIRQ
     /tmp/ccPRqU3T.s:1069   .text.HAL_NVIC_ClearPendingIRQ:0000000000000018 $d
     /tmp/ccPRqU3T.s:1074   .text.HAL_NVIC_GetActive:0000000000000000 $t
     /tmp/ccPRqU3T.s:1080   .text.HAL_NVIC_GetActive:0000000000000000 HAL_NVIC_GetActive
     /tmp/ccPRqU3T.s:1126   .text.HAL_NVIC_GetActive:0000000000000020 $d
     /tmp/ccPRqU3T.s:1131   .text.HAL_SYSTICK_CLKSourceConfig:0000000000000000 $t
     /tmp/ccPRqU3T.s:1137   .text.HAL_SYSTICK_CLKSourceConfig:0000000000000000 HAL_SYSTICK_CLKSourceConfig
     /tmp/ccPRqU3T.s:1170   .text.HAL_SYSTICK_Callback:0000000000000000 $t
     /tmp/ccPRqU3T.s:1176   .text.HAL_SYSTICK_Callback:0000000000000000 HAL_SYSTICK_Callback
     /tmp/ccPRqU3T.s:1189   .text.HAL_SYSTICK_IRQHandler:0000000000000000 $t
     /tmp/ccPRqU3T.s:1195   .text.HAL_SYSTICK_IRQHandler:0000000000000000 HAL_SYSTICK_IRQHandler

NO UNDEFINED SYMBOLS
